(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.09)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "LTO Battery Management System")
		(date "2025-11-20")
		(rev "C")
		(company "µArt.cz")
		(comment 1 "Vlastimil Slinták")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 73.323913 20)
		(grid_origin 73.323913 20)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Board_0-+BATT")
	(net 2 "Board_0-3V3CUTOFF")
	(net 3 "Board_0-ADC_BATT")
	(net 4 "Board_0-ADC_LN")
	(net 5 "Board_0-ADC_LOAD")
	(net 6 "Board_0-ADC_LP")
	(net 7 "Board_0-ADC_SP")
	(net 8 "Board_0-CUTOFF")
	(net 9 "Board_0-GND")
	(net 10 "Board_0-Net-(J2-Pin_1)")
	(net 11 "Board_0-Net-(J5-Pin_2)")
	(net 12 "Board_0-Net-(J5-Pin_3)")
	(net 13 "Board_0-Net-(J5-Pin_4)")
	(net 14 "Board_0-Net-(JP1-A)")
	(net 15 "Board_0-Net-(JP2-A)")
	(net 16 "Board_0-Net-(Q1-G)")
	(net 17 "Board_0-Net-(Q1-S)")
	(net 18 "Board_0-Net-(Q3-D)")
	(net 19 "Board_0-Net-(Q4-D)")
	(net 20 "Board_0-Net-(U1-SW)")
	(net 21 "Board_0-Net-(U1-V_{FB})")
	(net 22 "Board_0-Net-(U2-PB2)")
	(net 23 "Board_0-Net-(U2-PB3)")
	(net 24 "Board_0-SCL")
	(net 25 "Board_0-SDA")
	(net 26 "Board_0-TXD")
	(net 27 "Board_0-UPDI")
	(net 28 "Board_0-VCC")
	(net 29 "Board_1-+BATT")
	(net 30 "Board_1-3V3CUTOFF")
	(net 31 "Board_1-ADC_BATT")
	(net 32 "Board_1-ADC_LN")
	(net 33 "Board_1-ADC_LOAD")
	(net 34 "Board_1-ADC_LP")
	(net 35 "Board_1-ADC_SP")
	(net 36 "Board_1-CUTOFF")
	(net 37 "Board_1-GND")
	(net 38 "Board_1-Net-(J2-Pin_1)")
	(net 39 "Board_1-Net-(J5-Pin_2)")
	(net 40 "Board_1-Net-(J5-Pin_3)")
	(net 41 "Board_1-Net-(J5-Pin_4)")
	(net 42 "Board_1-Net-(JP1-A)")
	(net 43 "Board_1-Net-(JP2-A)")
	(net 44 "Board_1-Net-(Q1-G)")
	(net 45 "Board_1-Net-(Q1-S)")
	(net 46 "Board_1-Net-(Q3-D)")
	(net 47 "Board_1-Net-(Q4-D)")
	(net 48 "Board_1-Net-(U1-SW)")
	(net 49 "Board_1-Net-(U1-V_{FB})")
	(net 50 "Board_1-Net-(U2-PB2)")
	(net 51 "Board_1-Net-(U2-PB3)")
	(net 52 "Board_1-SCL")
	(net 53 "Board_1-SDA")
	(net 54 "Board_1-TXD")
	(net 55 "Board_1-UPDI")
	(net 56 "Board_1-VCC")
	(net 57 "Board_2-+BATT")
	(net 58 "Board_2-3V3CUTOFF")
	(net 59 "Board_2-ADC_BATT")
	(net 60 "Board_2-ADC_LN")
	(net 61 "Board_2-ADC_LOAD")
	(net 62 "Board_2-ADC_LP")
	(net 63 "Board_2-ADC_SP")
	(net 64 "Board_2-CUTOFF")
	(net 65 "Board_2-GND")
	(net 66 "Board_2-Net-(J2-Pin_1)")
	(net 67 "Board_2-Net-(J5-Pin_2)")
	(net 68 "Board_2-Net-(J5-Pin_3)")
	(net 69 "Board_2-Net-(J5-Pin_4)")
	(net 70 "Board_2-Net-(JP1-A)")
	(net 71 "Board_2-Net-(JP2-A)")
	(net 72 "Board_2-Net-(Q1-G)")
	(net 73 "Board_2-Net-(Q1-S)")
	(net 74 "Board_2-Net-(Q3-D)")
	(net 75 "Board_2-Net-(Q4-D)")
	(net 76 "Board_2-Net-(U1-SW)")
	(net 77 "Board_2-Net-(U1-V_{FB})")
	(net 78 "Board_2-Net-(U2-PB2)")
	(net 79 "Board_2-Net-(U2-PB3)")
	(net 80 "Board_2-SCL")
	(net 81 "Board_2-SDA")
	(net 82 "Board_2-TXD")
	(net 83 "Board_2-UPDI")
	(net 84 "Board_2-VCC")
	(net 85 "Board_3-+BATT")
	(net 86 "Board_3-3V3CUTOFF")
	(net 87 "Board_3-ADC_BATT")
	(net 88 "Board_3-ADC_LN")
	(net 89 "Board_3-ADC_LOAD")
	(net 90 "Board_3-ADC_LP")
	(net 91 "Board_3-ADC_SP")
	(net 92 "Board_3-CUTOFF")
	(net 93 "Board_3-GND")
	(net 94 "Board_3-Net-(J2-Pin_1)")
	(net 95 "Board_3-Net-(J5-Pin_2)")
	(net 96 "Board_3-Net-(J5-Pin_3)")
	(net 97 "Board_3-Net-(J5-Pin_4)")
	(net 98 "Board_3-Net-(JP1-A)")
	(net 99 "Board_3-Net-(JP2-A)")
	(net 100 "Board_3-Net-(Q1-G)")
	(net 101 "Board_3-Net-(Q1-S)")
	(net 102 "Board_3-Net-(Q3-D)")
	(net 103 "Board_3-Net-(Q4-D)")
	(net 104 "Board_3-Net-(U1-SW)")
	(net 105 "Board_3-Net-(U1-V_{FB})")
	(net 106 "Board_3-Net-(U2-PB2)")
	(net 107 "Board_3-Net-(U2-PB3)")
	(net 108 "Board_3-SCL")
	(net 109 "Board_3-SDA")
	(net 110 "Board_3-TXD")
	(net 111 "Board_3-UPDI")
	(net 112 "Board_3-VCC")
	(net 113 "Board_4-+BATT")
	(net 114 "Board_4-3V3CUTOFF")
	(net 115 "Board_4-ADC_BATT")
	(net 116 "Board_4-ADC_LN")
	(net 117 "Board_4-ADC_LOAD")
	(net 118 "Board_4-ADC_LP")
	(net 119 "Board_4-ADC_SP")
	(net 120 "Board_4-CUTOFF")
	(net 121 "Board_4-GND")
	(net 122 "Board_4-Net-(J2-Pin_1)")
	(net 123 "Board_4-Net-(J5-Pin_2)")
	(net 124 "Board_4-Net-(J5-Pin_3)")
	(net 125 "Board_4-Net-(J5-Pin_4)")
	(net 126 "Board_4-Net-(JP1-A)")
	(net 127 "Board_4-Net-(JP2-A)")
	(net 128 "Board_4-Net-(Q1-G)")
	(net 129 "Board_4-Net-(Q1-S)")
	(net 130 "Board_4-Net-(Q3-D)")
	(net 131 "Board_4-Net-(Q4-D)")
	(net 132 "Board_4-Net-(U1-SW)")
	(net 133 "Board_4-Net-(U1-V_{FB})")
	(net 134 "Board_4-Net-(U2-PB2)")
	(net 135 "Board_4-Net-(U2-PB3)")
	(net 136 "Board_4-SCL")
	(net 137 "Board_4-SDA")
	(net 138 "Board_4-TXD")
	(net 139 "Board_4-UPDI")
	(net 140 "Board_4-VCC")
	(net 141 "Board_5-+BATT")
	(net 142 "Board_5-3V3CUTOFF")
	(net 143 "Board_5-ADC_BATT")
	(net 144 "Board_5-ADC_LN")
	(net 145 "Board_5-ADC_LOAD")
	(net 146 "Board_5-ADC_LP")
	(net 147 "Board_5-ADC_SP")
	(net 148 "Board_5-CUTOFF")
	(net 149 "Board_5-GND")
	(net 150 "Board_5-Net-(J2-Pin_1)")
	(net 151 "Board_5-Net-(J5-Pin_2)")
	(net 152 "Board_5-Net-(J5-Pin_3)")
	(net 153 "Board_5-Net-(J5-Pin_4)")
	(net 154 "Board_5-Net-(JP1-A)")
	(net 155 "Board_5-Net-(JP2-A)")
	(net 156 "Board_5-Net-(Q1-G)")
	(net 157 "Board_5-Net-(Q1-S)")
	(net 158 "Board_5-Net-(Q3-D)")
	(net 159 "Board_5-Net-(Q4-D)")
	(net 160 "Board_5-Net-(U1-SW)")
	(net 161 "Board_5-Net-(U1-V_{FB})")
	(net 162 "Board_5-Net-(U2-PB2)")
	(net 163 "Board_5-Net-(U2-PB3)")
	(net 164 "Board_5-SCL")
	(net 165 "Board_5-SDA")
	(net 166 "Board_5-TXD")
	(net 167 "Board_5-UPDI")
	(net 168 "Board_5-VCC")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 140.192301 89.743891)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.2 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 152.557699 37.448953 180)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -0.05 2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 180)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 180)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 35 "Board_1-ADC_SP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 103.323913 23)
		(property "Reference" "KiKit_TO_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(solder_mask_margin 0)
		(attr through_hole board_only exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1.152 1.152)
			(drill 1.152)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 115.537645 82.123891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 0.97 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "Board_3-CUTOFF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 202.280646 31.739779)
		(property "Reference" "KiKit_MB_10_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 101.223043 44.248953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.45 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Board_0-Net-(J5-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Board_0-SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 155.102301 85.026391 90)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 1.5725 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "Board_4-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "Board_4-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "Board_4-+BATT")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 153.600796 29.449817)
		(property "Reference" "KiKit_MB_6_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 74.823913 28)
		(property "Reference" "KiKit_MB_33_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 88.623043 51.898953 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.878942 -0.045577 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Board_0-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 200.192355 40.748953 180)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F2"
			(at -2.35 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-020-9V"
			(at 0 1.65 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883102"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "Board_2-Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "Board_2-Net-(JP2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 140.504006 31.739827)
		(property "Reference" "KiKit_MB_5_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 180.192355 51.898953 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.878942 -0.045577 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "Board_2-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 203.059186 32.69825)
		(property "Reference" "KiKit_MB_10_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.507699 44.188953 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -1.51 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Board_1-3V3CUTOFF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 138.092301 85.343891 -90)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TLV61070ADBV"
			(at 0 2.4 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv61070a.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Boost Converter, 2.5A switch current limit, 2.2-5.5V Output Voltage, 0.5-5.5V Input Voltage, SOT-23-6"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6881375"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "Board_4-Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "Board_4-Net-(JP1-A)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "Board_4-Net-(U1-V_{FB})")
			(pinfunction "V_{FB}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pinfunction "V_{OUT}")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "Board_4-Net-(JP1-A)")
			(pinfunction "V_{IN}")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 107.845821 67.79642)
		(property "Reference" "KiKit_MB_4_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 159.792301 102.643891 -120)
		(descr "Terminal Block 4Ucon ItemNo. 19963, 2 pins, pitch 3.5mm, size 7.7x7mm, drill diameter 1.2mm, pad diameter 2.4mm, http://www.4uconnector.com/online/object/4udrawing/19963.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_4Ucon")
		(tags "THT Terminal Block 4Ucon ItemNo. 19963 pitch 3.5mm size 7.7x7mm drill 1.2mm pad 2.4mm")
		(property "Reference" "J2"
			(at 6.45237 -2.224167 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LOAD"
			(at 1.749999 4.66 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.900001 60)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 240)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 122 "Board_4-Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 240)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "Board_4-GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/TerminalBlock-01x02-3.5mm.step"
			(offset
				(xyz 1.8 3.5 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 89.893043 64.868953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 0.97 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Board_0-CUTOFF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 164.142301 99.893891 -120)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -2.21375 0.065672 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-100-6V"
			(at 0 1.65 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883112"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 240)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "Board_4-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 240)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "Board_4-Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 72.496422)
		(property "Reference" "KiKit_MB_28_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 107.84582 79.196426)
		(property "Reference" "KiKit_MB_14_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 95.584867 79.196422)
		(property "Reference" "KiKit_MB_13_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 92.307645 85.343891 -90)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TLV61070ADBV"
			(at 0 2.4 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv61070a.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Boost Converter, 2.5A switch current limit, 2.2-5.5V Output Voltage, 0.5-5.5V Input Voltage, SOT-23-6"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6881375"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "Board_3-Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "Board_3-Net-(JP1-A)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "Board_3-Net-(U1-V_{FB})")
			(pinfunction "V_{FB}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pinfunction "V_{OUT}")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "Board_3-Net-(JP1-A)")
			(pinfunction "V_{IN}")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 201.415133 67.796421)
		(property "Reference" "KiKit_MB_12_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 105.623043 60.548953 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 1.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MCU_VCC"
			(at 0 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 14 "Board_0-Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "Board_0-+BATT")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 160.607699 43.998953 30)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J3"
			(at -3.439102 -2.043301 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT-"
			(at 0 3.85 30)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 30)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 30)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 30)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 30)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Board_1-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 30)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 37 "Board_1-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 200.886957 85.026391 90)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 1.5725 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "Board_5-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "Board_5-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "Board_5-+BATT")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 135.452699 52.490626 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 1.878942 -0.045577 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Board_1-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 179.142355 51.298953 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 1.853942 -0.088878 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "Board_2-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "Board_2-ADC_LOAD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 125.607671 72.496422)
		(property "Reference" "KiKit_MB_26_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 181.466957 88.243891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0.01 -1.05 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 161 "Board_5-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 200.425584 116.876671)
		(property "Reference" "KiKit_MB_24_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 24.5)
		(property "Reference" "KiKit_MB_29_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(at 154.307699 62.148953 -90)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 2.75 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 1.9 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C139249"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.575 0 270)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 42 "Board_1-Net-(JP1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.575 0 270)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 48 "Board_1-Net-(U1-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 109.757645 87.563891 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.25 0.02 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "Board_3-Net-(Q1-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Board_3-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 158.884801 85.218891)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 1.7075 1.025 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "Board_4-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "Board_4-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "Board_4-ADC_LP")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 218.176087 28)
		(property "Reference" "KiKit_MB_35_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 109.757645 89.513891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.25 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "Board_3-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 23.5)
		(property "Reference" "KiKit_MB_29_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 156.207699 49.068953)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J4"
			(at 0.95 -1.77 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PROG"
			(at 0 7.41 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Board_1-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Board_1-UPDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Board_1-TXD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 206.392355 43.998953 30)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J3"
			(at -3.439102 -2.043301 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT-"
			(at 0 3.85 30)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 30)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 30)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 30)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 30)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Board_2-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 30)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 65 "Board_2-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 103.323913 123.992844)
		(property "Reference" "KiKit_TO_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(solder_mask_margin 0)
		(attr through_hole board_only exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1.152 1.152)
			(drill 1.152)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 108.623043 40.748953 180)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F2"
			(at -2.35 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-020-9V"
			(at 0 1.65 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883102"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Board_0-Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Board_0-Net-(JP2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 97.584868 67.796417)
		(property "Reference" "KiKit_MB_3_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 139.725468 32.698306)
		(property "Reference" "KiKit_MB_5_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 108.845821 67.79642)
		(property "Reference" "KiKit_MB_4_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 94.407645 89.743891)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.2 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 188.154179 67.796417)
		(property "Reference" "KiKit_MB_11_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 85.407645 90.193891 180)
		(property "Reference" "G***"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 114.638895 97.45579 -30)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -3.479775 -1.064647 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 330)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 90 "Board_3-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 330)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 88 "Board_3-ADC_LN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 156.807699 58.748953 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 113.613043 57.748953 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.61 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "270p"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C159807"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Board_0-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 92.330543 61.773953 180)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 1.7075 1.025 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Board_0-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Board_0-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Board_0-ADC_LP")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 113.613043 58.748953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -2.21 -1.1 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "560k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C132339"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Board_0-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 24.5)
		(property "Reference" "KiKit_MB_30_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 183.899855 61.773953 180)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 1.7075 1.025 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "Board_2-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Board_2-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Board_2-ADC_LP")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(at 108.523043 62.148953 -90)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 2.75 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 1.9 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C139249"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.575 0 270)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 14 "Board_0-Net-(JP1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.575 0 270)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 20 "Board_0-Net-(U1-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 143.399203 117.543027)
		(property "Reference" "KiKit_MB_19_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 183.876957 85.343891 -90)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TLV61070ADBV"
			(at 0 2.4 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv61070a.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Boost Converter, 2.5A switch current limit, 2.2-5.5V Output Voltage, 0.5-5.5V Input Voltage, SOT-23-6"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6881375"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "Board_5-Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "Board_5-Net-(JP1-A)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 161 "Board_5-Net-(U1-V_{FB})")
			(pinfunction "V_{FB}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pinfunction "V_{OUT}")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "Board_5-Net-(JP1-A)")
			(pinfunction "V_{IN}")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 143.192301 92.343891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 1.5 0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "Board_4-TXD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "Board_4-Net-(U2-PB2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 152.267301 90.043891 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.25 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 221.176087 118.992844)
		(property "Reference" "KiKit_MB_36_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 109.84582 79.196427)
		(property "Reference" "KiKit_MB_14_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 113.100145 85.218891)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 1.7075 1.025 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Board_3-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "Board_3-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "Board_3-ADC_LP")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 185.976957 88.243891)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.2 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 25.5)
		(property "Reference" "KiKit_MB_29_7"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 95.123043 50.448953 -30)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.580116 -0.02316 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.135 -0.09 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Board_0-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 206.208207 97.45579 -30)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -3.479775 -1.064647 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 330)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 146 "Board_5-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 330)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 144 "Board_5-ADC_LN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 141.457699 58.448953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.26 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Board_1-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 193.792355 44.248953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 1.5 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Board_2-Net-(J5-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "Board_2-SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.092301 96.543891 150)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.580116 -0.02316 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.135 -0.09 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "Board_4-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 154.630476 79.196426)
		(property "Reference" "KiKit_MB_18_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 126.492844)
		(property "Reference" "KiKit_MB_31_7"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 183.386957 89.243891)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.61 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "270p"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C159807"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 161 "Board_5-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 111.489874 32.69825)
		(property "Reference" "KiKit_MB_2_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 223.176087 28)
		(property "Reference" "KiKit_MB_35_7"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 139.369523 67.796416)
		(property "Reference" "KiKit_MB_7_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 104.207645 102.743891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.45 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "Board_3-Net-(J5-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "Board_3-SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 183.899855 65.308953)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 1.6925 1.24 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C112239"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Board_2-CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Board_2-Net-(Q4-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 97.407645 92.343891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 1.5 0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "Board_3-TXD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "Board_3-Net-(U2-PB2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 148.007699 44.248953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 1.5 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Board_1-Net-(J5-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Board_1-SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 141.369523 67.796416)
		(property "Reference" "KiKit_MB_7_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 182.176957 102.993891 -150)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J3"
			(at -3.439102 -2.043301 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT-"
			(at 0 3.85 210)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 210)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 210)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 30)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 210)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "Board_5-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 210)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 149 "Board_5-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 110.907645 95.543891 150)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.586814 0.088442 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "Board_3-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 154.407699 40.748953 180)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F2"
			(at -2.35 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-020-9V"
			(at 0 1.65 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883102"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "Board_1-Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Board_1-Net-(JP2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 108.856269 30.116141)
		(property "Reference" "KiKit_MB_2_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 125.492844)
		(property "Reference" "KiKit_MB_32_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 143.369523 67.796417)
		(property "Reference" "KiKit_MB_7_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 209.926957 99.893891 -120)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -2.21375 0.065672 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-100-6V"
			(at 0 1.65 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883112"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 240)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "Board_5-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 240)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "Board_5-Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 102.685145 95.343891 -90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -1.6 -5.3225 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny824-SSU"
			(at 0 5.28 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C3646981"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.4 -3.2225 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "Board_3-CUTOFF")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Board_3-3V3CUTOFF")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 0 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "Board_3-ADC_LN")
			(pinfunction "AIN6")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "Board_3-ADC_LP")
			(pinfunction "AIN7")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "Board_3-Net-(U2-PB3)")
			(pinfunction "RXD")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "Board_3-Net-(U2-PB2)")
			(pinfunction "TXD")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "Board_3-SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "Board_3-SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "Board_3-UPDI")
			(pinfunction "~{RESET}/PA0")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 2.475 0 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "Board_3-ADC_SP")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "Board_3-ADC_BATT")
			(pinfunction "AIN2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "Board_3-ADC_LOAD")
			(pinfunction "AIN3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 95.600948 116.117409)
		(property "Reference" "KiKit_MB_15_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 95.007645 97.923891 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J4"
			(at 0.95 -1.77 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PROG"
			(at 0 7.41 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "Board_3-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "Board_3-UPDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "Board_3-TXD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 188.143727 30.116173)
		(property "Reference" "KiKit_MB_9_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 161.322301 82.123891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 0.97 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "Board_4-CUTOFF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 141.457699 57.478953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.25 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Board_1-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 199.385452 29.449817)
		(property "Reference" "KiKit_MB_10_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(at 188.476957 84.843891 90)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 2.75 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 1.9 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C139249"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.575 0 90)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 154 "Board_5-Net-(JP1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.575 0 90)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 160 "Board_5-Net-(U1-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 182.992355 44.348953 60)
		(descr "Terminal Block 4Ucon ItemNo. 19963, 2 pins, pitch 3.5mm, size 7.7x7mm, drill diameter 1.2mm, pad diameter 2.4mm, http://www.4uconnector.com/online/object/4udrawing/19963.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_4Ucon")
		(tags "THT Terminal Block 4Ucon ItemNo. 19963 pitch 3.5mm size 7.7x7mm drill 1.2mm pad 2.4mm")
		(property "Reference" "J2"
			(at 6.45237 -2.224167 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LOAD"
			(at 1.749999 4.66 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.900001 60)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 60)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 66 "Board_2-Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 60)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Board_2-GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/TerminalBlock-01x02-3.5mm.step"
			(offset
				(xyz 1.8 3.5 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 126.492844)
		(property "Reference" "KiKit_MB_32_7"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 109.845821 67.796421)
		(property "Reference" "KiKit_MB_4_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 139.725469 114.294594)
		(property "Reference" "KiKit_MB_19_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 205.576957 102.643891 -120)
		(descr "Terminal Block 4Ucon ItemNo. 19963, 2 pins, pitch 3.5mm, size 7.7x7mm, drill diameter 1.2mm, pad diameter 2.4mm, http://www.4uconnector.com/online/object/4udrawing/19963.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_4Ucon")
		(tags "THT Terminal Block 4Ucon ItemNo. 19963 pitch 3.5mm size 7.7x7mm drill 1.2mm pad 2.4mm")
		(property "Reference" "J2"
			(at 6.45237 -2.224167 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LOAD"
			(at 1.749999 4.66 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.900001 60)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 240)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 150 "Board_5-Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 240)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "Board_5-GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/TerminalBlock-01x02-3.5mm.step"
			(offset
				(xyz 1.8 3.5 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 106.773043 37.448953 180)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -0.05 2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 180)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 180)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 7 "Board_0-ADC_SP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 110.711334 31.739779)
		(property "Reference" "KiKit_MB_2_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 182.361105 49.537054 150)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -3.479775 -1.064647 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 150)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 62 "Board_2-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 150)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 60 "Board_2-ADC_LN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 97.584867 79.196423)
		(property "Reference" "KiKit_MB_13_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 140.692301 85.568891 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.425 -0.1 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "Board_4-Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 78.823913 118.992844)
		(property "Reference" "KiKit_MB_34_7"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 181.462355 64.868953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 0.97 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Board_2-CUTOFF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 156.807699 57.248953 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 199.415133 67.79642)
		(property "Reference" "KiKit_MB_12_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 194.276957 115.143891)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J5"
			(at 2.7 -2.7 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "QWIIC"
			(at 0 3.98 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160404"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Board_5-ADC_SP")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "Board_5-Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "Board_5-Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 153 "Board_5-Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 149 "Board_5-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 149 "Board_5-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 1.4 -0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 109.757645 88.543891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.26 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "Board_3-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 94.523043 51.448953 -30)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.586814 0.088442 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Board_0-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 171.392327 73.496422)
		(property "Reference" "KiKit_MB_27_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 96.807645 106.243891)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F2"
			(at -2.35 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-020-9V"
			(at 0 1.65 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883102"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "Board_3-Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "Board_3-Net-(JP2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 107.816141 117.543)
		(property "Reference" "KiKit_MB_16_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 201.415132 79.196427)
		(property "Reference" "KiKit_MB_22_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 75.496422)
		(property "Reference" "KiKit_MB_25_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 111.845821 67.796421)
		(property "Reference" "KiKit_MB_4_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 201.326957 87.563891 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.25 0.02 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "Board_5-Net-(Q1-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "Board_5-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 189.183859 117.543027)
		(property "Reference" "KiKit_MB_23_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 186.576957 97.923891 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J4"
			(at 0.95 -1.77 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PROG"
			(at 0 7.41 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "Board_5-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 167 "Board_5-UPDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 166 "Board_5-TXD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 151.007699 40.748953 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 2.65 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "I2C_V"
			(at 0 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 43 "Board_1-Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 39 "Board_1-Net-(J5-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 102.607645 81.743891 180)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J1"
			(at 3.7 1.2 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT+"
			(at 0 3.85 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "Board_3-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 180)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 85 "Board_3-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 115.533043 58.748953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0.01 -1.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Board_0-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 202.592355 57.248953 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 199.992355 43.748953)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0.05 2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Board_2-3V3CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "Board_2-Net-(Q3-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 125.607671 73.496422)
		(property "Reference" "KiKit_MB_26_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 148.530199 51.648953 90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -1.6 -5.3225 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny824-SSU"
			(at 0 5.28 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C3646981"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.4 -3.2225 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Board_1-CUTOFF")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Board_1-3V3CUTOFF")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Board_1-ADC_LN")
			(pinfunction "AIN6")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Board_1-ADC_LP")
			(pinfunction "AIN7")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Board_1-Net-(U2-PB3)")
			(pinfunction "RXD")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "Board_1-Net-(U2-PB2)")
			(pinfunction "TXD")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Board_1-SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Board_1-SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Board_1-UPDI")
			(pinfunction "~{RESET}/PA0")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "Board_1-ADC_SP")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Board_1-ADC_BATT")
			(pinfunction "AIN2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Board_1-ADC_LOAD")
			(pinfunction "AIN3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 222.176087 118.992844)
		(property "Reference" "KiKit_MB_36_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 91.817645 89.243891)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.61 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "270p"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C159807"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "Board_3-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 153.600797 117.543)
		(property "Reference" "KiKit_MB_20_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 187.170256 30.875474)
		(property "Reference" "KiKit_MB_9_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 142.792301 103.243891 180)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0.05 2.3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "Board_4-3V3CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "Board_4-Net-(Q3-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 156.630476 79.196427)
		(property "Reference" "KiKit_MB_18_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 122.492844)
		(property "Reference" "KiKit_MB_31_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 100.207645 106.243891)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 2.65 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "I2C_V"
			(at 0 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 99 "Board_3-Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 95 "Board_3-Net-(J5-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 117.857645 95.693891 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 1.853942 -0.088878 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "Board_3-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "Board_3-ADC_LOAD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 106.482645 90.043891 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.25 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 75.823913 118.992844)
		(property "Reference" "KiKit_MB_34_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 159.397699 58.748953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -2.21 -1.1 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "560k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C132339"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Board_1-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 197.192355 60.548953 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 1.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MCU_VCC"
			(at 0 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 70 "Board_2-Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 57 "Board_2-+BATT")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 94.719354 115.253065)
		(property "Reference" "KiKit_MB_15_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 125.492844)
		(property "Reference" "KiKit_MB_31_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 204.669457 85.218891)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 1.7075 1.025 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "Board_5-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "Board_5-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Board_5-ADC_LP")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 87.573043 51.298953 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 1.853942 -0.088878 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Board_0-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Board_0-ADC_LOAD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 194.392355 65.248953)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J1"
			(at 3.7 1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT+"
			(at 0 3.85 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Board_2-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 57 "Board_2-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 96.584868 67.796417)
		(property "Reference" "KiKit_MB_3_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 144.732699 56.948953 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 148.992301 102.743891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 1.5 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "Board_4-Net-(J5-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "Board_4-SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 202.415132 79.196427)
		(property "Reference" "KiKit_MB_22_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 136.576449 49.537054 150)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -3.479775 -1.064647 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 150)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 34 "Board_1-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 150)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 32 "Board_1-ADC_LN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 89.668043 52.490626 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 1.878942 -0.045577 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Board_0-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 142.592301 106.243891)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F2"
			(at -2.35 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-020-9V"
			(at 0 1.65 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883102"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "Board_4-Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "Board_4-Net-(JP2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 197.292355 44.188953 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -1.51 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Board_2-3V3CUTOFF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 132.857699 47.098953 60)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -2.21375 0.065672 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-100-6V"
			(at 0 1.65 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883112"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 60)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Board_1-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 60)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "Board_1-Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 202.592355 58.748953 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 153.630477 67.79642)
		(property "Reference" "KiKit_MB_8_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 162.592301 95.093891 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.878942 -0.045577 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "Board_4-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 110.307645 96.543891 150)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.580116 -0.02316 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.135 -0.09 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "Board_3-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 113.123043 61.648953 90)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TLV61070ADBV"
			(at 0 2.4 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv61070a.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Boost Converter, 2.5A switch current limit, 2.2-5.5V Output Voltage, 0.5-5.5V Input Voltage, SOT-23-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6881375"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Board_0-Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Board_0-Net-(JP1-A)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Board_0-Net-(U1-V_{FB})")
			(pinfunction "V_{FB}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pinfunction "V_{OUT}")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Board_0-Net-(JP1-A)")
			(pinfunction "V_{IN}")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 125.607671 71.496422)
		(property "Reference" "KiKit_MB_26_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 99.707645 102.803891 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -1.51 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Board_3-3V3CUTOFF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 114.007645 102.643891 -120)
		(descr "Terminal Block 4Ucon ItemNo. 19963, 2 pins, pitch 3.5mm, size 7.7x7mm, drill diameter 1.2mm, pad diameter 2.4mm, http://www.4uconnector.com/online/object/4udrawing/19963.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_4Ucon")
		(tags "THT Terminal Block 4Ucon ItemNo. 19963 pitch 3.5mm size 7.7x7mm drill 1.2mm pad 2.4mm")
		(property "Reference" "J2"
			(at 6.45237 -2.224167 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LOAD"
			(at 1.749999 4.66 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.900001 60)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 240)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 94 "Board_3-Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 240)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "Board_3-GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/TerminalBlock-01x02-3.5mm.step"
			(offset
				(xyz 1.8 3.5 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 92.330543 65.308953)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 1.6925 1.24 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C112239"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Board_0-CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Board_0-Net-(Q4-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 202.476957 95.543891 150)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.586814 0.088442 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Board_5-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 124.492844)
		(property "Reference" "KiKit_MB_32_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 154.640925 30.116141)
		(property "Reference" "KiKit_MB_6_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 201.399052 30.875435)
		(property "Reference" "KiKit_MB_10_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 94.719351 31.739827)
		(property "Reference" "KiKit_MB_1_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 208.376957 95.093891 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.878942 -0.045577 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "Board_5-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 189.154178 79.196423)
		(property "Reference" "KiKit_MB_21_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 108.023043 54.648953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 1.5 0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Board_0-TXD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Board_0-Net-(U2-PB2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 75.823913 28)
		(property "Reference" "KiKit_MB_33_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 142.369522 79.196423)
		(property "Reference" "KiKit_MB_17_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 199.592355 54.648953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 1.5 0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "Board_2-TXD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "Board_2-Net-(U2-PB2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 157.27453 32.69825)
		(property "Reference" "KiKit_MB_6_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 186.288662 31.739827)
		(property "Reference" "KiKit_MB_9_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 20.5)
		(property "Reference" "KiKit_MB_29_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 22.5)
		(property "Reference" "KiKit_MB_30_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 220.176087 118.992844)
		(property "Reference" "KiKit_MB_36_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 151.407699 60.548953 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 1.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MCU_VCC"
			(at 0 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 42 "Board_1-Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 29 "Board_1-+BATT")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 158.884801 81.683891 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 1.6925 1.24 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C112239"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "Board_4-CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "Board_4-Net-(Q4-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 97.614547 29.449844)
		(property "Reference" "KiKit_MB_1_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 176.976957 90.193891 180)
		(property "Reference" "G***"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 108.84582 79.196426)
		(property "Reference" "KiKit_MB_14_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 155.614396 30.875435)
		(property "Reference" "KiKit_MB_6_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 149.992301 102.743891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.45 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "Board_4-Net-(J5-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "Board_4-SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 93.940813 32.698306)
		(property "Reference" "KiKit_MB_1_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 181.237355 52.490626 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 1.878942 -0.045577 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "Board_2-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 186.692355 50.448953 -30)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.580116 -0.02316 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.135 -0.09 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Board_2-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 186.322355 64.958953 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.09 1.57 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Board_2-Net-(Q4-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "Board_2-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 185.510125 114.294594)
		(property "Reference" "KiKit_MB_23_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 156.49599 31.739779)
		(property "Reference" "KiKit_MB_6_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 165.807699 56.798953)
		(property "Reference" "G***"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 111.489875 114.294538)
		(property "Reference" "KiKit_MB_16_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 199.456957 88.543891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -0.005 0.925 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "Board_5-+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Board_5-ADC_BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 141.897699 61.966453 -90)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 1.5725 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Board_1-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Board_1-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Board_1-+BATT")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 143.399202 29.449844)
		(property "Reference" "KiKit_MB_5_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 98.948043 56.948953 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 137.602301 88.243891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -2.21 -1.1 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "560k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C132339"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "Board_4-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 201.326957 88.543891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.26 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Board_5-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 116.807645 95.093891 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.878942 -0.045577 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "Board_3-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 190.226957 109.543891)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -0.05 2.3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 147 "Board_5-ADC_SP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 121.492844)
		(property "Reference" "KiKit_MB_31_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 77.823913 118.992844)
		(property "Reference" "KiKit_MB_34_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 191.276957 102.803891 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -1.51 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Board_5-3V3CUTOFF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 97.543043 58.448953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -0.005 0.925 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Board_0-+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Board_0-ADC_BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 113.100145 81.683891 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 1.6925 1.24 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C112239"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "Board_3-CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Board_3-Net-(Q4-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 157.274531 114.294538)
		(property "Reference" "KiKit_MB_20_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 153.672301 88.543891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -0.005 0.925 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "Board_4-+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "Board_4-ADC_BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 125.607671 75.496422)
		(property "Reference" "KiKit_MB_26_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 185.154179 67.796416)
		(property "Reference" "KiKit_MB_11_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 118.357645 99.893891 -120)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -2.21375 0.065672 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-100-6V"
			(at 0 1.65 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883112"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 240)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "Board_3-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 240)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "Board_3-Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 140.907699 50.448953 -30)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.580116 -0.02316 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.135 -0.09 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Board_1-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 201.399055 116.11737)
		(property "Reference" "KiKit_MB_24_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 110.423043 49.068953)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J4"
			(at 0.95 -1.77 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PROG"
			(at 0 7.41 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Board_0-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Board_0-UPDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Board_0-TXD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 91.817645 88.243891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -2.21 -1.1 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "560k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C132339"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "Board_3-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 97.007645 103.243891 180)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0.05 2.3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Board_3-3V3CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "Board_3-Net-(Q3-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 123.492844)
		(property "Reference" "KiKit_MB_31_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 74.823913 118.992844)
		(property "Reference" "KiKit_MB_34_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 93.584867 79.196422)
		(property "Reference" "KiKit_MB_13_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 192.792355 44.248953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.45 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Board_2-Net-(J5-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Board_2-SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 73.496422)
		(property "Reference" "KiKit_MB_28_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 90.791793 49.537054 150)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -3.479775 -1.064647 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 150)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 6 "Board_0-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 150)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 4 "Board_0-ADC_LN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 94.584868 67.796416)
		(property "Reference" "KiKit_MB_3_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 139.369522 79.196422)
		(property "Reference" "KiKit_MB_17_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 111.84582 79.196427)
		(property "Reference" "KiKit_MB_14_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 114.823043 43.998953 30)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J3"
			(at -3.439102 -2.043301 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT-"
			(at 0 3.85 30)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 30)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 30)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 30)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 30)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Board_0-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 30)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 9 "Board_0-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 141.369522 79.196422)
		(property "Reference" "KiKit_MB_17_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 102.723043 31.848953 180)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J5"
			(at 2.7 -2.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "QWIIC"
			(at 0 3.98 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160404"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Board_0-ADC_SP")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Board_0-Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Board_0-Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Board_0-Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 9 "Board_0-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 9 "Board_0-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 1.4 -0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 159.397699 57.748953 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.61 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "270p"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C159807"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Board_1-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 187.154179 67.796416)
		(property "Reference" "KiKit_MB_11_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102.223043 44.248953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 1.5 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Board_0-Net-(J5-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Board_0-SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 102.823043 65.248953)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J1"
			(at 3.7 1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT+"
			(at 0 3.85 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Board_0-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 1 "Board_0-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 75.496422)
		(property "Reference" "KiKit_MB_28_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 21.5)
		(property "Reference" "KiKit_MB_30_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 87.073043 47.098953 60)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -2.21375 0.065672 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-100-6V"
			(at 0 1.65 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883112"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 60)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Board_0-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 60)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Board_0-Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 201.876957 96.543891 150)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.580116 -0.02316 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.135 -0.09 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Board_5-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 95.584868 67.796416)
		(property "Reference" "KiKit_MB_3_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 163.642301 95.693891 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 1.853942 -0.088878 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "Board_4-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "Board_4-ADC_LOAD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.677645 82.033891 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.09 1.57 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Board_3-Net-(Q4-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Board_3-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 109.317645 85.026391 90)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 1.5725 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Board_3-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "Board_3-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "Board_3-+BATT")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 121.492844)
		(property "Reference" "KiKit_MB_32_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 194.176957 81.743891 180)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J1"
			(at 3.7 1.2 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT+"
			(at 0 3.85 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Board_5-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 180)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 141 "Board_5-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 189.183858 29.449844)
		(property "Reference" "KiKit_MB_9_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 115.762645 94.502218 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 1.878942 -0.045577 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "Board_3-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 154.640928 116.876671)
		(property "Reference" "KiKit_MB_20_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 185.154178 79.196422)
		(property "Reference" "KiKit_MB_21_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 141.3856 30.875474)
		(property "Reference" "KiKit_MB_5_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 185.976957 89.743891)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.2 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 95.600945 30.875474)
		(property "Reference" "KiKit_MB_1_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 154.207699 43.748953)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0.05 2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Board_1-3V3CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "Board_1-Net-(Q3-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 96.113043 61.966453 -90)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 1.5725 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Board_0-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Board_0-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Board_0-+BATT")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 194.292355 31.848953 180)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J5"
			(at 2.7 -2.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "QWIIC"
			(at 0 3.98 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160404"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Board_2-ADC_SP")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Board_2-Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Board_2-Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Board_2-Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 65 "Board_2-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 65 "Board_2-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 1.4 -0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 25.5)
		(property "Reference" "KiKit_MB_30_7"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 200.425581 30.116141)
		(property "Reference" "KiKit_MB_10_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 142.359071 30.116173)
		(property "Reference" "KiKit_MB_5_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 187.154178 79.196422)
		(property "Reference" "KiKit_MB_21_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 73.496422)
		(property "Reference" "KiKit_MB_25_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 90.607645 102.993891 -150)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J3"
			(at -3.439102 -2.043301 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT-"
			(at 0 3.85 210)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 210)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 210)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 30)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 210)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "Board_3-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 210)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 93 "Board_3-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 198.051957 90.043891 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.25 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 221.176087 28)
		(property "Reference" "KiKit_MB_35_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 125.607671 74.496422)
		(property "Reference" "KiKit_MB_26_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 110.84582 79.196427)
		(property "Reference" "KiKit_MB_14_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.673043 57.478953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.25 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Board_0-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 204.669457 81.683891 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 1.6925 1.24 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C112239"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "Board_5-CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "Board_5-Net-(Q4-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 191.376957 86.443891)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 1.7 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MCU_VCC"
			(at 0 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 154 "Board_5-Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 141 "Board_5-+BATT")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 137.592301 91.043891 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 1.6 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Board_4-UPDI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 78.823913 28)
		(property "Reference" "KiKit_MB_33_7"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 145.592301 86.443891)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 1.7 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MCU_VCC"
			(at 0 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 126 "Board_4-Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 113 "Board_4-+BATT")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 22.5)
		(property "Reference" "KiKit_MB_29_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 202.280649 115.253017)
		(property "Reference" "KiKit_MB_24_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 187.682355 61.966453 -90)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 1.5725 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "Board_2-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Board_2-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Board_2-+BATT")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 74.496422)
		(property "Reference" "KiKit_MB_25_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 140.537699 64.958953 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.09 1.57 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "Board_1-Net-(Q4-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Board_1-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 187.242355 59.428953)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.25 0.02 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Board_2-Net-(Q1-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "Board_2-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 107.81614 29.449817)
		(property "Reference" "KiKit_MB_2_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 71.496422)
		(property "Reference" "KiKit_MB_25_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 111.023043 57.248953 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 207.331957 94.502218 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 1.878942 -0.045577 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "Board_5-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 140.369522 79.196422)
		(property "Reference" "KiKit_MB_17_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 142.359074 116.876703)
		(property "Reference" "KiKit_MB_19_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 223.176087 118.992844)
		(property "Reference" "KiKit_MB_36_7"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 187.242355 57.478953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.25 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "Board_2-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 155.542301 87.563891 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.25 0.02 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "Board_4-Net-(Q1-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "Board_4-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 190.517355 56.948953 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 23.5)
		(property "Reference" "KiKit_MB_30_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 137.207699 44.348953 60)
		(descr "Terminal Block 4Ucon ItemNo. 19963, 2 pins, pitch 3.5mm, size 7.7x7mm, drill diameter 1.2mm, pad diameter 2.4mm, http://www.4uconnector.com/online/object/4udrawing/19963.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_4Ucon")
		(tags "THT Terminal Block 4Ucon ItemNo. 19963 pitch 3.5mm size 7.7x7mm drill 1.2mm pad 2.4mm")
		(property "Reference" "J2"
			(at 6.45237 -2.224167 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LOAD"
			(at 1.749999 4.66 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.900001 60)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 60)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 38 "Board_1-Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 60)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Board_1-GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/TerminalBlock-01x02-3.5mm.step"
			(offset
				(xyz 1.8 3.5 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 160.423551 97.45579 -30)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -3.479775 -1.064647 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 330)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 118 "Board_4-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 330)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 116 "Board_4-ADC_LN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 161.317699 58.748953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0.01 -1.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Board_1-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 194.254457 95.343891 -90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -1.6 -5.3225 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny824-SSU"
			(at 0 5.28 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C3646981"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.4 -3.2225 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "Board_5-CUTOFF")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Board_5-3V3CUTOFF")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 0 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "Board_5-ADC_LN")
			(pinfunction "AIN6")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Board_5-ADC_LP")
			(pinfunction "AIN7")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 163 "Board_5-Net-(U2-PB3)")
			(pinfunction "RXD")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "Board_5-Net-(U2-PB2)")
			(pinfunction "TXD")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 165 "Board_5-SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 164 "Board_5-SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 167 "Board_5-UPDI")
			(pinfunction "~{RESET}/PA0")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 2.475 0 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Board_5-ADC_SP")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Board_5-ADC_BATT")
			(pinfunction "AIN2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "Board_5-ADC_LOAD")
			(pinfunction "AIN3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 140.192301 88.243891)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.2 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 153.807699 54.648953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 1.5 0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "Board_1-TXD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "Board_1-Net-(U2-PB2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 178.642355 47.098953 60)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -2.21375 0.065672 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-100-6V"
			(at 0 1.65 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883112"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 60)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "Board_2-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 60)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Board_2-Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 96.574419 116.876703)
		(property "Reference" "KiKit_MB_15_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 131.192301 90.193891 180)
		(property "Reference" "G***"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 108.423043 43.748953)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0.05 2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Board_0-3V3CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Board_0-Net-(Q3-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 135.682301 88.243891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0.01 -1.05 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "Board_4-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 105.723043 44.188953 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -1.51 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Board_0-3V3CUTOFF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 94.753043 64.958953 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.09 1.57 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Board_0-Net-(Q4-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Board_0-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(at 142.692301 84.843891 90)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 2.75 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 1.9 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C139249"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.575 0 90)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 126 "Board_4-Net-(JP1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.575 0 90)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 132 "Board_4-Net-(U1-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 133.357699 51.298953 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 1.853942 -0.088878 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Board_1-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Board_1-ADC_LOAD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 94.907645 85.568891 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.425 -0.1 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "Board_3-Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 102.745543 51.648953 90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -1.6 -5.3225 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny824-SSU"
			(at 0 5.28 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C3646981"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.4 -3.2225 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Board_0-CUTOFF")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Board_0-3V3CUTOFF")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Board_0-ADC_LN")
			(pinfunction "AIN6")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Board_0-ADC_LP")
			(pinfunction "AIN7")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Board_0-Net-(U2-PB3)")
			(pinfunction "RXD")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Board_0-Net-(U2-PB2)")
			(pinfunction "TXD")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Board_0-SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Board_0-SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Board_0-UPDI")
			(pinfunction "~{RESET}/PA0")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Board_0-ADC_SP")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Board_0-ADC_BATT")
			(pinfunction "AIN2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Board_0-ADC_LOAD")
			(pinfunction "AIN3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 202.092355 61.423953 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.425 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Board_2-Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 205.182355 58.748953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -2.21 -1.1 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "560k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C132339"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Board_2-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 158.907699 61.648953 90)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TLV61070ADBV"
			(at 0 2.4 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv61070a.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Boost Converter, 2.5A switch current limit, 2.2-5.5V Output Voltage, 0.5-5.5V Input Voltage, SOT-23-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6881375"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Board_1-Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Board_1-Net-(JP1-A)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Board_1-Net-(U1-V_{FB})")
			(pinfunction "V_{FB}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pinfunction "V_{OUT}")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Board_1-Net-(JP1-A)")
			(pinfunction "V_{IN}")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 109.829743 116.11737)
		(property "Reference" "KiKit_MB_16_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 73.823913 118.992844)
		(property "Reference" "KiKit_MB_34_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 205.182355 57.748953 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.61 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "270p"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C159807"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Board_2-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 171.392327 72.496422)
		(property "Reference" "KiKit_MB_27_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 161.547301 94.502218 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 1.878942 -0.045577 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "Board_4-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 148.507699 31.848953 180)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J5"
			(at 2.7 -2.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "QWIIC"
			(at 0 3.98 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160404"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "Board_1-ADC_SP")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "Board_1-Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Board_1-Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Board_1-Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 37 "Board_1-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 37 "Board_1-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 1.4 -0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 91.423043 44.348953 60)
		(descr "Terminal Block 4Ucon ItemNo. 19963, 2 pins, pitch 3.5mm, size 7.7x7mm, drill diameter 1.2mm, pad diameter 2.4mm, http://www.4uconnector.com/online/object/4udrawing/19963.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_4Ucon")
		(tags "THT Terminal Block 4Ucon ItemNo. 19963 pitch 3.5mm size 7.7x7mm drill 1.2mm pad 2.4mm")
		(property "Reference" "J2"
			(at 6.45237 -2.224167 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LOAD"
			(at 1.749999 4.66 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.900001 60)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 60)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 10 "Board_0-Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 60)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Board_0-GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/TerminalBlock-01x02-3.5mm.step"
			(offset
				(xyz 1.8 3.5 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 148.469801 95.343891 -90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -1.6 -5.3225 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny824-SSU"
			(at 0 5.28 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C3646981"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.4 -3.2225 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "Board_4-CUTOFF")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "Board_4-3V3CUTOFF")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 0 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "Board_4-ADC_LN")
			(pinfunction "AIN6")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "Board_4-ADC_LP")
			(pinfunction "AIN7")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "Board_4-Net-(U2-PB3)")
			(pinfunction "RXD")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "Board_4-Net-(U2-PB2)")
			(pinfunction "TXD")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "Board_4-SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "Board_4-SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Board_4-UPDI")
			(pinfunction "~{RESET}/PA0")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 2.475 0 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "Board_4-ADC_SP")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "Board_4-ADC_BATT")
			(pinfunction "AIN2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "Board_4-ADC_LOAD")
			(pinfunction "AIN3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(at 96.907645 84.843891 90)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 2.75 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 1.9 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C139249"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.575 0 90)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 98 "Board_3-Net-(JP1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.575 0 90)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 104 "Board_3-Net-(U1-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1206_3216Metric"
		(layer "F.Cu")
		(at 200.092355 62.148953 -90)
		(descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 2.75 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 1.9 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C139249"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.575 0 270)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 70 "Board_2-Net-(JP1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.575 0 270)
			(size 1.05 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 76 "Board_2-Net-(U1-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 203.415133 67.796421)
		(property "Reference" "KiKit_MB_12_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 155.630477 67.796421)
		(property "Reference" "KiKit_MB_8_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 98.657645 109.543891)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -0.05 2.3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 91 "Board_3-ADC_SP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 144.442301 109.543891)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -0.05 2.3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 119 "Board_4-ADC_SP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 105.223043 40.748953 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 2.65 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "I2C_V"
			(at 0 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 15 "Board_0-Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 11 "Board_0-Net-(J5-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 123.492844)
		(property "Reference" "KiKit_MB_32_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 199.385453 117.543)
		(property "Reference" "KiKit_MB_24_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 140.792301 97.923891 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J4"
			(at 0.95 -1.77 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PROG"
			(at 0 7.41 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "Board_4-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Board_4-UPDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "Board_4-TXD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 201.326957 89.513891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.25 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Board_5-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.673043 59.428953)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.25 0.02 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Board_0-Net-(Q1-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Board_0-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 135.677699 64.868953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 0.97 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Board_1-CUTOFF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 155.542301 89.513891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.25 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "Board_4-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 156.495993 115.253017)
		(property "Reference" "KiKit_MB_20_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 155.614399 116.11737)
		(property "Reference" "KiKit_MB_20_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 137.602301 89.243891)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.61 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "270p"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C159807"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "Board_4-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 21.5)
		(property "Reference" "KiKit_MB_29_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 194.314855 51.648953 90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -1.6 -5.3225 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny824-SSU"
			(at 0 5.28 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C3646981"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.4 -3.2225 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Board_2-CUTOFF")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Board_2-3V3CUTOFF")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "Board_2-ADC_LN")
			(pinfunction "AIN6")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Board_2-ADC_LP")
			(pinfunction "AIN7")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "Board_2-Net-(U2-PB3)")
			(pinfunction "RXD")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "Board_2-Net-(U2-PB2)")
			(pinfunction "TXD")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "Board_2-SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Board_2-SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "Board_2-UPDI")
			(pinfunction "~{RESET}/PA0")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Board_2-ADC_SP")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "Board_2-ADC_BATT")
			(pinfunction "AIN2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "Board_2-ADC_LOAD")
			(pinfunction "AIN3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 188.976957 92.343891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 1.5 0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 166 "Board_5-TXD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "Board_5-Net-(U2-PB2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 91.807645 91.043891 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 1.6 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "Board_3-UPDI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 94.407645 88.243891)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.2 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "Board_3-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 156.462301 82.033891 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.09 1.57 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "Board_4-Net-(Q4-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "Board_4-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 222.176087 28)
		(property "Reference" "KiKit_MB_35_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 110.845821 67.796421)
		(property "Reference" "KiKit_MB_4_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 188.14373 116.876703)
		(property "Reference" "KiKit_MB_23_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric"
		(layer "F.Cu")
		(at 198.342355 37.448953 180)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -0.05 2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1R"
			(at 0 2.65 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2934341"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 180)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 180)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 63 "Board_2-ADC_SP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 193.676087 23)
		(property "Reference" "KiKit_TO_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(solder_mask_margin 0)
		(attr through_hole board_only exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1.152 1.152)
			(drill 1.152)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 157.630477 67.796421)
		(property "Reference" "KiKit_MB_8_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 138.115199 61.773953 180)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 1.7075 1.025 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Board_1-Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Board_1-Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Board_1-ADC_LP")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 186.092355 51.448953 -30)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.586814 0.088442 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Board_2-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 155.542301 88.543891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.26 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "Board_4-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 207.106957 82.123891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 0.97 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "Board_5-CUTOFF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 93.940814 114.294594)
		(property "Reference" "KiKit_MB_15_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 188.154178 79.196423)
		(property "Reference" "KiKit_MB_21_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 120.023043 56.798953)
		(property "Reference" "G***"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.692301 95.543891 150)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.586814 0.088442 150)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 150)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 150)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "Board_4-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 150)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Board_4-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 156.307699 61.423953 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.425 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Board_1-Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 109.82974 30.875435)
		(property "Reference" "KiKit_MB_2_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 187.242355 58.448953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.26 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "Board_2-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 122.492844)
		(property "Reference" "KiKit_MB_32_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 97.614548 117.543027)
		(property "Reference" "KiKit_MB_15_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 187.170259 116.117409)
		(property "Reference" "KiKit_MB_23_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 201.992355 49.068953)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J4"
			(at 0.95 -1.77 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PROG"
			(at 0 7.41 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Board_2-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "Board_2-UPDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "Board_2-TXD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 138.115199 65.308953)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 1.6925 1.24 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSS138"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C112239"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Board_1-CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "Board_1-Net-(Q4-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 186.154178 79.196422)
		(property "Reference" "KiKit_MB_21_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 140.307699 51.448953 -30)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.586814 0.088442 330)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 330)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 330)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 150)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Board_1-ADC_LP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 330)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 203.415132 79.196427)
		(property "Reference" "KiKit_MB_22_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 96.574416 30.116173)
		(property "Reference" "KiKit_MB_1_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 196.792355 40.748953 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 2.65 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "I2C_V"
			(at 0 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 71 "Board_2-Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 67 "Board_2-Net-(J5-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 183.376957 91.043891 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 1.6 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 167 "Board_5-UPDI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 77.823913 28)
		(property "Reference" "KiKit_MB_33_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 155.630476 79.196427)
		(property "Reference" "KiKit_MB_18_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 140.369523 67.796416)
		(property "Reference" "KiKit_MB_7_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 111.023043 58.748953 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 94.584867 79.196422)
		(property "Reference" "KiKit_MB_13_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 159.407699 55.948953)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Board_1-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Board_1-UPDI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 171.392327 74.496422)
		(property "Reference" "KiKit_MB_27_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 108.856272 116.876671)
		(property "Reference" "KiKit_MB_16_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 188.576957 103.243891 180)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0.05 2.3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EV3415/SI23333"
			(at 0 2.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C344008"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Board_5-3V3CUTOFF")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "Board_5-Net-(Q3-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.673043 58.448953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.26 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Board_0-ADC_BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 194.776957 102.743891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 1.5 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "Board_5-Net-(J5-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 165 "Board_5-SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 76.823913 118.992844)
		(property "Reference" "KiKit_MB_34_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 141.457699 59.428953)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.25 0.02 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Board_1-Net-(Q1-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Board_1-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 93.584868 67.796416)
		(property "Reference" "KiKit_MB_3_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 107.887645 88.543891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -0.005 0.925 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "Board_3-+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "Board_3-ADC_BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 124.492844)
		(property "Reference" "KiKit_MB_31_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 110.711337 115.253017)
		(property "Reference" "KiKit_MB_16_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 207.102355 58.748953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0.01 -1.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Board_2-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 76.823913 28)
		(property "Reference" "KiKit_MB_33_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 20.5)
		(property "Reference" "KiKit_MB_30_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 134.407699 51.898953 -120)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.878942 -0.045577 60)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 60)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 240)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Board_1-ADC_LOAD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 240)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Board_1-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 205.192355 55.948953)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "Board_2-UPDI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 145.992301 106.243891)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 2.65 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "I2C_V"
			(at 0 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 127 "Board_4-Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 123 "Board_4-Net-(J5-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 156.630477 67.796421)
		(property "Reference" "KiKit_MB_8_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 219.176087 28)
		(property "Reference" "KiKit_MB_35_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 143.369522 79.196423)
		(property "Reference" "KiKit_MB_17_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 191.776957 106.243891)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 2.65 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "I2C_V"
			(at 0 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 155 "Board_5-Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 151 "Board_5-Net-(J5-Pin_2)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 189.112355 58.448953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -0.005 0.925 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Board_2-+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "Board_2-ADC_BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 148.607699 65.248953)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J1"
			(at 3.7 1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT+"
			(at 0 3.85 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Board_1-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 29 "Board_1-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 96.584867 79.196423)
		(property "Reference" "KiKit_MB_13_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 103.207645 102.743891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 1.5 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "Board_3-Net-(J5-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "Board_3-SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 147.007699 44.248953 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.45 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Board_1-Net-(J5-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Board_1-SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 186.476957 85.568891 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.425 -0.1 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "Board_5-Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Board_5-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 81.323913 72.496422)
		(property "Reference" "KiKit_MB_25_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 202.415133 67.796421)
		(property "Reference" "KiKit_MB_12_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 73.823913 28)
		(property "Reference" "KiKit_MB_33_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 200.415132 79.196426)
		(property "Reference" "KiKit_MB_22_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 136.392301 102.993891 -150)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J3"
			(at -3.439102 -2.043301 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT-"
			(at 0 3.85 210)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 210)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 210)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 30)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 210)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "Board_4-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 210)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 121 "Board_4-GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 204.692355 61.648953 90)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TLV61070ADBV"
			(at 0 2.4 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv61070a.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Boost Converter, 2.5A switch current limit, 2.2-5.5V Output Voltage, 0.5-5.5V Input Voltage, SOT-23-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6881375"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "Board_2-Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Board_2-GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Board_2-Net-(JP1-A)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Board_2-Net-(U1-V_{FB})")
			(pinfunction "V_{FB}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Board_2-VCC")
			(pinfunction "V_{OUT}")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Board_2-Net-(JP1-A)")
			(pinfunction "V_{IN}")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 154.630477 67.79642)
		(property "Reference" "KiKit_MB_8_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 148.492301 115.143891)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J5"
			(at 2.7 -2.7 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "QWIIC"
			(at 0 3.98 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160404"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "Board_4-ADC_SP")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "Board_4-Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "Board_4-Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "Board_4-Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 121 "Board_4-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 121 "Board_4-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 1.4 -0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 200.415133 67.79642)
		(property "Reference" "KiKit_MB_12_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 185.510124 32.698306)
		(property "Reference" "KiKit_MB_9_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 203.059187 114.294538)
		(property "Reference" "KiKit_MB_24_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 153.630476 79.196426)
		(property "Reference" "KiKit_MB_18_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 218.176087 118.992844)
		(property "Reference" "KiKit_MB_36_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 110.523043 61.423953 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.425 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Board_0-Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Board_0-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 211.592355 56.798953)
		(property "Reference" "G***"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 186.288665 115.253065)
		(property "Reference" "KiKit_MB_23_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 183.386957 88.243891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -2.21 -1.1 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "560k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C132339"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 161 "Board_5-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Board_5-VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 142.369523 67.796417)
		(property "Reference" "KiKit_MB_7_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 199.415132 79.196426)
		(property "Reference" "KiKit_MB_22_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 219.176087 118.992844)
		(property "Reference" "KiKit_MB_36_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 220.176087 28)
		(property "Reference" "KiKit_MB_35_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 71.496422)
		(property "Reference" "KiKit_MB_28_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 143.327699 58.448953 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -0.005 0.925 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Board_1-+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Board_1-ADC_BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 215.676087 74.496422)
		(property "Reference" "KiKit_MB_28_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 148.392301 81.743891 180)
		(descr "Mounting Hole 3.2mm, M3, ISO7380")
		(tags "mounting hole 3.2mm m3 iso7380")
		(property "Reference" "J1"
			(at 3.7 1.2 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BATT+"
			(at 0 3.85 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "Board_4-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" connect circle
			(at 0 0 180)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(net 113 "Board_4-+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 89.897645 88.243891)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0.01 -1.05 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Board_3-GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "Board_3-Net-(U1-V_{FB})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 195.776957 102.743891 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.45 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 153 "Board_5-Net-(J5-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 164 "Board_5-SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 140.504009 115.253065)
		(property "Reference" "KiKit_MB_19_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 113.623043 55.948953)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Board_0-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Board_0-UPDI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 189.154179 67.796417)
		(property "Reference" "KiKit_MB_11_1"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 171.392327 75.496422)
		(property "Reference" "KiKit_MB_27_6"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 171.392327 71.496422)
		(property "Reference" "KiKit_MB_27_2"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 202.246957 82.033891 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.09 1.57 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "Board_5-Net-(Q4-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "Board_5-Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 188.376957 106.243891)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F2"
			(at -2.35 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-020-9V"
			(at 0 1.65 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883102"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "Board_5-Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "Board_5-Net-(JP2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 209.426957 95.693891 60)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 1.853942 -0.088878 240)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 240)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 60)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "Board_5-ADC_LN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 60)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "Board_5-ADC_LOAD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 186.154179 67.796416)
		(property "Reference" "KiKit_MB_11_4"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 157.630476 79.196427)
		(property "Reference" "KiKit_MB_18_5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 145.492301 102.803891 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -1.51 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Board_4-VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "Board_4-3V3CUTOFF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 99.807645 86.443891)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 1.7 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MCU_VCC"
			(at 0 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 98 "Board_3-Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 85 "Board_3-+BATT")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "NPTH"
		(layer "F.Cu")
		(at 141.385603 116.117409)
		(property "Reference" "KiKit_MB_19_3"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NPTH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 102.707645 115.143891)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J5"
			(at 2.7 -2.7 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "QWIIC"
			(at 0 3.98 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160404"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "Board_3-ADC_SP")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "Board_3-Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "Board_3-Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "Board_3-Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 93 "Board_3-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 93 "Board_3-GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 1.4 -0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 207.176957 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 146 "Board_5-ADC_LP")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 194.176957 85.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 141 "Board_5-+BATT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 98.607645 103.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 86 "Board_3-3V3CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 86.823043 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 4 "Board_0-ADC_LN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 181.392355 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 62 "Board_2-ADC_LP")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 103.823043 37.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 12 "Board_0-Net-(J5-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 152.607699 43.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 30 "Board_1-3V3CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 135.607699 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 34 "Board_1-ADC_LP")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 197.176957 109.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 153 "Board_5-Net-(J5-Pin_4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 164.392301 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 116 "Board_4-ADC_LN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 106.823043 43.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "Board_0-3V3CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 157.742301 86.163891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0.35175 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 120 "Board_4-CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 102.607645 88.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 107 "Board_3-Net-(U2-PB3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 145.607699 37.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 41 "Board_1-Net-(J5-Pin_4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 161.392301 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 118 "Board_4-ADC_LP")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 105.607645 109.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 97 "Board_3-Net-(J5-Pin_4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 204.176957 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 168 "Board_5-VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 184.392355 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 84 "Board_2-VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 93.473043 60.828953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0.35175 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 8 "Board_0-CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 148.392301 85.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 113 "Board_4-+BATT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 138.607699 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 56 "Board_1-VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 106.823043 61.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 9 "Board_0-GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 158.392301 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 140 "Board_4-VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 210.176957 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 144 "Board_5-ADC_LN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 190.176957 85.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 149 "Board_5-GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 111.957645 86.163891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0.35175 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 92 "Board_3-CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 190.176957 103.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 142 "Board_5-3V3CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 149.607699 37.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 40 "Board_1-Net-(J5-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 101.607645 109.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 96 "Board_3-Net-(J5-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 89.823043 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 6 "Board_0-ADC_LP")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 195.392355 37.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 68 "Board_2-Net-(J5-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 194.392355 58.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 79 "Board_2-Net-(U2-PB3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 191.392355 37.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 69 "Board_2-Net-(J5-Pin_4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 193.176957 109.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 152 "Board_5-Net-(J5-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 139.257699 60.828953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0.35175 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 36 "Board_1-CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 194.176957 88.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 163 "Board_5-Net-(U2-PB3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 115.607645 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 90 "Board_3-ADC_LP")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 152.607699 61.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 37 "Board_1-GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 203.526957 86.163891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0.35175 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 148 "Board_5-CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 102.823043 58.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 23 "Board_0-Net-(U2-PB3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 132.607699 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 32 "Board_1-ADC_LN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 185.042355 60.828953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0.35175 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 64 "Board_2-CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 98.607645 85.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 93 "Board_3-GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 102.823043 61.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 1 "Board_0-+BATT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 92.823043 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 28 "Board_0-VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 198.392355 43.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 58 "Board_2-3V3CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 148.607699 61.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 29 "Board_1-+BATT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 178.392355 55.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 60 "Board_2-ADC_LN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 148.392301 88.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 135 "Board_4-Net-(U2-PB3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 147.392301 109.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 124 "Board_4-Net-(J5-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 198.392355 61.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 65 "Board_2-GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 151.392301 109.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 125 "Board_4-Net-(J5-Pin_4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 148.607699 58.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 51 "Board_1-Net-(U2-PB3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 118.607645 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 88 "Board_3-ADC_LN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 102.607645 85.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 85 "Board_3-+BATT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 144.392301 103.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 114 "Board_4-3V3CUTOFF")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 194.392355 61.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 57 "Board_2-+BATT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 112.607645 91.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 112 "Board_3-VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 99.823043 37.248953 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 1.448 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 13 "Board_0-Net-(J5-Pin_4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 144.392301 85.743891)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 1.448 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 121 "Board_4-GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 189.226051 26.095914)
		(end 189.270877 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.209257 60.168833)
		(end 215.351369 59.651696)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.449324 26.365241)
		(end 217.479491 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.195266 28.922977)
		(end 98.146021 28.927272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.007922 79.513228)
		(end 207.983626 79.505539)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.191284 32.185235)
		(end 157.175273 32.13782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.281462 26.403896)
		(end 97.311629 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.915132 69.997409)
		(end 199.913929 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.893388 90.124156)
		(end 172.893713 90.149637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.098164 76.164784)
		(end 189.13959 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.753098 70.991611)
		(end 184.704197 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.684118 78.24016)
		(end 188.673374 78.192318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.058829 113.986212)
		(end 185.361749 114.428777)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.869523 77.997409)
		(end 139.868319 78.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.595781 120.330396)
		(end 185.578134 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.512994 76.092336)
		(end 93.556792 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.473128 80.681283)
		(end 86.451563 80.694861)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.028894 28.916251)
		(end 143.979922 28.922977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.100477 81.700162)
		(end 84.704684 82.062065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.465626 78.799826)
		(end 139.425537 78.82806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.910322 70.095341)
		(end 199.90432 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.850327 120.188739)
		(end 139.839584 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.389267 68.324534)
		(end 157.423077 68.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.748358 85.742851)
		(end 173.738531 85.766363)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.826506 76.705427)
		(end 139.839583 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.421471 120.949827)
		(end 153.374214 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.177458 78.55244)
		(end 108.149224 78.592529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.248437 78.468352)
		(end 157.226391 78.424555)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.653191 75.996422)
		(end 198.91612 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.577477 28.791353)
		(end 97.535499 28.765249)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.40795 32.54337)
		(end 157.334986 32.44765)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.266614 28.920007)
		(end 153.217486 28.92548)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.011652 76.481833)
		(end 143.037885 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.188487 79.055406)
		(end 90.656547 79.12371)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.84113 120.962904)
		(end 97.793872 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.773948 70.900507)
		(end 107.729121 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.54141 70.737631)
		(end 139.504281 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.655166 78.996422)
		(end 183.89872 78.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.292818 28.907111)
		(end 98.244238 28.916251)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.749717 78.799831)
		(end 111.711062 78.769664)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.246902 68.001232)
		(end 112.295802 67.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.084114 56.281784)
		(end 124.036234 55.747618)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.631371 67.86523)
		(end 90.656556 67.86912)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.268074 84.244226)
		(end 167.976554 83.794068)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.730223 120.376144)
		(end 188.712576 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.249906 120.420971)
		(end 108.22786 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.536218 70.468347)
		(end 185.512049 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.115504 28.568253)
		(end 108.083001 28.605496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.506595 78.98561)
		(end 189.458283 78.977227)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.298839 70.552436)
		(end 157.272606 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.601557 61.739398)
		(end 214.820943 61.250016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.430804 80.144556)
		(end 86.956418 80.394723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.946779 26.2926)
		(end 188.982291 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.673627 76.015617)
		(end 143.721939 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.495718 68.223184)
		(end 157.534373 68.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.880335 76.848838)
		(end 142.888718 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.5444 86.266357)
		(end 173.535786 86.29034)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.658989 78.095342)
		(end 188.655382 78.046442)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.383486 76.289022)
		(end 217.417296 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.397381 91.270591)
		(end 81.472473 91.801615)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.089677 26.90108)
		(end 97.095679 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.946779 76.289022)
		(end 188.982291 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.839483 120.949827)
		(end 157.792924 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.513778 120.916799)
		(end 153.46803 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.638421 26.2926)
		(end 111.673933 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.149926 120.973648)
		(end 112.102084 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.578528 70.953405)
		(end 143.53197 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.252823 120.916799)
		(end 139.207076 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.556791 26.11796)
		(end 93.599455 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.409468 85.230442)
		(end 82.398453 85.253422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.858177 28.593379)
		(end 197.346864 28.431565)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.11326 120.962904)
		(end 139.065418 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.395839 120.99164)
		(end 107.346809 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.973204 67.937432)
		(end 136.998554 67.940031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.672934 28.084687)
		(end 195.139423 28.02999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.730223 68.613116)
		(end 188.750094 68.56829)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.870745 27.979625)
		(end 142.869522 27.930196)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.341448 68.114377)
		(end 139.384111 68.138545)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.659838 53.556026)
		(end 127.504568 54.069366)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.422522 118.20149)
		(end 199.4645 118.227594)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.037885 78.552438)
		(end 143.011652 78.511012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.504561 54.069391)
		(end 127.497809 54.093963)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.234764 70.769659)
		(end 143.197635 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.742866 55.191203)
		(end 169.738655 55.16607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.018741 28.288982)
		(end 150.993928 28.283176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.328723 26.90108)
		(end 79.334725 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.100537 76.752684)
		(end 154.111281 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.506595 70.985609)
		(end 189.458283 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.62424 120.236581)
		(end 185.611162 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.033093 76.524496)
		(end 203.057262 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.103746 95.014057)
		(end 174.363001 95.49082)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.273894 70.995218)
		(end 80.224993 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.141896 120.627602)
		(end 203.111729 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.830764 85.766381)
		(end 214.820937 85.742869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.072079 120.330396)
		(end 154.054432 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.504281 78.769659)
		(end 139.465626 78.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.624239 76.752684)
		(end 185.634983 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.129488 78.996427)
		(end 158.080458 78.995224)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.940612 120.916799)
		(end 79.895785 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.796308 68.481829)
		(end 188.822541 68.440403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.647862 79.228165)
		(end 181.125662 79.350364)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.575418 60.168839)
		(end 127.582796 60.193231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.306769 87.914719)
		(end 127.21814 88.443652)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.945567 78.379724)
		(end 142.92792 78.333976)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.111281 76.800526)
		(end 154.119664 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.576922 76.289022)
		(end 139.610732 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.994827 80.992135)
		(end 210.548428 80.694891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.874412 118.963941)
		(end 142.880512 118.914887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.793478 78.379722)
		(end 139.773608 78.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.652025 26.25879)
		(end 79.689154 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.234764 78.76966)
		(end 143.197635 78.737633)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.656342 76.324534)
		(end 199.68837 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.09762 118.39114)
		(end 152.600003 118.203428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.194124 85.230442)
		(end 128.183109 85.253422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.719905 54.069391)
		(end 81.713153 54.093963)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.905872 64.531413)
		(end 166.923307 64.512827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.443609 118.823033)
		(end 150.468687 118.818501)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.417182 83.318004)
		(end 213.081271 82.899924)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.012515 26.528074)
		(end 154.034561 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.880263 65.309408)
		(end 211.899503 65.292698)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.658551 70.878461)
		(end 157.615888 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.672927 68.400312)
		(end 139.70116 68.440401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.686491 76.164784)
		(end 153.72658 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.673627 78.977227)
		(end 143.625785 78.966484)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.656739 26.095914)
		(end 97.701565 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.903704 87.88967)
		(end 123.788181 87.365952)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.485816 78.552436)
		(end 185.457583 78.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.768158 118.992843)
		(end 148.793633 118.992193)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.55033 32.44765)
		(end 111.520991 32.407092)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.375861 76.039438)
		(end 93.422419 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.554332 114.715479)
		(end 185.575006 114.761054)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.983518 27.999999)
		(end 102.447211 27.999999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.475679 33.028065)
		(end 93.192418 33.490969)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.468167 76.072466)
		(end 93.512994 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.326313 118.866176)
		(end 108.334832 118.914868)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.702349 78.900512)
		(end 157.658551 78.878466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.47303 59.103167)
		(end 215.477882 59.07815)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.113998 78.99659)
		(end 113.101254 78.996428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.472477 91.80164)
		(end 81.476688 91.826773)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.020076 28.922959)
		(end 152.971104 28.916233)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.213862 79.052804)
		(end 91.188512 79.055403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.207076 120.934446)
		(end 139.160517 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.542416 76.400318)
		(end 111.572583 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.87051 78.996422)
		(end 138.114064 78.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.883439 89.562372)
		(end 169.849215 89.027156)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.404218 76.658869)
		(end 111.421865 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.175274 114.854967)
		(end 157.191285 114.807552)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.111721 118.908156)
		(end 147.645232 118.962853)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.20752 114.428777)
		(end 203.510441 113.986211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.15887 76.026361)
		(end 199.206127 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.214565 88.468935)
		(end 127.15306 89.001704)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.464198 86.290358)
		(end 123.455584 86.266375)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.395389 68.324529)
		(end 185.427416 68.361657)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.566519 58.549166)
		(end 215.570087 58.523933)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.334952 28.837157)
		(end 199.289575 28.856764)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.612942 120.874883)
		(end 97.570278 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.930678 118.065589)
		(end 143.979923 118.069884)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.346808 75.996422)
		(end 107.395839 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.248437 68.524496)
		(end 157.272606 68.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.966906 76.524496)
		(end 93.988952 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.196618 28.288989)
		(end 99.67771 28.424485)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.604611 68.324534)
		(end 111.638421 68.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.930677 28.927272)
		(end 143.88128 28.929126)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.260306 113.9648)
		(end 139.274159 113.986191)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.937283 78.98561)
		(end 97.888971 78.977227)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.007979 67.47962)
		(end 208.514994 67.3048)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.114101 67.996416)
		(end 138.870511 67.996416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.82254 26.443985)
		(end 188.850774 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.869523 119.993831)
		(end 139.868319 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.970549 33.501943)
		(end 128.584561 51.490844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.417216 60.193249)
		(end 169.424594 60.168857)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.313668 82.079771)
		(end 212.295307 82.0621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.443208 120.874883)
		(end 203.400544 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.616513 120.700243)
		(end 79.582703 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.867657 28.605496)
		(end 153.833351 28.641085)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.636815 120.949827)
		(end 107.589558 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.980579 68.223183)
		(end 108.017708 68.25521)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.874333 120.091763)
		(end 142.870726 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.359118 78.828065)
		(end 203.319029 78.799831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.017708 68.25521)
		(end 108.05322 68.28902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.526969 87.889676)
		(end 81.522117 87.914693)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.903714 78.631185)
		(end 153.871686 78.668313)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.878783 82.46143)
		(end 175.861348 82.480016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.461086 79.696981)
		(end 87.96366 79.897461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.803807 118.103713)
		(end 97.851585 118.091033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.638421 76.289022)
		(end 111.673933 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.024911 60.726486)
		(end 215.033525 60.702503)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.711062 70.769659)
		(end 111.673933 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.721939 70.985609)
		(end 143.673627 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.839088 120.376144)
		(end 199.819218 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.009002 118.992192)
		(end 103.54461 118.964807)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.258948 66.598107)
		(end 164.281178 66.585649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.719625 78.769659)
		(end 93.68097 78.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.919943 26.90108)
		(end 202.925945 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.034561 78.424553)
		(end 154.012516 78.468351)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.130476 68.995434)
		(end 157.13168 68.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.119488 118.914868)
		(end 154.125588 118.963922)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.88827 26.403896)
		(end 93.916504 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.684118 70.240159)
		(end 188.673374 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.493405 120.982031)
		(end 107.44474 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.012671 118.31789)
		(end 108.048695 118.351739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.558762 79.123719)
		(end 160.026821 79.055414)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.270878 70.920377)
		(end 189.226051 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.640881 120.824481)
		(end 93.599455 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.238374 66.859602)
		(end 133.724916 67.085221)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.515018 67.304791)
		(end 208.538889 67.295872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.704197 75.997625)
		(end 184.753098 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.622532 78.703825)
		(end 199.58702 78.737636)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.058075 76.193017)
		(end 189.098164 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.143264 120.330396)
		(end 97.127884 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.224993 70.991611)
		(end 80.176329 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.129489 70.996422)
		(end 158.080458 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.243245 26.25879)
		(end 203.280374 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.18461 118.203428)
		(end 190.686994 118.39114)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.224993 120.988033)
		(end 80.176329 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.664991 70.144005)
		(end 188.658989 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.625786 68.026356)
		(end 143.673628 68.015613)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.427416 120.627602)
		(end 185.395389 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.012516 120.464769)
		(end 153.988348 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.206127 70.953405)
		(end 199.15887 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.319029 78.799831)
		(end 203.280374 78.769664)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.549891 76.223184)
		(end 199.58702 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.412979 78.737633)
		(end 97.377467 78.703823)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.611161 26.709005)
		(end 185.624239 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.15887 68.026359)
		(end 199.206127 68.039437)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.793478 120.376144)
		(end 139.773608 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34582 68.995432)
		(end 108.34582 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.365016 70.192317)
		(end 111.356633 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.789806 70.828059)
		(end 111.749717 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.281463 120.588947)
		(end 97.253229 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.957636 28.881684)
		(end 189.910198 28.895579)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.965437 78.42455)
		(end 142.945567 78.379724)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.775006 26.00481)
		(end 216.82367 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.129489 67.996421)
		(end 158.885935 67.996421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.065418 68.015612)
		(end 139.11326 68.026355)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.860409 70.854292)
		(end 107.817746 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.747176 76.072466)
		(end 157.792924 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.72658 120.796248)
		(end 153.686491 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.888972 68.015613)
		(end 97.937283 68.00723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.490459 67.085235)
		(end 117.977 66.859617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.141289 76.848838)
		(end 157.149672 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.429721 78.854297)
		(end 199.387058 78.878465)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.119664 70.144005)
		(end 154.111281 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.846385 54.614612)
		(end 123.717527 54.094016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.421471 68.039437)
		(end 153.46803 68.054818)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.054432 120.376144)
		(end 154.034562 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.149925 26.019195)
		(end 112.198237 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.914144 78.996427)
		(end 203.865114 78.995224)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.246901 76.001232)
		(end 112.295802 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.23245 26.010812)
		(end 93.280761 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.128923 28.087936)
		(end 104.103647 28.08469)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.673374 78.192318)
		(end 188.664991 78.144007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.909696 114.585751)
		(end 93.936961 114.627717)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.048695 28.641085)
		(end 108.01267 28.674934)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.898985 79.35682)
		(end 115.874329 79.350382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.655382 76.946403)
		(end 188.658989 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.531702 67.636023)
		(end 89.556358 67.642461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.196602 118.703861)
		(end 100.221415 118.709667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.97353 26.662447)
		(end 202.991177 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.803397 28.288982)
		(end 196.778584 28.283176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.366212 93.965803)
		(end 123.547491 93.461061)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.527522 55.191203)
		(end 215.523311 55.16607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.168767 78.854292)
		(end 185.126104 78.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.877089 65.666368)
		(end 119.897156 65.650662)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.279736 118.136079)
		(end 189.326027 118.11874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.556325 79.35037)
		(end 89.531668 79.356808)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.011652 78.511012)
		(end 142.987483 78.468348)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.468167 26.076044)
		(end 93.512994 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.669836 65.292681)
		(end 176.689075 65.309391)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.664992 120.140427)
		(end 188.658989 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.916504 26.443985)
		(end 93.942737 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.143264 70.333974)
		(end 97.127883 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.054432 76.613121)
		(end 154.072079 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.659862 93.436812)
		(end 127.667861 93.461007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.68097 76.193017)
		(end 93.719625 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.229395 26.00481)
		(end 153.27806 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.561744 84.752872)
		(end 168.54957 84.730484)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.354725 118.962853)
		(end 149.888236 118.908156)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.077474 28.907111)
		(end 144.028894 28.916251)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.769675 32.27742)
		(end 139.746745 32.321903)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.202827 76.524496)
		(end 97.226996 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.880941 76.361663)
		(end 188.912969 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.225973 28.404627)
		(end 108.201428 28.447535)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.773003 26.485411)
		(end 199.797171 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.084867 77.997411)
		(end 97.084867 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.398471 61.739404)
		(end 82.409486 61.762383)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.602401 26.11796)
		(end 153.645065 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.483418 84.244226)
		(end 122.191898 83.794068)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.114806 68.75268)
		(end 97.127883 68.705423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.083495 70.552436)
		(end 203.057262 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.652924 31.892106)
		(end 185.649167 31.94201)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.901835 120.824481)
		(end 107.860409 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.041789 91.80164)
		(end 173.046 91.826773)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.226391 78.424555)
		(end 157.206521 78.379728)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.497822 92.898852)
		(end 127.504575 92.923425)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.808115 63.198796)
		(end 174.822509 63.219825)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.576922 70.703821)
		(end 139.54141 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.437815 118.561286)
		(end 145.4623 118.568352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.522787 52.001487)
		(end 82.290976 52.485109)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.46666 79.011753)
		(end 159.44121 79.010452)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.507724 26.443985)
		(end 217.533957 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.325116 70.04644)
		(end 79.323913 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.957508 80.681286)
		(end 118.496513 80.407222)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.313508 78.828061)
		(end 143.273419 78.799827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.572848 59.62691)
		(end 169.688369 59.103192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.994877 66.00071)
		(end 211.015721 65.986048)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.522113 87.914719)
		(end 81.433484 88.443652)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.033021 28.360558)
		(end 154.010629 28.404627)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.244828 33.501933)
		(end 112.238317 33.490979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.871686 70.668309)
		(end 153.837876 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.468029 70.938024)
		(end 153.421471 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.656891 26.804104)
		(end 217.665274 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.040552 118.503667)
		(end 143.069217 118.463395)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.48795 68.481833)
		(end 111.514183 68.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.22786 68.524495)
		(end 108.249906 68.568293)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.429909 88.468935)
		(end 81.368404 89.001704)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.767549 68.007234)
		(end 203.816214 68.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.425537 120.824481)
		(end 139.384111 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.591656 28.79896)
		(end 98.480863 28.846939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.206339 95.490856)
		(end 214.465591 95.014093)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.110969 118.866176)
		(end 154.119488 118.914868)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.182253 76.114382)
		(end 189.226051 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.561332 79.513223)
		(end 180.054317 79.688043)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.572583 68.361662)
		(end 111.604611 68.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.564981 118.127385)
		(end 198.611675 118.111159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.574462 68.164783)
		(end 157.615888 68.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.359118 26.168362)
		(end 203.400544 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.053686 114.90318)
		(end 94.064873 114.951958)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.88518 65.292681)
		(end 130.904419 65.309391)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.796308 70.51101)
		(end 188.772139 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.318215 65.650646)
		(end 131.338283 65.666352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.833351 118.351739)
		(end 153.867657 118.387329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.335008 70.144005)
		(end 108.326625 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.149225 68.400317)
		(end 108.177458 68.440405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.858104 68.361657)
		(end 93.888271 68.400312)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.480863 118.145923)
		(end 98.591615 118.193883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.119663 26.852416)
		(end 154.125666 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.945567 120.376144)
		(end 142.92792 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.099838 28.568272)
		(end 143.069216 28.529466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.024059 114.807608)
		(end 94.04007 114.855023)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.864712 68.897497)
		(end 139.868319 68.946397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.649368 70.095341)
		(end 185.643366 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.574462 70.828059)
		(end 157.534373 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.252823 78.920377)
		(end 139.207075 78.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.441735 26.571872)
		(end 111.463781 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.134885 26.001203)
		(end 93.183785 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.451541 80.694875)
		(end 86.005143 80.992119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.253229 68.440403)
		(end 97.281463 68.400314)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.034562 70.424549)
		(end 154.012516 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.206303 51.502012)
		(end 214.200073 51.490895)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.399972 28.789424)
		(end 144.376336 28.79895)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.935183 82.880436)
		(end 83.91872 82.899887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.946313 32.089663)
		(end 202.935126 32.040885)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.934196 66.585633)
		(end 86.956426 66.598092)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4525 53.531806)
		(end 173.444502 53.556002)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.065671 120.188739)
		(end 94.054928 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.674883 76.946403)
		(end 217.676087 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.643366 120.140427)
		(end 185.634983 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.668095 89.562372)
		(end 215.633871 89.027156)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.656343 68.324533)
		(end 199.68837 68.361661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.675599 90.149658)
		(end 215.675924 90.124177)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.127883 78.287417)
		(end 97.114806 78.24016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.280374 120.766081)
		(end 203.243246 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.741104 66.598104)
		(end 133.215491 66.848272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.884416 89.587862)
		(end 169.88344 89.562397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.080056 78.095341)
		(end 94.074054 78.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.682065 67.981095)
		(end 114.216799 67.940042)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.520508 70.592525)
		(end 79.492275 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.672899 67.769849)
		(end 182.200658 67.865226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.032918 120.949827)
		(end 79.98636 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.286853 92.898855)
		(end 215.415709 92.378257)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.711134 118.399464)
		(end 191.222447 118.561278)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.126104 76.114382)
		(end 185.168767 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.656342 26.328112)
		(end 199.688369 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.48795 26.485411)
		(end 111.514182 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.104214 120.896929)
		(end 217.059387 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.100052 118.817965)
		(end 154.110969 118.866176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.751634 118.632285)
		(end 188.774026 118.588216)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.590531 61.762401)
		(end 214.601546 61.739421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.630788 95.501988)
		(end 122.637021 95.490867)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.057262 70.51101)
		(end 203.033093 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.549891 78.769663)
		(end 199.511236 78.79983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.945072 70.240159)
		(end 202.934328 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.417296 76.324534)
		(end 217.449324 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.885948 67.996421)
		(end 158.898691 67.996259)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.017708 120.734053)
		(end 107.98058 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.945072 76.752684)
		(end 202.958149 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.13959 26.142129)
		(end 189.182253 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.942737 26.485411)
		(end 93.966905 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.486222 76.072466)
		(end 143.53197 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.648029 63.654549)
		(end 167.962154 63.219864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.506273 114.627717)
		(end 185.531402 114.670996)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.280374 78.769664)
		(end 203.243245 78.737637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.839482 68.039438)
		(end 157.88674 68.02636)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.985948 120.988033)
		(end 97.937283 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.188548 67.937432)
		(end 91.213898 67.940031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.273419 70.799826)
		(end 143.234764 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.953891 61.226462)
		(end 127.963718 61.249974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.773003 68.481831)
		(end 199.797172 68.524495)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.249906 70.424549)
		(end 108.22786 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.206521 78.379728)
		(end 157.188874 78.33398)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.654179 77.997411)
		(end 188.654179 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.711062 26.226762)
		(end 111.749717 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.324076 90.124156)
		(end 81.324401 90.149637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.38231 120.330396)
		(end 79.366929 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.058075 26.196595)
		(end 189.098164 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.356633 78.144011)
		(end 111.350631 78.095346)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.868534 78.996423)
		(end 143.819504 78.99522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.654179 76.995434)
		(end 185.654179 77.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.533511 81.342197)
		(end 85.119755 81.683418)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.926263 53.003268)
		(end 214.719446 52.508443)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.751562 70.468347)
		(end 139.727393 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.925945 70.144005)
		(end 202.919943 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.128017 76.015617)
		(end 80.176329 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.982292 120.734053)
		(end 188.946779 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.819504 75.997625)
		(end 143.868535 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.914145 70.996422)
		(end 203.865114 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.417221 63.674837)
		(end 213.43267 63.65457)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.725976 82.062082)
		(end 120.330182 81.700179)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.77214 120.464769)
		(end 188.750094 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.116811 93.461037)
		(end 215.124809 93.436841)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.23542 28.922959)
		(end 107.186448 28.916233)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.162123 70.703821)
		(end 143.128313 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.850074 68.015612)
		(end 184.897916 68.026355)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.570278 26.142129)
		(end 97.612941 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.503232 84.265989)
		(end 174.235078 84.730444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.15084 53.027047)
		(end 169.141616 53.003292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.131464 78.996426)
		(end 143.868534 78.996423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.468728 28.174342)
		(end 150.443651 28.16981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.725826 33.006631)
		(end 157.422906 32.564066)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.083879 75.996422)
		(end 107.346808 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.417296 120.664731)
		(end 217.383486 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.203691 76.481833)
		(end 108.22786 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.874333 78.095342)
		(end 142.870726 78.046442)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.558604 70.900507)
		(end 153.513777 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.443207 68.114382)
		(end 203.487005 68.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.710761 54.069394)
		(end 123.555488 53.556056)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.344617 120.042862)
		(end 108.34101 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.611162 78.287416)
		(end 185.595781 78.333975)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.531832 76.072466)
		(end 203.57758 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.720478 28.737083)
		(end 153.679843 28.765231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.183785 78.991611)
		(end 93.134885 78.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.656739 68.092332)
		(end 97.701566 68.072462)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.354934 26.142129)
		(end 143.397597 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.934812 94.484434)
		(end 169.141626 93.989606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.084867 77.997409)
		(end 94.083663 78.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.148012 76.114382)
		(end 217.190675 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.965151 75.997625)
		(end 199.014052 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.424601 60.168833)
		(end 169.566713 59.651696)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.671395 76.026361)
		(end 203.719237 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.366929 76.705427)
		(end 79.38231 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.687018 118.391149)
		(end 190.711109 118.399456)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.432685 63.654549)
		(end 213.74681 63.219864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.409497 61.762406)
		(end 82.653587 62.239949)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.141607 53.003268)
		(end 168.93479 52.508443)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34101 26.90108)
		(end 108.344617 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.72658 70.799826)
		(end 153.686491 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.68097 120.796248)
		(end 93.640881 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.767898 120.824481)
		(end 79.727809 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.207733 120.700243)
		(end 203.173923 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.288937 76.223184)
		(end 185.326066 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.017106 68.007229)
		(end 139.065418 68.015612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.248437 70.468347)
		(end 157.226391 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.162123 26.2926)
		(end 143.197635 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.399957 26.616699)
		(end 79.419827 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.054432 26.616699)
		(end 154.072079 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.375861 120.949827)
		(end 93.328604 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.751122 86.290364)
		(end 127.582791 86.79957)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.721938 26.010812)
		(end 143.770603 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.966906 120.464769)
		(end 93.942737 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.104062 26.804104)
		(end 97.114805 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.602627 91.270589)
		(end 215.605549 91.245274)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.03351 86.290358)
		(end 215.024896 86.266375)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.831232 68.138551)
		(end 111.873895 68.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.90432 120.140427)
		(end 199.895937 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.513777 78.920381)
		(end 153.468029 78.938028)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.08746 68.705426)
		(end 154.100537 68.752683)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.975088 86.266357)
		(end 81.966474 86.29034)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.356951 53.003268)
		(end 123.150134 52.508443)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.45041 84.730467)
		(end 128.438236 84.752854)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.470942 82.079772)
		(end 130.094145 82.461412)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.225974 118.588197)
		(end 108.248366 118.632267)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.602618 55.722252)
		(end 215.527526 55.191228)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.782513 28.925498)
		(end 143.733385 28.920025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.08703 78.668313)
		(end 108.05322 78.703825)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.512994 120.896929)
		(end 93.468167 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.941924 120.796248)
		(end 107.901835 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 207.983602 79.505532)
		(end 207.468322 79.356827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.328723 120.091763)
		(end 79.325116 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.919824 26.029939)
		(end 216.967081 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.095679 78.144007)
		(end 97.089677 78.095342)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.037831 83.773)
		(end 129.023437 83.794029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.756754 70.737631)
		(end 93.719625 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.207733 78.703827)
		(end 203.173922 78.668314)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.574484 66.000708)
		(end 178.020883 66.297952)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.922525 28.907093)
		(end 152.874457 28.895561)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.064557 89.027131)
		(end 124.062282 89.001749)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.135287 78.095346)
		(end 157.13168 78.046446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.82367 70.985609)
		(end 216.775006 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.684604 118.817983)
		(end 188.697893 118.770371)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.083495 76.440407)
		(end 203.111728 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.031557 26.00481)
		(end 158.080458 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.63256 60.193249)
		(end 123.639938 60.168857)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.962114 78.55244)
		(end 153.93388 78.592529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.748683 67.98109)
		(end 91.774133 67.982391)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.504281 68.223179)
		(end 139.54141 68.255206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.012516 68.524495)
		(end 154.034562 68.568293)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.203691 78.511014)
		(end 108.177458 78.55244)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.860409 78.854297)
		(end 107.817746 78.878465)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.27219 26.196595)
		(end 217.310845 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.68837 68.361661)
		(end 199.718537 68.400317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.69323 59.078124)
		(end 169.781859 58.549191)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.858363 53.003261)
		(end 127.84914 53.027016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.945072 78.240164)
		(end 202.934328 78.192322)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.773607 26.571872)
		(end 139.793477 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.329307 28.028036)
		(end 148.7937 28.000651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.488763 78.799827)
		(end 97.450108 78.76966)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.856735 26.662447)
		(end 199.872115 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.240327 28.706978)
		(end 143.202672 28.674953)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.005172 66.000708)
		(end 86.451571 66.297952)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.312981 28.601694)
		(end 106.28889 28.593387)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.841129 78.966484)
		(end 97.793872 78.953406)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.851585 118.091033)
		(end 97.899932 118.080733)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.891267 56.868687)
		(end 169.890942 56.843206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.572831 87.365927)
		(end 169.566708 87.34119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.615888 120.850714)
		(end 157.574462 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.903714 68.361661)
		(end 153.933881 68.400317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.452525 93.461031)
		(end 173.633806 93.965772)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.141822 118.399464)
		(end 99.653135 118.561278)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.129273 76.946403)
		(end 154.130476 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.767549 26.010812)
		(end 203.816213 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.895937 120.188739)
		(end 199.885194 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.864511 31.94201)
		(end 139.858259 31.991663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.065671 76.800526)
		(end 94.074054 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.910322 120.091763)
		(end 199.90432 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.913563 118.904904)
		(end 150.443584 118.823037)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.633815 93.965796)
		(end 173.643039 93.989551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.769676 114.715479)
		(end 139.79035 114.761054)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.231825 118.992844)
		(end 148.768132 118.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.3271 79.222994)
		(end 114.799341 79.127617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.180781 26.571872)
		(end 97.202827 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.43283 28.92548)
		(end 107.383491 28.928516)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.029484 33.501933)
		(end 158.022973 33.490979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.23245 76.007234)
		(end 93.280762 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.043551 80.394739)
		(end 209.569164 80.144571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.955008 113.964778)
		(end 112.238269 113.501874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.495718 120.766081)
		(end 157.45859 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.797171 26.528074)
		(end 199.819217 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.08607 120.042862)
		(end 97.084867 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.60416 26.001203)
		(end 189.65319 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.520508 120.588947)
		(end 79.492275 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.248366 118.632267)
		(end 108.268551 118.67739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.919943 78.095346)
		(end 202.916336 78.046446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.353852 26.756262)
		(end 79.366929 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.512049 26.485411)
		(end 185.536217 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.751562 78.468347)
		(end 139.727393 78.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.486222 78.920378)
		(end 143.441395 78.900508)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.953865 85.766387)
		(end 127.759753 86.266333)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.774159 67.982392)
		(end 92.316676 67.996252)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.925945 26.852416)
		(end 202.934328 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.850775 120.588947)
		(end 188.822541 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.177459 120.548858)
		(end 108.149225 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.792452 114.428798)
		(end 93.807378 114.449453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.469244 118.080733)
		(end 189.518041 118.072836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.658989 120.091763)
		(end 188.655382 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.289575 28.856764)
		(end 199.243284 28.874103)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.365016 68.800526)
		(end 111.37576 68.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.042363 118.111159)
		(end 107.089801 118.097264)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.357239 70.63118)
		(end 157.327072 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.340886 118.097282)
		(end 98.388325 118.111178)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.488763 70.799826)
		(end 97.450108 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.913929 78.046444)
		(end 199.910322 78.095345)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.522126 59.07813)
		(end 81.526978 59.103148)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.654179 69.997409)
		(end 185.652975 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.119664 68.848836)
		(end 154.125666 68.897501)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.654178 27.930196)
		(end 188.654178 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.861374 64.51281)
		(end 175.878809 64.531395)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.377467 120.700243)
		(end 97.343657 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.421865 26.616699)
		(end 111.441735 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.916387 115.100737)
		(end 202.920144 115.050833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.872115 26.709005)
		(end 199.885193 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.533957 26.485411)
		(end 217.558126 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.952803 28.928516)
		(end 198.903375 28.929108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.363184 78.953406)
		(end 189.316625 78.938025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.062716 78.985613)
		(end 199.014051 78.991615)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.489544 33.006653)
		(end 93.475692 33.028043)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.727393 76.481833)
		(end 139.751562 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.813551 118.07661)
		(end 189.86213 118.08575)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.582703 120.664731)
		(end 79.550675 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.910322 26.90108)
		(end 199.913929 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.114806 78.24016)
		(end 97.104062 78.192318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.908561 87.914713)
		(end 123.903709 87.889695)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.578528 76.039438)
		(end 143.625785 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.986085 118.54529)
		(end 154.01063 118.588197)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.136734 79.22817)
		(end 161.111781 79.222999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.874333 26.90108)
		(end 142.880335 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.529057 64.913071)
		(end 166.905854 64.531431)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.427416 76.361663)
		(end 185.457583 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.347074 31.89205)
		(end 111.34582 31.842008)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.824725 32.137876)
		(end 139.808714 32.185291)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.935442 57.965712)
		(end 172.937717 57.991094)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.072079 26.662447)
		(end 154.087459 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.811125 68.658863)
		(end 139.826506 68.705421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.234763 26.226762)
		(end 143.273419 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.02119 85.230437)
		(end 122.7771 84.752894)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.886052 28.028037)
		(end 101.860643 28.029988)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.246901 70.991611)
		(end 112.198237 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.839088 76.613121)
		(end 199.856735 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.217486 118.067345)
		(end 153.266614 118.072818)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.937282 26.010812)
		(end 97.985947 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.455599 60.726486)
		(end 123.464213 60.702503)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.476693 91.826798)
		(end 81.578801 92.353296)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.793872 68.039434)
		(end 97.84113 68.026356)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.846942 57.991114)
		(end 169.849217 57.965732)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.988952 120.420971)
		(end 93.966906 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.420897 28.901828)
		(end 189.373119 28.889149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.495079 28.856783)
		(end 143.449702 28.837176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.822541 68.440403)
		(end 188.850775 68.400314)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.991177 70.379722)
		(end 202.97353 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.784485 80.14456)
		(end 163.761648 80.133252)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.924378 94.507711)
		(end 168.934802 94.484457)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.885193 68.752683)
		(end 199.895937 68.800525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.026469 78.333975)
		(end 94.008822 78.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.192411 33.49098)
		(end 93.185899 33.501932)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.934329 120.188739)
		(end 202.925946 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.826077 68.324529)
		(end 93.858104 68.361657)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.188874 78.33398)
		(end 157.173493 78.287422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.2001 95.501988)
		(end 214.206333 95.490867)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.094171 64.531414)
		(end 130.470969 64.913054)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.455672 118.285884)
		(end 97.494865 118.25576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.684816 28.568253)
		(end 199.652313 28.605496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.257133 91.80164)
		(end 127.261344 91.826773)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.642916 115.001236)
		(end 185.649168 115.050889)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.207075 26.058397)
		(end 139.252823 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.633787 53.02704)
		(end 173.452508 53.531782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.057262 76.481833)
		(end 203.083495 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.058075 120.796248)
		(end 189.01942 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.60461 26.328112)
		(end 111.638421 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.591638 118.193893)
		(end 98.615274 118.203419)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.673972 28.874103)
		(end 107.62688 28.88913)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.747313 26.058397)
		(end 97.793872 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.246902 120.988033)
		(end 112.198237 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.54141 120.734053)
		(end 139.504281 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.34684 28.431557)
		(end 197.322355 28.424491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.023423 83.79405)
		(end 128.731904 84.244208)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.024984 118.285884)
		(end 189.064177 118.25576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.131465 120.992844)
		(end 143.868535 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.054826 78.95341)
		(end 112.008267 78.938029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.335007 26.852416)
		(end 108.34101 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.219674 28.865458)
		(end 144.17298 28.881684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.341448 78.878461)
		(end 139.29765 78.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.325158 126.992573)
		(end 73.33616 126.992843)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.541409 26.25879)
		(end 139.576922 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.361578 78.703821)
		(end 185.326066 78.737632)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.658551 26.11796)
		(end 157.702349 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.604611 70.668309)
		(end 111.572583 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.013914 28.447553)
		(end 142.989369 28.404646)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.417196 86.799588)
		(end 169.248863 86.290382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.886001 67.996253)
		(end 183.898745 67.996415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.419827 120.420971)
		(end 79.399957 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.872116 78.28742)
		(end 199.856735 78.333979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.345821 115.150779)
		(end 111.347075 115.100737)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.351358 87.341166)
		(end 215.209245 86.824029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.912968 78.66831)
		(end 188.880941 78.631182)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.764933 62.262376)
		(end 122.777107 62.239989)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.704197 26.001203)
		(end 184.753097 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.288937 26.226762)
		(end 185.326065 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.582817 63.674839)
		(end 83.918728 64.092919)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.389266 26.328112)
		(end 157.423077 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.441395 70.900507)
		(end 143.397597 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.125542 118.097282)
		(end 144.172981 118.111178)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.083879 67.996417)
		(end 107.346809 67.99642)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.365016 76.800526)
		(end 111.37576 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.653599 62.239971)
		(end 82.665773 62.262359)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.839583 70.240159)
		(end 139.826506 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.054826 26.043016)
		(end 112.102083 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.083494 26.443985)
		(end 203.111728 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.36613 57.965712)
		(end 81.368405 57.991094)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.083878 78.996423)
		(end 98.034848 78.99522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.837876 78.703825)
		(end 153.802364 78.737636)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.749717 26.196595)
		(end 111.789806 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.526983 59.103173)
		(end 81.642506 59.626891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.60461 78.668314)
		(end 111.572583 78.631186)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.129597 56.307244)
		(end 127.109057 56.843159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.062286 57.991114)
		(end 124.064561 57.965732)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.901835 78.828064)
		(end 107.860409 78.854297)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.00433 118.127403)
		(end 190.050175 118.145923)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.801762 120.982031)
		(end 184.753098 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.129489 26)
		(end 184.655166 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.799316 79.127613)
		(end 114.774131 79.123723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.87051 75.996422)
		(end 138.919541 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.253253 32.321847)
		(end 157.230323 32.277364)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.729121 68.072465)
		(end 107.773948 68.092335)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.119664 120.140427)
		(end 154.111281 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.719238 120.973648)
		(end 203.671396 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.915132 31.842008)
		(end 202.915132 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.365016 78.192322)
		(end 111.356633 78.144011)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.217486 28.92548)
		(end 153.168147 28.928516)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.899932 28.912129)
		(end 97.851585 28.901828)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.207547 32.564045)
		(end 203.192621 32.54339)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.853978 118.065571)
		(end 198.903375 118.063717)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.870746 119.013237)
		(end 142.874412 118.963941)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.272606 120.507432)
		(end 157.248438 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.182253 26.11796)
		(end 189.226051 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.869523 76.995434)
		(end 142.870726 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.210193 76.164784)
		(end 185.250282 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.748622 79.011748)
		(end 91.213888 79.052801)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.655166 26)
		(end 184.704197 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.638421 70.703821)
		(end 111.604611 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.095856 118.914887)
		(end 97.104375 118.866194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.252685 78.938028)
		(end 199.206127 78.953409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.63307 76.705427)
		(end 217.646147 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.169209 85.766387)
		(end 81.975097 86.266333)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.441395 76.092336)
		(end 143.486222 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.549892 120.766081)
		(end 199.511236 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.919541 78.995218)
		(end 138.87051 78.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.213923 67.940033)
		(end 91.748658 67.981088)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.313508 76.164784)
		(end 143.354934 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.97353 76.658869)
		(end 202.991177 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.023459 63.198796)
		(end 129.037853 63.219825)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.269776 120.376144)
		(end 108.249906 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.807588 113.501863)
		(end 203.8141 113.490911)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.761723 33.49098)
		(end 184.755211 33.501932)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.642915 31.991663)
		(end 185.634185 32.040941)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.075621 52.485132)
		(end 128.065197 52.508386)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.368958 92.378231)
		(end 127.497816 92.898827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.084867 68.995428)
		(end 94.084867 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.150868 93.965803)
		(end 169.332147 93.461061)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.150786 57.965712)
		(end 127.153061 57.991094)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.744356 82.079771)
		(end 120.725995 82.0621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.719625 120.766081)
		(end 93.68097 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.315881 78.240163)
		(end 108.302804 78.28742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.488763 26.196595)
		(end 97.528852 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.589557 26.029939)
		(end 107.636815 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.547499 93.461037)
		(end 123.555497 93.436841)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.837876 70.703821)
		(end 153.802364 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.686491 68.164782)
		(end 153.72658 68.193016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.328723 76.897502)
		(end 79.334725 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.687035 28.601703)
		(end 190.184652 28.789415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.947234 84.24423)
		(end 82.933933 84.265967)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.23831 33.490968)
		(end 111.95505 33.028065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.269694 67.304786)
		(end 134.776709 67.479607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.489517 113.986212)
		(end 93.792437 114.428777)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.388837 26.709005)
		(end 111.404218 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.901213 89.562376)
		(end 172.900237 89.587841)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.839088 78.379727)
		(end 199.819217 78.424553)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.449702 28.837176)
		(end 143.40535 28.815348)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.719625 26.226762)
		(end 93.756753 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.895936 26.804104)
		(end 199.904319 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.344832 78.996427)
		(end 112.295802 78.995224)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.194153 61.762406)
		(end 128.438243 62.239949)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.658989 26.90108)
		(end 188.664991 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.421865 70.379722)
		(end 111.404218 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.374213 26.029939)
		(end 153.421471 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.441873 76.524496)
		(end 79.466042 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.838341 32.089719)
		(end 139.824725 32.137876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.311629 76.361663)
		(end 97.343657 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.719237 78.977231)
		(end 203.671395 78.966488)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.429721 26.142129)
		(end 199.471147 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.017106 120.982031)
		(end 138.968442 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.618007 118.351739)
		(end 199.652313 118.387329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.831232 26.142129)
		(end 111.873895 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.160911 68.613116)
		(end 97.180782 68.56829)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.298838 26.443985)
		(end 157.327072 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.441395 68.092332)
		(end 143.486222 68.072462)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.368688 67.865236)
		(end 206.896446 67.76986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.395839 70.995218)
		(end 107.346808 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.880335 78.144007)
		(end 142.874333 78.095342)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.998518 79.052804)
		(end 136.973168 79.055403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.447185 28)
		(end 102.42171 28.00065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.190006 28.815348)
		(end 189.146789 28.791353)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.868319 68.946397)
		(end 139.869523 68.995428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.148102 54.639521)
		(end 173.045996 55.16602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.951304 28.641104)
		(end 188.916998 28.605514)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.636815 26.043016)
		(end 107.683373 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.869523 69.997409)
		(end 142.869523 68.995429)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.623294 32.54337)
		(end 111.55033 32.44765)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.85871 120.140427)
		(end 139.850327 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.235098 62.262381)
		(end 174.503253 62.726837)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.441177 79.123713)
		(end 136.415993 79.127603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.347075 115.100737)
		(end 111.350832 115.050833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.232101 76.164784)
		(end 217.27219 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.200067 51.490884)
		(end 203.814147 33.501944)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.450108 68.22318)
		(end 97.488763 68.193013)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.273419 68.193013)
		(end 143.313508 68.164779)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.655382 78.046442)
		(end 188.654179 77.997411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.315943 28.174347)
		(end 191.790793 28.283171)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.076718 64.51281)
		(end 130.094153 64.531395)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.130477 119.062647)
		(end 154.130477 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.888271 70.592525)
		(end 93.858104 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.387058 68.114381)
		(end 199.429721 68.138549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.135287 70.095341)
		(end 157.13168 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.915132 77.997415)
		(end 202.915132 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.793872 70.953405)
		(end 97.747314 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.22786 70.468347)
		(end 108.203691 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.419827 70.424549)
		(end 79.399957 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.967754 85.253445)
		(end 173.748368 85.742827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.898707 78.996422)
		(end 183.885964 78.996584)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.407924 114.449453)
		(end 157.42285 114.428798)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.898654 78.99659)
		(end 158.88591 78.996428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.802363 26.25879)
		(end 153.837876 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.841129 70.966482)
		(end 97.793872 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.658989 68.897498)
		(end 188.664991 68.848833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.512049 68.481827)
		(end 185.536218 68.524491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.860409 120.850714)
		(end 107.817746 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.160416 68.752684)
		(end 157.173493 68.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.956448 66.598104)
		(end 87.430835 66.848272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.692519 52.0015)
		(end 168.680921 51.978809)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.172981 118.111178)
		(end 144.219674 118.127403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.252823 26.076044)
		(end 139.29765 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.945173 78.953405)
		(end 184.897915 78.966483)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.177458 26.443985)
		(end 108.203691 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.885193 70.240159)
		(end 199.872116 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.183786 70.991611)
		(end 93.134885 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.888243 67.769849)
		(end 136.416002 67.865226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.817678 118.632267)
		(end 199.837863 118.67739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.330163 81.700162)
		(end 120.310924 81.683452)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.037479 68.07246)
		(end 185.082306 68.092331)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.138625 82.480033)
		(end 121.12119 82.461448)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.993903 28.28317)
		(end 150.468753 28.174347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.533559 65.650646)
		(end 85.553627 65.666352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.477175 52.0015)
		(end 214.465577 51.978809)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.717541 92.898855)
		(end 123.846397 92.378257)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.689154 76.223184)
		(end 79.727809 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.64276 120.627602)
		(end 139.610733 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.643366 76.848838)
		(end 185.649368 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.553647 65.666367)
		(end 85.984287 65.986017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.248854 86.290358)
		(end 169.24024 86.266375)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.602402 68.114381)
		(end 153.645065 68.138549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.203691 26.485411)
		(end 108.227859 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.033533 60.702479)
		(end 215.201864 60.193273)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.825208 28.489194)
		(end 188.79857 28.447553)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.34326 26.095914)
		(end 199.387057 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.27952 28.737101)
		(end 143.240327 28.706978)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.395839 78.995222)
		(end 107.346808 78.996426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.636815 78.953409)
		(end 107.589557 78.966487)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.510482 33.006631)
		(end 203.207562 32.564066)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.936961 32.365182)
		(end 93.909696 32.407148)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.988952 68.568288)
		(end 94.008822 68.613115)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.923281 82.480033)
		(end 166.905846 82.461448)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.856735 120.330396)
		(end 199.839088 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.387057 26.11796)
		(end 199.429721 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.661696 81.326476)
		(end 165.231056 81.006826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.785434 58.523908)
		(end 169.846939 57.991139)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.467051 67.095372)
		(end 117.490436 67.085245)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.656739 120.896929)
		(end 97.612942 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.895785 76.092336)
		(end 79.940612 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.226996 76.481833)
		(end 97.253229 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.604611 76.324534)
		(end 111.638421 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.344833 70.996422)
		(end 112.295802 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.34582 26.999012)
		(end 111.347024 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.584555 51.490855)
		(end 128.578322 51.501976)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.398442 85.253445)
		(end 82.179056 85.742827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.945706 67.304791)
		(end 116.969577 67.295872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.006112 28.283176)
		(end 145.981299 28.288983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.323913 76.995434)
		(end 79.325116 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.211824 59.626916)
		(end 173.217947 59.651653)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.541716 76.015617)
		(end 107.589558 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.109056 56.843185)
		(end 127.108731 56.868666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.793696 95.490831)
		(end 82.799926 95.501948)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.466042 70.51101)
		(end 79.441873 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.306782 59.07813)
		(end 127.311634 59.103148)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.083495 68.440407)
		(end 203.111728 68.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.064563 57.965707)
		(end 124.098785 57.430492)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.15887 70.966482)
		(end 199.111028 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.991177 68.613121)
		(end 203.011047 68.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.999829 80.14456)
		(end 117.976992 80.133252)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.934581 26.019195)
		(end 157.982893 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.915132 77.997414)
		(end 199.913929 78.046444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.512049 70.51101)
		(end 185.485816 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.611162 70.287416)
		(end 185.595781 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.654178 26.999012)
		(end 188.655382 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.871686 78.668313)
		(end 153.837876 78.703825)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.916336 70.04644)
		(end 202.915132 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.899044 67.636028)
		(end 116.414323 67.487324)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.874333 68.897498)
		(end 142.880335 68.848833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.792266 68.289016)
		(end 93.826077 68.324529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.998579 67.940033)
		(end 137.533314 67.981088)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.764579 118.069884)
		(end 189.813551 118.07661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.422864 114.428777)
		(end 157.725785 113.986211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.450107 26.226762)
		(end 97.488763 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.82367 26.010812)
		(end 216.871982 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.555259 70.991611)
		(end 189.506595 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.724884 79.907608)
		(end 133.238343 80.133226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.898704 67.996258)
		(end 159.44122 67.982399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.082306 70.900507)
		(end 185.037479 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.511984 64.092936)
		(end 121.847894 63.674857)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.819218 76.568294)
		(end 199.839088 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.888971 70.977226)
		(end 97.841129 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.234358 28.837176)
		(end 189.190006 28.815348)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.92792 76.658869)
		(end 142.945567 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.179046 85.742851)
		(end 82.169219 85.766363)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.084866 27.930196)
		(end 97.084866 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.395388 78.668309)
		(end 185.361578 78.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.656739 78.900508)
		(end 97.612941 78.878462)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.161658 114.903124)
		(end 157.175274 114.854967)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.858104 120.627602)
		(end 93.826077 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.645065 78.854297)
		(end 153.602402 78.878465)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.656891 120.188739)
		(end 217.646147 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.26855 28.315435)
		(end 108.248365 28.360558)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.326625 76.800526)
		(end 108.335008 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.989369 28.404646)
		(end 142.966977 28.360576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.162137 118.677408)
		(end 97.182322 118.632285)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.940612 70.920377)
		(end 79.895785 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.16095 118.193893)
		(end 190.184586 118.203419)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.770741 118.54529)
		(end 199.795286 118.588197)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.326371 78.97723)
		(end 153.27806 78.985613)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.701566 76.072466)
		(end 97.747314 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.006096 118.709673)
		(end 146.531246 118.818496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.359118 70.828059)
		(end 203.319029 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.587019 26.25879)
		(end 199.622532 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.518041 118.072836)
		(end 189.567169 118.067363)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.637866 118.20149)
		(end 153.679844 118.227594)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.860601 118.962855)
		(end 101.88601 118.964806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.126103 26.11796)
		(end 185.168767 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.759744 86.266357)
		(end 127.75113 86.29034)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.945173 76.039438)
		(end 184.991731 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.899462 78.24016)
		(end 142.888718 78.192318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.531643 79.356815)
		(end 89.016364 79.505519)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.250282 120.796248)
		(end 185.210193 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.899948 118.817983)
		(end 142.913237 118.770371)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.665754 84.730467)
		(end 82.65358 84.752854)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.317995 67.98109)
		(end 183.343445 67.982391)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.153064 57.991119)
		(end 127.214571 58.523889)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.528852 76.164784)
		(end 97.570278 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.179103 55.747595)
		(end 127.131226 56.281762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.008822 70.379722)
		(end 93.988952 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.672927 78.592525)
		(end 139.64276 78.631181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.541715 78.97723)
		(end 107.493404 78.985613)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.654179 115.150835)
		(end 185.654179 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.523306 55.166045)
		(end 215.421198 54.639547)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.326026 28.874121)
		(end 189.279735 28.856783)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.558753 79.010445)
		(end 137.533303 79.011746)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.639925 86.824004)
		(end 123.632547 86.799612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.861331 82.480035)
		(end 175.504512 82.880417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.839088 68.613119)
		(end 199.856735 68.658867)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.384111 78.854292)
		(end 139.341448 78.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.610733 120.664731)
		(end 139.576922 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.711062 78.769664)
		(end 111.673933 78.737637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.34582 76.995434)
		(end 111.347024 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.544424 60.726492)
		(end 173.738537 61.226438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.673374 76.800526)
		(end 188.684118 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.917693 70.900507)
		(end 111.873895 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.149925 76.015617)
		(end 112.198237 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.203691 68.481831)
		(end 108.22786 68.524495)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.868318 26.949981)
		(end 139.869522 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.388838 120.283838)
		(end 111.37576 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.767898 70.828059)
		(end 79.727809 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.738521 85.766387)
		(end 173.544409 86.266333)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.468712 118.818496)
		(end 150.993862 118.709672)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.816213 78.991616)
		(end 203.767549 78.985614)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.322925 120.992844)
		(end 80.273894 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.33021 65.292681)
		(end 120.726003 64.930778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.527534 91.80164)
		(end 215.602624 91.270614)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.58702 120.734053)
		(end 199.549892 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.953994 55.166045)
		(end 123.851886 54.639547)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.792266 78.703821)
		(end 93.756754 78.737632)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.253175 83.773)
		(end 83.238781 83.794029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.084867 115.150835)
		(end 94.084867 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.168767 120.850714)
		(end 185.126104 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.624239 26.756262)
		(end 185.634982 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.789828 66.000708)
		(end 132.236227 66.297952)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.721939 76.007234)
		(end 143.770603 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.084866 26.999012)
		(end 94.084866 31.842064)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.09556 81.683435)
		(end 165.681804 81.342213)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.530755 118.080714)
		(end 107.579102 118.091015)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.139398 28.029988)
		(end 195.113989 28.028037)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.982291 78.737633)
		(end 188.946779 78.703823)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.206127 120.949827)
		(end 199.15887 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.884495 118.42459)
		(end 188.916998 118.387347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.925945 68.848838)
		(end 202.934328 68.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.88903 28.126667)
		(end 142.880511 28.077975)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.43328 87.341171)
		(end 127.427157 87.365908)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.917693 120.896929)
		(end 111.873896 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.441237 67.869124)
		(end 136.973178 67.937429)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.809324 76.138551)
		(end 79.851987 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.940612 76.072466)
		(end 79.98636 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.322925 75.996422)
		(end 93.085854 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.753097 78.991611)
		(end 184.704197 78.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.618007 28.641085)
		(end 199.581982 28.674934)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.384111 68.138545)
		(end 139.425537 68.164778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.148414 118.091015)
		(end 199.196192 118.103694)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.670604 67.996421)
		(end 204.683347 67.996259)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.328604 68.026355)
		(end 93.375861 68.039433)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.309515 64.531414)
		(end 84.686313 64.913054)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.68837 70.63118)
		(end 199.656342 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.869523 115.150835)
		(end 139.869523 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.850327 78.192317)
		(end 139.839583 78.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.057262 26.485411)
		(end 203.083494 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.70116 68.440401)
		(end 139.727393 68.481827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.471147 70.828059)
		(end 199.429721 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.425515 80.992135)
		(end 118.979116 80.694891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.315396 118.817965)
		(end 108.326313 118.866176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.268109 62.748613)
		(end 168.28141 62.726876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.014052 68.001231)
		(end 199.062716 68.007233)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.091425 87.914719)
		(end 173.002796 88.443652)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.780325 28.86544)
		(end 152.73448 28.84692)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.533957 76.481833)
		(end 217.558126 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.479008 114.585751)
		(end 185.506273 114.627717)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.941924 78.79983)
		(end 107.901835 78.828064)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.225893 67.869124)
		(end 182.757834 67.937429)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.353852 120.236581)
		(end 79.343108 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.652974 26.949981)
		(end 185.654178 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.631041 54.614612)
		(end 169.502183 54.094016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.319029 68.193017)
		(end 203.359118 68.164783)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.516581 62.748617)
		(end 174.808101 63.198775)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.190675 120.850714)
		(end 217.148012 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.677074 26)
		(end 216.726105 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.624138 68.039438)
		(end 203.671396 68.02636)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.530755 28.91211)
		(end 107.481958 28.920007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.575006 114.761054)
		(end 185.593371 114.807608)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.774106 79.123719)
		(end 114.242165 79.055414)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.863206 79.228165)
		(end 135.341006 79.350364)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.054432 78.379727)
		(end 154.034561 78.424553)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.206127 26.043016)
		(end 199.252685 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.176329 120.982031)
		(end 80.128017 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.363758 28.90181)
		(end 153.315411 28.91211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.602402 76.114382)
		(end 153.645065 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.149225 76.400318)
		(end 108.177458 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.970515 113.49091)
		(end 138.977026 113.501864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.869523 69.997409)
		(end 139.868319 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.849876 94.484424)
		(end 173.8603 94.507678)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.792266 76.289022)
		(end 93.826076 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.329395 78.996422)
		(end 92.316652 78.996584)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.807393 114.449473)
		(end 93.880357 114.545193)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.11326 70.966482)
		(end 139.065418 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.646147 26.756262)
		(end 217.656891 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.190007 118.177514)
		(end 189.234359 118.155686)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.343656 26.328112)
		(end 97.377467 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.505134 28.737083)
		(end 199.464499 28.765231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.506594 26.010812)
		(end 189.555259 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.141895 76.361663)
		(end 203.173923 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.316626 76.054819)
		(end 189.363184 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.412979 26.25879)
		(end 97.450107 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.935524 93.965803)
		(end 215.116803 93.461061)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.103605 118.908153)
		(end 104.128881 118.904907)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.160416 70.240159)
		(end 157.149672 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.860409 68.138549)
		(end 107.901835 68.164782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.750093 70.424549)
		(end 188.730223 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.158869 78.966487)
		(end 199.111027 78.97723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.512994 78.900507)
		(end 93.468167 78.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.46803 120.934446)
		(end 153.421471 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.934328 26.804104)
		(end 202.945071 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.761679 66.859606)
		(end 163.784516 66.848298)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.15887 120.962904)
		(end 199.111028 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.672927 70.592525)
		(end 139.64276 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.242139 79.055411)
		(end 114.216789 79.052812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.330927 57.404981)
		(end 81.331903 57.430446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.090303 114.585695)
		(end 203.119643 114.545137)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.199003 67.487317)
		(end 162.223299 67.479628)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.531832 70.920377)
		(end 203.487005 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.670708 28.028037)
		(end 147.645299 28.029988)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.849131 53.02704)
		(end 127.667852 53.531782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.04007 114.855023)
		(end 94.053686 114.90318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.919824 70.966482)
		(end 216.871982 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.06567 26.804104)
		(end 94.074053 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.036271 85.742845)
		(end 168.816883 85.253463)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.249906 76.568294)
		(end 108.269776 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.270877 26.076044)
		(end 189.316625 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.719625 76.223184)
		(end 93.756754 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.991731 26.058397)
		(end 185.037479 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.361578 76.289022)
		(end 185.395388 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.198237 78.985614)
		(end 112.149925 78.977231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.29765 120.896929)
		(end 139.252823 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.29765 76.092336)
		(end 139.341448 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.083495 120.548858)
		(end 203.057262 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.081296 64.092936)
		(end 213.417206 63.674857)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.302107 118.770352)
		(end 108.315396 118.817965)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.702349 120.896929)
		(end 157.658552 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.295333 64.93076)
		(end 212.313695 64.913089)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.322314 118.568352)
		(end 197.346798 118.561286)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.765235 76.223184)
		(end 153.802364 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.665168 118.914887)
		(end 188.673687 118.866194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.444494 53.556026)
		(end 173.289224 54.069366)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.582703 70.668309)
		(end 79.550675 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.895785 70.900507)
		(end 79.851987 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.62688 28.88913)
		(end 107.579102 28.90181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.777528 28.431557)
		(end 105.753043 28.424491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.149926 68.015617)
		(end 112.198237 68.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.715333 28.927272)
		(end 189.665936 28.929126)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.455575 86.266351)
		(end 123.261462 85.766405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.129273 68.946401)
		(end 154.130476 68.995432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.281463 68.400314)
		(end 97.311629 68.361658)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.801762 76.007234)
		(end 184.850074 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.511236 26.196595)
		(end 199.549891 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.457583 76.400318)
		(end 185.485816 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.485817 120.548858)
		(end 185.457583 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.98058 120.766081)
		(end 107.941924 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.558126 76.524496)
		(end 217.580172 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.128312 78.66831)
		(end 143.096285 78.631182)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.153614 92.378231)
		(end 173.282472 92.898827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.654179 76.995434)
		(end 188.655382 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.206522 120.376144)
		(end 157.188875 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.816901 61.739398)
		(end 169.036287 61.250016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.041849 26.709005)
		(end 94.054927 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.93772 57.991119)
		(end 172.999227 58.523889)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.357239 78.631186)
		(end 157.327072 78.592531)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.084867 119.993831)
		(end 94.083663 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.326027 118.11874)
		(end 189.373119 118.103713)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.059387 70.920377)
		(end 217.013639 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.177475 83.772997)
		(end 121.86335 83.338311)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.288937 78.769659)
		(end 185.250282 78.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.441735 78.424555)
		(end 111.421865 78.379728)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.88128 28.929126)
		(end 143.831851 28.928534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.3244 56.843185)
		(end 81.324075 56.868666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.352078 79.22817)
		(end 115.327125 79.222999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.701566 70.920377)
		(end 97.656739 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.315182 28.568272)
		(end 97.28456 28.529466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.397372 55.722254)
		(end 81.39445 55.747569)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.368408 57.991119)
		(end 81.429915 58.523889)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.839584 120.236581)
		(end 139.826506 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.759672 118.285865)
		(end 153.797327 118.31789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.985947 76.001232)
		(end 98.034848 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.466488 65.650646)
		(end 211.880244 65.309425)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.481958 28.920007)
		(end 107.43283 28.92548)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.511943 82.899905)
		(end 121.495479 82.880453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.686491 26.168362)
		(end 153.72658 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.68097 68.193012)
		(end 93.719625 68.223179)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.504281 70.769659)
		(end 139.465626 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.083663 120.042862)
		(end 94.080056 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.880511 28.077975)
		(end 142.874411 28.028921)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.113947 118.964806)
		(end 195.139356 118.962855)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.98502 114.715479)
		(end 94.005694 114.761054)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.864512 115.050889)
		(end 139.868269 115.100793)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.577579 78.938029)
		(end 203.531832 78.920383)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.733385 118.072836)
		(end 143.782513 118.067363)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.359118 76.164784)
		(end 203.400544 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.934581 70.977226)
		(end 157.886739 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.130476 27.930177)
		(end 154.129253 27.979606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.195267 118.069884)
		(end 98.244239 118.07661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.649167 31.94201)
		(end 185.642915 31.991663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.287423 68.658867)
		(end 108.302804 68.705426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.819504 70.995218)
		(end 143.770603 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.85321 118.20149)
		(end 107.895188 118.227594)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.895937 76.800526)
		(end 199.90432 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.933954 62.726859)
		(end 82.947255 62.748595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.441735 76.568294)
		(end 111.463781 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.733385 28.920025)
		(end 143.684588 28.912129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.30178 28.087939)
		(end 100.771759 28.169806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.243245 70.737631)
		(end 203.207733 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.280119 82.880434)
		(end 166.923298 82.480052)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.579102 28.90181)
		(end 107.530755 28.91211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.905828 82.461429)
		(end 166.52903 82.079789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.185859 113.49091)
		(end 93.19237 113.501864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.248877 60.702479)
		(end 169.417208 60.193273)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.981258 118.703861)
		(end 146.006071 118.709667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.479491 76.400318)
		(end 217.507724 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.377467 78.703823)
		(end 97.343656 78.66831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.556792 120.874883)
		(end 93.512994 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.915132 68.995432)
		(end 199.915132 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.642495 87.365933)
		(end 81.526974 87.889651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.046134 61.226456)
		(end 169.240246 60.72651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.6837 67.636028)
		(end 162.198979 67.487324)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.08607 26.949981)
		(end 97.089677 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.065417 26.019195)
		(end 139.113259 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.074054 76.848838)
		(end 94.080056 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.064176 28.737101)
		(end 189.024983 28.706978)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.486222 70.920377)
		(end 143.441395 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.197635 68.255207)
		(end 143.234764 68.22318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.225902 67.982398)
		(end 205.251352 67.981097)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.58702 68.25521)
		(end 199.622532 68.28902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.240231 86.266351)
		(end 169.046118 85.766405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.421865 76.613121)
		(end 111.441735 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.773948 68.092335)
		(end 107.817746 68.114381)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.572583 70.63118)
		(end 111.542416 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.210171 80.992135)
		(end 164.763772 80.694891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.033093 26.528074)
		(end 203.057262 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.470987 64.913072)
		(end 130.489348 64.930743)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.252686 120.934446)
		(end 199.206127 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.058075 78.799827)
		(end 189.01942 78.76966)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.764578 28.922977)
		(end 189.715333 28.927272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.347024 26.949981)
		(end 111.350631 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.312964 118.39114)
		(end 106.815347 118.203428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.554331 32.27742)
		(end 185.531401 32.321903)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.190675 26.142129)
		(end 217.232101 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.197636 120.734053)
		(end 143.162123 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.111281 68.800525)
		(end 154.119664 68.848836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.599455 76.138551)
		(end 93.640881 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.217936 87.341171)
		(end 173.211813 87.365908)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.914257 90.685602)
		(end 172.915883 90.711033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.664991 78.144007)
		(end 188.658989 78.095342)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.890943 90.149658)
		(end 169.891268 90.124177)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.948729 118.072836)
		(end 97.997857 118.067363)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.492275 70.552436)
		(end 79.466042 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.773608 68.568288)
		(end 139.793478 68.613115)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.747314 70.938024)
		(end 97.701566 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.96252 70.920377)
		(end 111.917693 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.747313 78.938025)
		(end 97.701566 78.920378)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.019419 26.226762)
		(end 189.058075 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.511236 120.796248)
		(end 199.471147 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.541715 26.019195)
		(end 107.589557 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.599455 120.850714)
		(end 93.556792 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.466042 120.507432)
		(end 79.441873 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.935126 114.951902)
		(end 202.946314 114.903124)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.083662 26.949981)
		(end 94.084866 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.653159 118.561286)
		(end 99.677644 118.568352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.334063 118.063717)
		(end 107.383492 118.064309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.624138 78.95341)
		(end 203.577579 78.938029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.085854 70.996422)
		(end 80.322925 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.160517 68.039433)
		(end 139.207076 68.054814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.756754 76.255212)
		(end 93.792266 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.858104 76.361663)
		(end 93.888271 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34101 70.095341)
		(end 108.335008 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.366929 120.283838)
		(end 79.353852 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.684588 118.080733)
		(end 143.733385 118.072836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.328604 70.966482)
		(end 93.280762 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.864712 70.095341)
		(end 139.85871 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.856735 70.333974)
		(end 199.839088 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.357239 26.365241)
		(end 157.389266 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.387058 70.878461)
		(end 199.34326 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.062279 89.001724)
		(end 124.000772 88.468954)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.363184 70.953405)
		(end 189.316626 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.329291 118.964806)
		(end 149.3547 118.962855)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.702349 26.095914)
		(end 157.747176 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.819504 67.997621)
		(end 143.868535 67.996417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.756754 78.737632)
		(end 93.719625 78.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.689095 65.309408)
		(end 177.102851 65.65063)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.410442 68.026356)
		(end 189.458284 68.015613)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.341046 28.16981)
		(end 192.315968 28.174342)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.703359 82.899907)
		(end 129.367449 83.317986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.88128 118.063735)
		(end 143.930678 118.065589)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.792266 120.700243)
		(end 93.756754 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.390617 32.13782)
		(end 111.377001 32.089663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.177458 70.552436)
		(end 108.149225 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.53197 76.054819)
		(end 143.578528 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.096281 87.889676)
		(end 173.091429 87.914693)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.421471 76.039438)
		(end 153.468029 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.749717 70.799826)
		(end 111.711062 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.2812 66.585636)
		(end 164.742194 66.311573)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.658989 76.897502)
		(end 188.664991 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.111028 70.977226)
		(end 199.062716 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.158869 26.029939)
		(end 199.206127 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.350632 120.091763)
		(end 111.347025 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.11656 57.430471)
		(end 127.150784 57.965687)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.533957 70.51101)
		(end 217.507724 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.493404 78.985613)
		(end 107.444739 78.991615)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.548458 66.297968)
		(end 210.994856 66.000724)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.592075 32.54339)
		(end 139.577149 32.564045)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.292062 64.51281)
		(end 84.309497 64.531395)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.273419 120.796248)
		(end 143.234764 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.717521 54.093991)
		(end 123.710768 54.069418)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.772139 68.524492)
		(end 188.796308 68.481829)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.85871 70.144005)
		(end 139.850327 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.101345 67.996253)
		(end 138.114089 67.996415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.111738 28.08469)
		(end 147.086462 28.087936)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.253229 76.440407)
		(end 97.281462 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.739664 113.964778)
		(end 158.022925 113.501874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.450108 120.766081)
		(end 97.41298 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.899462 120.236581)
		(end 142.888719 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.059387 26.076044)
		(end 217.104214 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.888271 68.400312)
		(end 93.916504 68.440401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.701566 120.916799)
		(end 97.656739 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.967081 70.953405)
		(end 216.919824 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.919944 120.091763)
		(end 202.916337 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.226051 76.092336)
		(end 189.270878 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.357239 76.361663)
		(end 157.389267 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.672927 76.400318)
		(end 139.70116 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.872116 70.287416)
		(end 199.856735 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.114805 26.756262)
		(end 97.127883 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.269776 76.613121)
		(end 108.287423 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.449324 120.627602)
		(end 217.417296 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.180781 78.42455)
		(end 97.160911 78.379724)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.422419 70.938024)
		(end 93.375861 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.072079 68.658867)
		(end 154.08746 68.705426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.727809 26.196595)
		(end 79.767898 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.033093 78.468352)
		(end 203.011047 78.424555)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.410441 78.966484)
		(end 189.363184 78.953406)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.561389 67.479615)
		(end 180.585685 67.487304)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.463781 70.468347)
		(end 111.441735 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.919824 76.026361)
		(end 216.967081 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.357487 87.365927)
		(end 215.351364 87.34119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.249905 78.424553)
		(end 108.22786 78.468351)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.612941 26.11796)
		(end 97.656739 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.01498 114.715423)
		(end 203.03791 114.67094)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.951304 118.351758)
		(end 188.987329 118.317909)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.141895 26.365241)
		(end 203.173922 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.343657 76.324534)
		(end 97.377467 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.084119 90.711056)
		(end 124.085745 90.685624)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.008268 120.934446)
		(end 111.96252 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.68336 67.996258)
		(end 205.225876 67.982399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.631059 92.378232)
		(end 169.636548 92.353347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.031557 78.991616)
		(end 157.982893 78.985614)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.334725 26.852416)
		(end 79.343108 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.160517 76.039438)
		(end 139.207075 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.281462 70.592525)
		(end 97.253229 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.343478 67.86913)
		(end 206.368662 67.86524)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.141289 26.852416)
		(end 157.149672 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.037885 120.548858)
		(end 143.011652 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.777511 118.561278)
		(end 106.288824 118.399463)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.622532 120.700243)
		(end 199.58702 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.871418 28.222472)
		(end 199.855791 28.269369)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.362133 28.791353)
		(end 143.320155 28.765249)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.335008 68.848836)
		(end 108.34101 68.897501)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.146126 28.529448)
		(end 108.115504 28.568253)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.257784 80.681283)
		(end 132.236219 80.694861)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.343657 120.664731)
		(end 97.31163 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.994306 114.760998)
		(end 203.01498 114.715423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.93392 84.265989)
		(end 82.665766 84.730444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.250282 78.799826)
		(end 185.210193 78.82806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.487005 78.900512)
		(end 203.443207 78.878466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.388837 68.705427)
		(end 111.404218 68.658868)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.520508 26.403896)
		(end 79.550675 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.819218 68.568293)
		(end 199.839088 68.613119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.433297 59.651677)
		(end 127.57541 60.168814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.697195 70.287416)
		(end 188.684118 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.05273 84.244226)
		(end 213.76121 83.794068)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.298839 76.440407)
		(end 157.327072 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.084866 31.842064)
		(end 94.083612 31.892106)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.715334 118.065589)
		(end 189.764579 118.069884)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.37586 26.043016)
		(end 93.422419 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.188874 70.333974)
		(end 157.173493 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.367439 86.799594)
		(end 173.360061 86.823986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.065418 120.973648)
		(end 139.017106 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.22144 118.709673)
		(end 100.74659 118.818496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.01942 76.223184)
		(end 189.058075 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.640881 68.164778)
		(end 93.68097 68.193012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.841129 26.029939)
		(end 97.888971 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.400544 78.854298)
		(end 203.359118 78.828065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.085854 120.992844)
		(end 80.322925 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.008268 70.938024)
		(end 111.96252 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.052765 62.748613)
		(end 214.066066 62.726876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.934328 78.192322)
		(end 202.925945 78.144011)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.232101 70.828059)
		(end 217.190675 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.916505 120.548858)
		(end 93.888271 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.253228 26.443985)
		(end 97.281462 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.053206 28.315435)
		(end 154.033021 28.360558)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.946779 78.703823)
		(end 188.912968 78.66831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.711062 68.223184)
		(end 111.749717 68.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.75786 67.937432)
		(end 182.78321 67.940031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.008267 78.938029)
		(end 111.96252 78.920383)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.421192 54.639522)
		(end 215.415703 54.614637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.221456 28.283176)
		(end 100.196643 28.288983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.746631 28.174347)
		(end 100.221481 28.283171)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.134885 120.99164)
		(end 93.085854 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.080056 68.897497)
		(end 94.083663 68.946397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.612941 78.878462)
		(end 97.570278 78.854294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.689154 120.766081)
		(end 79.652025 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.868319 78.04644)
		(end 139.864712 78.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.298434 120.916799)
		(end 199.252686 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.770604 120.988033)
		(end 143.721939 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.531832 26.076044)
		(end 203.577579 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.863334 83.338291)
		(end 121.847886 83.318024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.369211 51.490855)
		(end 174.362978 51.501976)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.849213 89.027131)
		(end 169.846938 89.001749)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.654179 68.995428)
		(end 185.654179 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.206325 118.992193)
		(end 148.2318 118.992843)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.567314 83.338294)
		(end 83.253189 83.772979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.65319 26)
		(end 198.91612 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.111728 78.592531)
		(end 203.083495 78.552442)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.718537 76.400318)
		(end 199.74677 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.511236 68.193016)
		(end 199.549891 68.223183)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.593371 114.807608)
		(end 185.609382 114.855023)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.940283 67.085231)
		(end 87.963668 67.095358)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.222471 118.561286)
		(end 191.246956 118.568352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.429913 118.962855)
		(end 193.455322 118.964806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.011047 76.568294)
		(end 203.033093 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.730223 76.613121)
		(end 188.750093 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.70116 26.443985)
		(end 139.727393 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.38231 26.662447)
		(end 79.399957 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.57758 70.938024)
		(end 203.531832 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.566702 87.341166)
		(end 169.424589 86.824029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.234764 120.766081)
		(end 143.197636 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.946779 68.289018)
		(end 188.982291 68.255207)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.367459 60.193255)
		(end 173.535792 60.702461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.625785 26.029939)
		(end 143.673627 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.127884 120.283838)
		(end 97.114806 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.343657 68.32453)
		(end 97.377467 68.289018)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.826077 120.664731)
		(end 93.792266 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.654179 68.995429)
		(end 188.655382 68.946399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.718536 26.403896)
		(end 199.74677 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.767898 76.164784)
		(end 79.809324 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.755761 118.076592)
		(end 198.804733 118.069866)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.884708 118.817965)
		(end 199.895625 118.866176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.084867 69.997409)
		(end 94.083663 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.014051 26.00481)
		(end 199.062716 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.805875 61.762401)
		(end 168.81689 61.739421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.623268 114.449453)
		(end 111.638194 114.428798)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.673687 118.866194)
		(end 188.684604 118.817983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.615888 68.138551)
		(end 157.658551 68.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.324075 56.868691)
		(end 81.330926 57.404956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.127883 76.705427)
		(end 97.143264 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.60416 70.995218)
		(end 189.555259 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.422522 28.791334)
		(end 199.379304 28.815329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.97353 70.333974)
		(end 202.958149 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.085854 26)
		(end 93.134885 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.344617 76.946403)
		(end 108.34582 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.982291 76.255212)
		(end 189.01942 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.576922 26.2926)
		(end 139.610732 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.12858 28.222491)
		(end 97.115291 28.174878)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.054826 68.039438)
		(end 112.102084 68.02636)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178.020853 80.694875)
		(end 177.574455 80.992119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.149672 26.804104)
		(end 157.160415 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.077474 118.08575)
		(end 144.125542 118.097282)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.435018 118.127403)
		(end 98.480863 118.145923)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.197635 76.255212)
		(end 143.234764 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.126104 68.114377)
		(end 185.168767 68.138545)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.640881 26.168362)
		(end 93.68097 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.570278 70.854292)
		(end 97.528852 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.450108 76.223184)
		(end 97.488763 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.210193 68.164778)
		(end 185.250282 68.193012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.316625 26.058397)
		(end 189.363184 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.599455 68.138545)
		(end 93.640881 68.164778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.400544 26.142129)
		(end 203.443207 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.849529 32.040941)
		(end 139.838341 32.089719)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.871982 120.973648)
		(end 216.82367 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.676087 76.995434)
		(end 217.676087 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.311629 26.365241)
		(end 97.343656 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.244239 118.07661)
		(end 98.292818 118.08575)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.553569 81.00681)
		(end 177.122931 81.326459)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.624239 68.752679)
		(end 185.634983 68.800521)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.414347 67.487317)
		(end 116.438643 67.479628)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.343108 76.800526)
		(end 79.353852 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.802364 76.255212)
		(end 153.837876 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.033093 68.524496)
		(end 203.057262 68.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.97878 85.230442)
		(end 173.967765 85.253422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.654179 69.997409)
		(end 188.654179 68.995429)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.183785 26.00481)
		(end 93.23245 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.054927 26.756262)
		(end 94.06567 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.837876 76.289022)
		(end 153.871686 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.100537 68.752683)
		(end 154.111281 68.800525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.388837 76.705427)
		(end 111.404218 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.432646 83.338291)
		(end 213.417198 83.318024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.328603 78.966483)
		(end 93.280761 78.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.935823 118.255742)
		(end 107.975016 118.285865)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.653191 67.996417)
		(end 198.916121 67.99642)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.354934 120.850714)
		(end 143.313508 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.765236 120.766081)
		(end 153.72658 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.72658 68.193016)
		(end 153.765235 68.223183)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.494865 118.25576)
		(end 97.5355 118.227612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.941924 26.196595)
		(end 107.980579 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.780325 118.127385)
		(end 152.827019 118.111159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.988952 76.568294)
		(end 94.008822 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.588463 118.103713)
		(end 143.636241 118.091033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.080056 120.091763)
		(end 94.074054 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.128017 70.977226)
		(end 80.080175 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.749717 76.193017)
		(end 111.789806 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.86213 28.907111)
		(end 189.81355 28.916251)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.783235 67.940033)
		(end 183.31797 67.981088)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.655166 70.996422)
		(end 171.393043 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.179072 61.249998)
		(end 82.39846 61.73938)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.449324 76.361663)
		(end 217.479491 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34582 76.995434)
		(end 108.34582 77.997414)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.96209 114.670996)
		(end 93.98502 114.715479)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.837863 118.67739)
		(end 199.855791 118.723456)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.455671 28.706978)
		(end 97.418016 28.674953)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.421865 78.379728)
		(end 111.404218 78.33398)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.209237 86.824004)
		(end 215.201859 86.799612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.831232 78.854298)
		(end 111.789806 78.828065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.718799 80.407207)
		(end 132.257805 80.68127)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.131464 75.996422)
		(end 153.180495 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.082306 68.092331)
		(end 185.126104 68.114377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.008268 68.054819)
		(end 112.054826 68.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.251707 67.095372)
		(end 163.275092 67.085245)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.226051 68.092332)
		(end 189.270878 68.072462)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.458283 76.015617)
		(end 189.506595 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.902379 28.601703)
		(end 144.399996 28.789415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.856735 76.658869)
		(end 199.872116 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.531287 28.174347)
		(end 146.006137 28.283171)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.315882 120.236581)
		(end 108.302804 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.727809 70.799826)
		(end 79.689154 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.795286 118.588197)
		(end 199.817678 118.632267)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.483453 62.748613)
		(end 122.496754 62.726876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.793872 26.043016)
		(end 97.841129 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.578134 78.379722)
		(end 185.558264 78.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.531969 78.938025)
		(end 143.486222 78.920378)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.572583 26.365241)
		(end 111.60461 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.536218 120.464769)
		(end 185.512049 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.022932 113.501863)
		(end 158.029444 113.490911)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.720264 118.13606)
		(end 107.765641 118.155667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.083878 26)
		(end 107.346808 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.566508 88.443672)
		(end 215.477877 87.914738)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.719237 70.977226)
		(end 203.671395 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.07855 79.228165)
		(end 89.55635 79.350364)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.35698 93.989582)
		(end 123.366203 93.965827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.245798 67.295858)
		(end 134.26967 67.304778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.604611 120.664731)
		(end 111.572584 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.492275 120.548858)
		(end 79.466042 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.885194 120.236581)
		(end 199.872116 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.350631 70.095341)
		(end 111.347024 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.839088 70.379722)
		(end 199.819218 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.826076 78.668309)
		(end 93.792266 78.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.433491 58.549171)
		(end 81.522122 59.078105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.144208 28.269387)
		(end 97.12858 28.222491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.298433 70.920377)
		(end 199.252685 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.350631 76.897502)
		(end 111.356633 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.790752 118.709673)
		(end 192.315902 118.818496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.365814 114.951902)
		(end 111.377002 114.903124)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.346568 56.281787)
		(end 81.344942 56.307219)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.183127 61.739404)
		(end 128.194142 61.762383)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.125666 70.095341)
		(end 154.119664 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 223.663839 126.992843)
		(end 223.674841 126.992573)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.899461 26.756262)
		(end 142.912539 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.073604 115.001236)
		(end 94.079856 115.050889)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.322331 28.424484)
		(end 196.803422 28.288989)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.869523 68.995429)
		(end 142.870726 68.946399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.849159 93.965796)
		(end 127.858383 93.989551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.907863 52.0015)
		(end 122.896265 51.978809)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.3464 84.752872)
		(end 214.334226 84.730484)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.888271 78.592525)
		(end 93.858104 78.631181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.100955 79.356815)
		(end 180.585676 79.505519)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.522824 94.991343)
		(end 82.534422 95.014034)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.671396 120.962904)
		(end 203.624139 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.999231 58.523914)
		(end 173.002799 58.549146)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.226995 26.485411)
		(end 97.253228 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.997857 28.925498)
		(end 97.948729 28.920025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.520991 114.585695)
		(end 111.550331 114.545137)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.982291 68.255207)
		(end 189.01942 68.22318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.226996 70.51101)
		(end 97.202827 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.363758 118.091015)
		(end 153.411536 118.103694)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.918703 82.899907)
		(end 83.582793 83.317986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.992077 67.479615)
		(end 89.016373 67.487304)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.720263 28.856764)
		(end 107.673972 28.874103)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.062716 76.007234)
		(end 199.111028 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.677074 120.992844)
		(end 203.914145 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.363463 92.353321)
		(end 127.368952 92.378206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.166648 28.641104)
		(end 143.132342 28.605514)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.753019 28.424484)
		(end 105.23411 28.288989)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.058075 70.799826)
		(end 189.01942 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.487005 68.092336)
		(end 203.531832 68.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.234069 118.703854)
		(end 105.752977 118.568358)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.009018 28.00065)
		(end 102.983543 28)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.649368 78.095341)
		(end 185.643366 78.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.653176 28.431565)
		(end 99.141863 28.59338)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.087031 120.664731)
		(end 108.05322 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.084867 119.993831)
		(end 97.084867 119.062666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.611162 76.705427)
		(end 185.624239 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.116557 89.562376)
		(end 127.115581 89.587841)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.102083 26.029939)
		(end 112.149925 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.725799 113.98619)
		(end 157.739651 113.9648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.53197 68.054815)
		(end 143.578528 68.039434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.534373 120.796248)
		(end 157.495718 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.574462 120.824481)
		(end 157.534373 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.648624 87.341171)
		(end 81.642501 87.365908)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.839482 76.039438)
		(end 157.886739 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.945567 76.613121)
		(end 142.965437 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.655382 68.946399)
		(end 188.658989 68.897498)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.792479 32.564066)
		(end 93.489558 33.006632)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.153596 54.614611)
		(end 173.148107 54.639496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.820888 55.747593)
		(end 169.817965 55.722278)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.710782 92.923452)
		(end 123.717534 92.89888)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.744401 64.913071)
		(end 121.121198 64.531431)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.48795 76.481833)
		(end 111.514183 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.851987 26.11796)
		(end 79.895785 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.083663 68.946397)
		(end 94.084867 68.995428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.125637 79.35037)
		(end 181.10098 79.356808)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.74677 70.552436)
		(end 199.718537 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.936961 114.627717)
		(end 93.96209 114.670996)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.100538 120.236581)
		(end 154.08746 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.395388 70.668309)
		(end 185.361578 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.350631 78.095346)
		(end 111.347024 78.046446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.652313 28.605496)
		(end 199.618007 28.641085)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.916336 26.949981)
		(end 202.919943 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.55283 27.999999)
		(end 194.016523 27.999999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.08746 78.28742)
		(end 154.072079 78.333979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.326372 68.015616)
		(end 153.374214 68.026359)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.228265 118.823033)
		(end 196.253343 118.818501)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.749717 120.796248)
		(end 111.711062 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.089755 28.028921)
		(end 97.086089 27.979625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.544327 28.706959)
		(end 199.505134 28.737083)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.096624 118.063735)
		(end 98.146022 118.065589)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.160911 76.613121)
		(end 97.180781 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.574462 76.164784)
		(end 157.615888 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.751145 60.702485)
		(end 127.759759 60.726468)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.616508 118.064327)
		(end 189.665936 118.063735)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.987484 120.464769)
		(end 142.965438 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.982893 70.985609)
		(end 157.934581 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.200683 67.86523)
		(end 182.225868 67.86912)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.531832 68.072466)
		(end 203.57758 68.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.44474 68.001231)
		(end 107.493404 68.007233)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.344833 120.992844)
		(end 112.295802 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.824726 114.855023)
		(end 139.838342 114.90318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.274023 64.930761)
		(end 176.669817 65.292664)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.149224 26.403896)
		(end 108.177458 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.466996 79.897476)
		(end 116.969568 79.696994)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.617689 26.662447)
		(end 217.63307 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.673627 26.019195)
		(end 143.721938 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.204713 28.404646)
		(end 97.182321 28.360576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.781863 58.549166)
		(end 169.785431 58.523933)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.976969 80.133241)
		(end 117.490427 79.907622)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.404218 78.33398)
		(end 111.388837 78.287422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.037479 26.076044)
		(end 185.082306 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.01634 79.505526)
		(end 88.992044 79.513215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.468029 26.058397)
		(end 153.513777 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.64276 78.631181)
		(end 139.610732 78.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.74677 68.440405)
		(end 199.773003 68.481831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.888718 76.800526)
		(end 142.899462 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.904143 28.077956)
		(end 199.895624 28.126649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.656521 79.123713)
		(end 90.631337 79.127603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.090303 32.407092)
		(end 203.063038 32.365126)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.457583 68.400312)
		(end 185.485816 68.440401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.197635 70.737631)
		(end 143.162123 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.160517 120.949827)
		(end 139.11326 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.008268 76.054819)
		(end 112.054826 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.750093 76.568294)
		(end 188.772139 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.471147 78.828064)
		(end 199.429721 78.854297)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.925946 120.140427)
		(end 202.919944 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.209649 32.231789)
		(end 157.191284 32.185235)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.729122 120.916799)
		(end 107.683374 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.38231 76.658869)
		(end 79.399957 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.202672 28.674953)
		(end 143.166648 28.641104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.826076 26.328112)
		(end 93.858103 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.919541 67.997619)
		(end 138.968442 68.001227)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.425537 76.164784)
		(end 139.465626 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.704197 70.995218)
		(end 184.655166 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.054927 70.240159)
		(end 94.04185 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.88674 120.962904)
		(end 157.839483 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.315881 76.752684)
		(end 108.326625 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.851897 92.353322)
		(end 123.954003 91.826823)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.223266 79.513228)
		(end 162.19897 79.505539)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.982893 120.982031)
		(end 157.934582 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.914145 67.996421)
		(end 204.670591 67.996421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.888971 76.015617)
		(end 97.937283 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.698235 28.087936)
		(end 195.672959 28.08469)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.945567 68.613116)
		(end 142.965438 68.56829)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.280094 92.923452)
		(end 215.286846 92.89888)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.870402 90.685599)
		(end 169.890942 90.149684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.132342 28.605514)
		(end 143.099838 28.568272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.29765 70.900507)
		(end 139.252823 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.115583 57.404981)
		(end 127.116559 57.430446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.793477 26.616699)
		(end 139.811124 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.458628 28.874103)
		(end 153.411536 28.88913)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.250282 26.196595)
		(end 185.288937 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.273894 120.99164)
		(end 80.224993 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.082306 120.896929)
		(end 185.037479 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.083663 70.04644)
		(end 94.080056 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.244238 28.916251)
		(end 98.195266 28.922977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.919541 26.001203)
		(end 138.968441 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.655382 70.04644)
		(end 188.654179 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.365017 120.188739)
		(end 111.356634 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.792924 76.054819)
		(end 157.839482 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.106285 56.843181)
		(end 124.085743 56.307267)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.537658 118.568352)
		(end 151.562142 118.561286)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.912969 120.664731)
		(end 188.880942 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.985947 78.991612)
		(end 97.937283 78.98561)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.350832 115.050833)
		(end 111.357084 115.00118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.083001 28.605496)
		(end 108.048695 28.641085)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.34582 31.842008)
		(end 111.34582 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.080458 67.997625)
		(end 158.129489 67.996421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.702349 76.092336)
		(end 157.747176 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.790742 86.82401)
		(end 81.64863 87.341147)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.873895 76.114382)
		(end 111.917693 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.761196 83.794047)
		(end 213.746802 83.773018)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.128313 68.32453)
		(end 143.162123 68.289018)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.888972 120.973648)
		(end 97.84113 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.437832 28.431565)
		(end 144.926519 28.59338)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.40535 28.815348)
		(end 143.362133 28.791353)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.310845 70.769659)
		(end 217.27219 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.08746 120.283838)
		(end 154.072079 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.42242 120.934446)
		(end 93.375861 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.616513 76.289022)
		(end 79.652025 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.578134 76.613121)
		(end 185.595781 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.897915 26.029939)
		(end 184.945172 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.837876 68.28902)
		(end 153.871687 68.324533)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.005693 32.231845)
		(end 93.985019 32.27742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.311629 70.63118)
		(end 97.281462 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.427416 68.361657)
		(end 185.457583 68.400312)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.346573 90.711059)
		(end 81.394453 91.245225)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.64799 83.338291)
		(end 167.632542 83.318024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.326625 70.192317)
		(end 108.315881 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.410441 70.966482)
		(end 189.363184 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.324402 90.149662)
		(end 81.344944 90.685576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.677074 70.996422)
		(end 203.914145 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.121172 82.461429)
		(end 120.744374 82.079789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.129489 120.992844)
		(end 158.080458 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.567353 63.654552)
		(end 83.582801 63.674819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.748347 67.095367)
		(end 134.245775 67.295849)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.290999 94.507701)
		(end 82.522812 94.991321)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.919541 70.995218)
		(end 138.87051 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.625785 70.966482)
		(end 143.578528 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.047196 118.064327)
		(end 98.096624 118.063735)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.173923 120.664731)
		(end 203.141896 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.870726 78.046442)
		(end 142.869523 77.997411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.815371 118.203419)
		(end 106.839007 118.193893)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.582783 86.799594)
		(end 127.575405 86.823986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.709 52.485142)
		(end 214.477187 52.001522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.31163 120.627602)
		(end 97.281463 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.251652 79.897476)
		(end 162.754224 79.696994)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.531832 78.920383)
		(end 203.487005 78.900512)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.885898 78.996427)
		(end 158.129488 78.996427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.315395 28.17486)
		(end 108.302106 28.222472)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.976576 63.198793)
		(end 168.268095 62.748635)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.334725 76.848838)
		(end 79.343108 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.096285 78.631182)
		(end 143.066118 78.592526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.13959 68.138546)
		(end 189.182253 68.114378)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.885193 78.240163)
		(end 199.872116 78.28742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.253229 70.552436)
		(end 97.226996 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.085854 78.996422)
		(end 92.329408 78.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.966906 68.524491)
		(end 93.988952 68.568288)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.485816 68.440401)
		(end 185.512049 68.481827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.980579 26.226762)
		(end 108.017707 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.625785 78.966484)
		(end 143.578528 78.953406)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.053685 32.089719)
		(end 94.040069 32.137876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.600042 76.613121)
		(end 217.617689 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.33213 53.531812)
		(end 169.150849 53.027071)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.319029 120.796248)
		(end 203.280374 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.987483 70.468347)
		(end 142.965437 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.97353 78.33398)
		(end 202.958149 78.287422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.895625 118.866176)
		(end 199.904144 118.914868)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.537675 28.424484)
		(end 151.018766 28.288989)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.174791 28.489176)
		(end 108.146126 28.529448)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.350831 31.941954)
		(end 111.347074 31.89205)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.273894 26.001203)
		(end 80.322925 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34101 78.095345)
		(end 108.335008 78.14401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.082306 78.900507)
		(end 185.037479 78.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.729121 26.076044)
		(end 107.773948 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.474239 80.394739)
		(end 117.999852 80.144571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.888971 78.977227)
		(end 97.841129 78.966484)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.990981 118.992193)
		(end 194.016456 118.992843)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.904392 81.683435)
		(end 130.885152 81.700145)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.246901 78.991616)
		(end 112.198237 78.985614)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.71352 118.723474)
		(end 188.731449 118.677408)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.206521 68.613121)
		(end 157.226391 68.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.730305 79.688057)
		(end 162.22329 79.513236)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.638235 32.564045)
		(end 111.623309 32.54339)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.097637 28.601694)
		(end 152.073546 28.593387)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.230323 32.277364)
		(end 157.209649 32.231789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.926495 28.593388)
		(end 144.902403 28.601694)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.536218 76.524496)
		(end 185.558264 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.115505 118.424571)
		(end 108.146127 118.463377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.71861 62.726859)
		(end 128.731911 62.748595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.721617 32.365182)
		(end 139.694352 32.407148)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.129273 78.046444)
		(end 154.125666 78.095345)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.531401 32.321903)
		(end 185.506273 32.365182)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.671276 120.091763)
		(end 217.665274 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.160416 76.752684)
		(end 157.173493 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.104063 120.188739)
		(end 97.09568 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.656739 70.900507)
		(end 97.612941 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.991177 78.379728)
		(end 202.97353 78.33398)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.837862 28.315435)
		(end 199.817677 28.360558)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.080175 120.962904)
		(end 80.032918 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.250282 70.799826)
		(end 185.210193 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.280761 26.019195)
		(end 93.328603 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.912539 76.705427)
		(end 142.92792 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.399957 70.379722)
		(end 79.38231 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.959929 32.13782)
		(end 202.946313 32.089663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.796308 78.511012)
		(end 188.772139 78.468348)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.981274 28.288989)
		(end 145.462366 28.424485)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.286479 28.269369)
		(end 108.26855 28.315435)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.93388 78.592529)
		(end 153.903714 78.631185)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.753098 120.988033)
		(end 184.704197 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.319029 70.799826)
		(end 203.280374 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.991178 120.376144)
		(end 202.973531 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.871982 70.977226)
		(end 216.82367 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.325116 26.949981)
		(end 79.328723 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.059387 76.072466)
		(end 217.104214 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.465565 51.978786)
		(end 214.20631 51.502023)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.280531 52.508409)
		(end 82.073717 53.003237)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.493404 68.007233)
		(end 107.541716 68.015616)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.675923 56.868687)
		(end 215.675598 56.843206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.869523 119.993831)
		(end 142.869523 119.062666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.344617 26.949981)
		(end 108.34582 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.210193 70.828059)
		(end 185.168767 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.934328 70.192317)
		(end 202.925945 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.495504 64.112407)
		(end 121.511967 64.092956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.08642 118.904907)
		(end 147.111696 118.908153)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.915132 26.999012)
		(end 199.915132 27.930177)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.755205 33.501943)
		(end 174.369217 51.490844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.880941 26.365241)
		(end 188.912968 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.111728 70.592525)
		(end 203.083495 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.574462 26.168362)
		(end 157.615888 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.574462 78.828065)
		(end 157.534373 78.799831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.595781 68.658863)
		(end 185.611162 68.705421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.552814 118.992843)
		(end 194.578289 118.992193)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.962114 70.552436)
		(end 153.933881 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.422419 78.938024)
		(end 93.375861 78.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.727393 68.481827)
		(end 139.751562 68.524491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.099763 57.404977)
		(end 124.106611 56.868713)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.712576 68.658864)
		(end 188.730223 68.613116)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34101 68.897501)
		(end 108.344617 68.946401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.599455 70.854292)
		(end 93.556792 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.146127 118.463377)
		(end 108.174791 118.503649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.634983 120.188739)
		(end 185.62424 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.341448 70.878461)
		(end 139.29765 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.690484 82.461429)
		(end 212.313686 82.079789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.55526 120.988033)
		(end 189.506595 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.793478 68.613115)
		(end 139.811125 68.658863)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.23245 68.007229)
		(end 93.280762 68.015612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.948729 28.920025)
		(end 97.899932 28.912129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.682004 79.011753)
		(end 113.656554 79.010452)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.129253 27.979606)
		(end 154.125587 28.028902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.031557 70.991611)
		(end 157.982893 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.128017 26.019195)
		(end 80.176329 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.673934 120.734053)
		(end 111.638421 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.11326 68.026355)
		(end 139.160517 68.039433)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.141839 28.593388)
		(end 99.117747 28.601694)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.673933 26.25879)
		(end 111.711062 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.870726 70.04644)
		(end 142.869523 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.774025 28.404646)
		(end 188.751633 28.360576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.135487 31.941954)
		(end 157.13173 31.89205)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.106287 90.149658)
		(end 124.106612 90.124177)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.01942 78.76966)
		(end 188.982291 78.737633)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.217953 59.651677)
		(end 173.360066 60.168814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.871076 118.904907)
		(end 192.896352 118.908153)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.536218 68.524491)
		(end 185.558264 68.568288)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.72658 78.79983)
		(end 153.686491 78.828064)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.715439 118.463377)
		(end 199.744103 118.503649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.089801 28.895561)
		(end 107.042362 28.881665)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.46803 68.054818)
		(end 153.513777 68.072465)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.774026 118.588216)
		(end 188.798571 118.545308)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.34582 68.995434)
		(end 111.347024 68.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.141895 68.361662)
		(end 203.173923 68.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.609382 114.855023)
		(end 185.622998 114.90318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.942737 76.481833)
		(end 93.966906 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.420897 118.091033)
		(end 189.469244 118.080733)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.298839 68.440407)
		(end 157.327072 68.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.754201 79.696985)
		(end 162.730329 79.688065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.774166 67.86913)
		(end 114.79935 67.86524)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.37576 76.752684)
		(end 111.388837 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.125587 28.028902)
		(end 154.119487 28.077956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.582803 60.193255)
		(end 127.751136 60.702461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.773003 78.511014)
		(end 199.74677 78.55244)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.793872 120.949827)
		(end 97.747314 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.916336 78.046446)
		(end 202.915132 77.997415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.965437 70.424549)
		(end 142.945567 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.261452 85.766381)
		(end 123.251625 85.742869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.229396 68.001231)
		(end 153.27806 68.007233)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.871982 26.019195)
		(end 216.919824 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.684056 118.818496)
		(end 105.209206 118.709672)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.08609 119.013237)
		(end 97.089756 118.963941)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.406628 32.185235)
		(end 111.390617 32.13782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.037885 68.440403)
		(end 143.066119 68.400314)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.111027 78.97723)
		(end 199.062716 78.985613)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.363184 120.949827)
		(end 189.316626 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.298433 78.920381)
		(end 199.252685 78.938028)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.968441 78.991611)
		(end 138.919541 78.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.895187 28.765231)
		(end 107.85321 28.791334)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.775006 120.988033)
		(end 216.726105 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.91588 56.281787)
		(end 172.914254 56.307219)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.839088 26.616699)
		(end 199.856735 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.169235 61.226462)
		(end 82.179062 61.249974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.98636 76.054819)
		(end 80.032918 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.347025 120.042862)
		(end 111.345821 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.059387 120.916799)
		(end 217.013639 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.868319 120.042862)
		(end 139.864712 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.218136 88.443677)
		(end 127.214568 88.46891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.379305 118.177495)
		(end 199.422522 118.20149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.822487 83.773)
		(end 174.808093 83.794029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.183786 76.001232)
		(end 93.23245 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.026856 67.937437)
		(end 160.558796 67.869133)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.002792 88.443677)
		(end 172.999224 88.46891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.934328 76.800526)
		(end 202.945072 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.176329 70.985609)
		(end 80.128017 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.066118 26.403896)
		(end 143.096285 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.576922 120.700243)
		(end 139.54141 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.999221 88.468935)
		(end 172.937716 89.001704)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.219674 118.127403)
		(end 144.265519 118.145923)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.913236 28.222491)
		(end 142.899947 28.174878)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.570069 118.962853)
		(end 104.10358 118.908156)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.450108 78.76966)
		(end 97.412979 78.737633)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.510677 64.93076)
		(end 166.529039 64.913089)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 223.675816 126.991598)
		(end 223.676086 126.980596)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.089801 118.097264)
		(end 107.137869 118.085732)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.966693 91.270591)
		(end 173.041785 91.801615)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.352009 63.654552)
		(end 129.367457 63.674819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.243245 76.255212)
		(end 203.280374 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.496491 80.40721)
		(end 118.474261 80.394751)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.384111 26.142129)
		(end 139.425537 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.96252 78.920383)
		(end 111.917693 78.900512)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.985019 32.27742)
		(end 93.962089 32.321903)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.131464 26)
		(end 153.180495 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.789806 68.164783)
		(end 111.831232 68.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.062716 26.010812)
		(end 199.111027 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.207075 76.054819)
		(end 139.252823 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.610732 76.324534)
		(end 139.64276 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.558264 78.424549)
		(end 185.536218 78.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.008822 120.376144)
		(end 93.988952 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.210193 78.82806)
		(end 185.168767 78.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.679844 118.227594)
		(end 153.720479 118.255742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.017106 76.007234)
		(end 139.065418 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.869523 68.995428)
		(end 139.869523 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.493404 26.010812)
		(end 107.541715 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.896253 51.978786)
		(end 122.636998 51.502023)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.60416 78.99522)
		(end 189.555259 78.991612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.325116 76.946403)
		(end 79.328723 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.631591 89.001724)
		(end 215.570084 88.468954)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.15078 89.027136)
		(end 127.116558 89.562351)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.847909 63.674837)
		(end 121.863358 63.65457)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.512049 76.481833)
		(end 185.536218 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.017106 78.985609)
		(end 138.968441 78.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.653191 70.996422)
		(end 189.60416 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.104374 28.126667)
		(end 97.095855 28.077975)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.611675 118.111159)
		(end 198.659113 118.097264)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.108732 90.124156)
		(end 127.109057 90.149637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.655382 26.949981)
		(end 188.658989 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.472465 55.191203)
		(end 81.397375 55.722229)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.595781 76.658869)
		(end 185.611162 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.900239 57.404981)
		(end 172.901215 57.430446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.765641 118.155667)
		(end 107.809993 118.177495)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.886739 26.029939)
		(end 157.934581 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.417296 26.328112)
		(end 217.449324 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.161657 32.089663)
		(end 157.15047 32.040885)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.558126 70.468347)
		(end 217.533957 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.653431 90.711056)
		(end 215.655057 90.685624)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.180782 120.420971)
		(end 97.160911 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.466721 67.981095)
		(end 160.001455 67.940042)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.773004 120.507432)
		(end 199.746771 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.188874 26.662447)
		(end 157.206521 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.656528 79.010451)
		(end 113.114011 78.996591)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.511236 76.193017)
		(end 199.549891 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.111728 26.403896)
		(end 203.141895 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.773608 120.420971)
		(end 139.751562 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.831232 76.138551)
		(end 111.873895 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 207.443616 79.350376)
		(end 206.921415 79.228175)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.665274 76.848838)
		(end 217.671276 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.553619 65.986032)
		(end 177.574463 66.000693)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.610732 78.668309)
		(end 139.576922 78.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.182253 70.878461)
		(end 189.13959 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.207733 70.703821)
		(end 203.173923 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.805846 85.230437)
		(end 168.561756 84.752894)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.064816 64.112407)
		(end 213.081279 64.092956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.643366 78.144005)
		(end 185.634983 78.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.083613 115.100793)
		(end 94.084867 115.150835)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.22786 76.524496)
		(end 108.249906 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.15047 114.951902)
		(end 157.161658 114.903124)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.901216 57.430471)
		(end 172.93544 57.965687)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.72658 26.196595)
		(end 153.765235 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.265519 28.846939)
		(end 144.219674 28.865458)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.427168 59.626916)
		(end 127.433291 59.651653)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.772139 78.468348)
		(end 188.750093 78.42455)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.395839 67.997623)
		(end 107.44474 68.001231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.640881 70.828059)
		(end 93.599455 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.915885 90.711059)
		(end 172.963765 91.245225)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.236197 80.694875)
		(end 131.789799 80.992119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.184628 28.789424)
		(end 190.160992 28.79895)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.114819 81.700162)
		(end 166.09558 81.683452)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.744103 28.489176)
		(end 199.715438 28.529448)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.87051 120.992844)
		(end 112.344833 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.149225 120.588947)
		(end 108.119058 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.329445 67.996416)
		(end 93.085855 67.996416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.315927 118.818501)
		(end 192.341004 118.823033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.400544 68.138551)
		(end 203.443207 68.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.971105 118.076592)
		(end 153.020077 118.069866)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.125666 26.90108)
		(end 154.129273 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.457582 26.403896)
		(end 185.485816 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.248437 76.524496)
		(end 157.272606 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.076675 82.480035)
		(end 129.719856 82.880417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.477886 59.078124)
		(end 215.566515 58.549191)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.65897 28.169806)
		(end 104.128948 28.087939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.534373 70.799826)
		(end 157.495718 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.697195 78.287417)
		(end 188.684118 78.24016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.002142 28.92548)
		(end 198.952803 28.928516)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.30748 94.991343)
		(end 128.319078 95.014034)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.751562 68.524491)
		(end 139.773608 68.568288)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.347686 118.387347)
		(end 97.381992 118.351758)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.197635 78.737633)
		(end 143.162123 78.703823)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.903375 28.929108)
		(end 198.853977 28.927254)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.564981 28.86544)
		(end 198.519136 28.84692)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.37576 78.240164)
		(end 111.365016 78.192322)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.466042 26.485411)
		(end 79.492275 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.990997 28.000651)
		(end 193.455389 28.028036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.558126 120.464769)
		(end 217.533957 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.526871 66.31156)
		(end 210.548436 66.297982)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.22288 84.752877)
		(end 173.978791 85.230419)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.087031 68.324533)
		(end 108.119058 68.361661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.186448 28.916233)
		(end 107.137869 28.907093)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.778543 118.709667)
		(end 196.803356 118.70386)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.275115 67.085235)
		(end 163.761656 66.859617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.176329 76.007234)
		(end 80.224993 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.751562 120.464769)
		(end 139.727393 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.57758 68.054819)
		(end 203.624138 68.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.864712 78.095341)
		(end 139.85871 78.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.05322 120.700243)
		(end 108.017708 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.656891 70.192317)
		(end 217.646147 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.770603 78.991612)
		(end 143.721939 78.98561)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.315881 26.756262)
		(end 108.326624 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.858709 26.852416)
		(end 139.864711 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.319029 76.193017)
		(end 203.359118 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.415697 54.614612)
		(end 215.286839 54.094016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.901835 26.168362)
		(end 107.941924 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.092099 52.001487)
		(end 173.860288 52.485109)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.334831 28.077956)
		(end 108.326312 28.126649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.95815 120.283838)
		(end 202.945072 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.451593 66.297966)
		(end 86.473158 66.311544)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.302803 26.709005)
		(end 108.315881 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.809992 28.815329)
		(end 107.76564 28.837157)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.021219 61.762401)
		(end 123.032234 61.739421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.102084 120.962904)
		(end 112.054827 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.335008 76.848838)
		(end 108.34101 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.902362 118.391149)
		(end 144.926453 118.399456)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.08607 68.946399)
		(end 97.089677 68.897498)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.558126 26.528074)
		(end 217.580172 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.797172 68.524495)
		(end 199.819218 68.568293)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.97353 68.658868)
		(end 202.991177 68.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.034562 76.568294)
		(end 154.054432 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.676087 26.999012)
		(end 217.676087 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.050175 28.846939)
		(end 190.00433 28.865458)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.910244 118.963922)
		(end 199.91391 119.013218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.252686 68.054818)
		(end 199.298433 68.072465)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.965151 120.99164)
		(end 198.916121 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.231036 81.006811)
		(end 165.210192 80.99215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.798127 86.799594)
		(end 81.790749 86.823986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.146021 28.927272)
		(end 98.096624 28.929126)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.988952 78.424549)
		(end 93.966906 78.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.495438 92.923452)
		(end 169.50219 92.89888)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.550675 120.627602)
		(end 79.520508 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.04185 70.287416)
		(end 94.026469 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.302106 28.222472)
		(end 108.286479 28.269369)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.118719 28.929108)
		(end 153.069321 28.927254)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.665786 62.262381)
		(end 82.933941 62.726837)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.468029 76.054819)
		(end 153.513777 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.028895 118.07661)
		(end 144.077474 118.08575)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.298433 26.076044)
		(end 199.34326 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.226051 120.896929)
		(end 189.182254 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.636536 54.639522)
		(end 169.631047 54.614637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.487005 120.896929)
		(end 203.443208 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.069217 118.463395)
		(end 143.099839 118.42459)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.266614 118.072818)
		(end 153.315411 118.080714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.855791 28.269369)
		(end 199.837862 28.315435)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.798147 60.193255)
		(end 81.96648 60.702461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.919541 75.997625)
		(end 138.968442 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.343471 67.982392)
		(end 183.885988 67.996252)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.376294 118.193893)
		(end 144.39993 118.203419)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.391612 70.996422)
		(end 158.129489 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.128581 118.770371)
		(end 97.144208 118.723474)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.130476 77.997414)
		(end 154.129273 78.046444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.226391 26.571872)
		(end 157.248437 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.288937 120.766081)
		(end 185.250282 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.160517 70.953405)
		(end 139.11326 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.05127 118.072818)
		(end 199.100067 118.080714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.768913 81.00681)
		(end 131.338275 81.326459)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.746615 118.818501)
		(end 100.771692 118.823033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.495417 54.069394)
		(end 169.340144 53.556056)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.888184 79.222988)
		(end 135.863231 79.228159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.814106 113.4909)
		(end 214.200094 95.501999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 207.468356 67.636028)
		(end 207.983635 67.487324)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.612941 70.878461)
		(end 97.570278 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.343418 79.123719)
		(end 205.811477 79.055414)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.512049 120.507432)
		(end 185.485817 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.683374 120.934446)
		(end 107.636815 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.497802 54.093988)
		(end 127.368946 54.614586)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.947269 62.748617)
		(end 83.238789 63.198775)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.425537 68.164778)
		(end 139.465626 68.193012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.640881 76.164784)
		(end 93.68097 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.01942 68.22318)
		(end 189.058075 68.193013)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.580172 70.424549)
		(end 217.558126 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.295802 26.001203)
		(end 112.344833 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.945567 70.379722)
		(end 142.92792 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.713146 54.093988)
		(end 81.58429 54.614586)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.697195 26.709005)
		(end 188.712576 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.74677 78.55244)
		(end 199.718536 78.592529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.850074 120.973648)
		(end 184.801762 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.896291 95.01407)
		(end 122.907889 94.991379)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.533003 67.095367)
		(end 180.030431 67.295849)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.152129 63.674839)
		(end 175.48804 64.092919)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.925945 78.144011)
		(end 202.919943 78.095346)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.49508 118.136079)
		(end 143.541371 118.11874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.962131 83.772997)
		(end 167.648006 83.338311)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.746787 83.772997)
		(end 213.432662 83.338311)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.514183 70.552436)
		(end 111.48795 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.962114 68.440405)
		(end 153.988347 68.481831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.496733 84.265984)
		(end 122.483432 84.244248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.652975 78.04644)
		(end 185.649368 78.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.466042 76.481833)
		(end 79.492275 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.850327 68.800521)
		(end 139.85871 68.848832)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.182254 120.874883)
		(end 189.13959 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.250282 76.193017)
		(end 185.288937 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.849219 57.965707)
		(end 169.883441 57.430492)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.802364 120.734053)
		(end 153.765236 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.868535 67.996417)
		(end 153.131465 67.99642)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.082306 76.092336)
		(end 185.126104 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.44474 120.988033)
		(end 107.395839 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.296599 82.899905)
		(end 167.280135 82.880453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.799899 51.490855)
		(end 82.793666 51.501976)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.066118 76.400318)
		(end 143.096285 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.113963 28.028036)
		(end 194.578356 28.000651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.904319 26.852416)
		(end 199.910322 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.677074 75.996422)
		(end 216.726105 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.896412 79.222994)
		(end 206.368653 79.127617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.514183 76.440407)
		(end 111.542416 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.227859 26.528074)
		(end 108.249905 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.968442 76.001232)
		(end 139.017106 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.269776 78.379727)
		(end 108.249905 78.424553)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.915132 68.995434)
		(end 202.916336 68.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.360074 60.168839)
		(end 173.367452 60.193231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.968442 68.001227)
		(end 139.017106 68.007229)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.098164 120.824481)
		(end 189.058075 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.390618 114.854967)
		(end 111.406629 114.807552)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.600045 28.789415)
		(end 152.097661 28.601703)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.624239 70.240159)
		(end 185.611162 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.870511 67.996416)
		(end 138.919541 67.997619)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.289238 92.923449)
		(end 173.444511 93.436787)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.119664 76.848838)
		(end 154.125666 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.126104 78.878461)
		(end 185.082306 78.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.538913 67.295862)
		(end 209.036339 67.095382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.281462 78.592526)
		(end 97.253229 78.552438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.656342 70.668309)
		(end 199.622532 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.771734 28.16981)
		(end 100.746656 28.174342)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.68097 26.196595)
		(end 93.719625 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.975015 28.706959)
		(end 107.935822 28.737083)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.327072 78.592531)
		(end 157.298839 78.552442)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.128017 120.973648)
		(end 80.080175 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.648641 59.651677)
		(end 81.790754 60.168814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.76593 28.288989)
		(end 191.247022 28.424485)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.13959 78.854294)
		(end 189.098164 78.828061)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.311629 68.361658)
		(end 97.343657 68.32453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.684603 28.174878)
		(end 188.673686 28.126667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.065187 52.508409)
		(end 127.858373 53.003237)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.235066 84.730467)
		(end 174.222892 84.752854)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.388837 70.287416)
		(end 111.37576 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.636815 76.039438)
		(end 107.683373 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.504281 26.226762)
		(end 139.541409 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.422891 32.564045)
		(end 157.407965 32.54339)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.941143 113.98619)
		(end 111.954995 113.9648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 223.676086 20.012247)
		(end 223.675816 20.001245)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.104062 70.192317)
		(end 97.095679 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.126104 70.878461)
		(end 185.082306 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.510455 113.98619)
		(end 203.524307 113.9648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.616507 28.928534)
		(end 189.567169 28.925498)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.819218 120.420971)
		(end 199.797172 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.288937 68.223179)
		(end 185.326066 68.255206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.520991 32.407092)
		(end 111.493726 32.365126)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.096285 68.361658)
		(end 143.128313 68.32453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.991731 78.938024)
		(end 184.945173 78.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.347024 76.946403)
		(end 111.350631 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.24698 118.568359)
		(end 191.765889 118.703854)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.488763 120.796248)
		(end 97.450108 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.01267 28.674934)
		(end 107.975015 28.706959)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.756754 120.734053)
		(end 93.719625 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.578528 26.043016)
		(end 143.625785 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.838342 114.90318)
		(end 139.849529 114.951958)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.656739 76.092336)
		(end 97.701566 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.085855 67.996416)
		(end 93.134885 67.997619)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.874333 70.095341)
		(end 142.870726 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.91391 119.013218)
		(end 199.915133 119.062647)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.888271 76.400318)
		(end 93.916504 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.602402 70.878461)
		(end 153.558604 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.085854 75.996422)
		(end 93.134885 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.688374 59.103167)
		(end 169.693226 59.07815)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.851987 76.114382)
		(end 79.895785 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.967081 120.949827)
		(end 216.919824 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.729121 78.920381)
		(end 107.683373 78.938028)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.826506 78.287416)
		(end 139.811125 78.333975)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.141636 93.989582)
		(end 169.150859 93.965827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.144208 118.723474)
		(end 97.162137 118.677408)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.273419 76.193017)
		(end 143.313508 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.287423 26.662447)
		(end 108.302803 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.008822 68.613115)
		(end 94.026469 68.658863)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.850774 78.592526)
		(end 188.822541 78.552438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.485816 26.443985)
		(end 185.512049 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.513777 26.076044)
		(end 153.558604 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.602402 120.874883)
		(end 153.558604 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.196192 28.88913)
		(end 199.148414 28.90181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.64276 70.63118)
		(end 139.610732 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.13959 120.850714)
		(end 189.098164 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.580172 76.568294)
		(end 217.600042 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.328603 26.029939)
		(end 93.37586 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.412979 70.737631)
		(end 97.377467 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.523319 91.826798)
		(end 215.52753 91.801665)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.395389 120.664731)
		(end 185.361578 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.53197 120.934446)
		(end 143.486222 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.265519 118.145923)
		(end 144.376271 118.193883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.541716 70.977226)
		(end 107.493404 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.465626 26.196595)
		(end 139.504281 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.898757 67.996416)
		(end 184.655167 67.996416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.341448 76.114382)
		(end 139.384111 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.914253 56.307244)
		(end 172.893713 56.843159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.664991 68.848833)
		(end 188.673374 68.800522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.315183 118.42459)
		(end 97.347686 118.387347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.180495 70.995218)
		(end 153.131464 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.287423 78.333979)
		(end 108.269776 78.379727)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.084866 26.999012)
		(end 97.08607 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.207733 68.289022)
		(end 203.243245 68.255211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.135287 26.90108)
		(end 157.141289 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.131681 120.042862)
		(end 157.130477 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.550296 28.837157)
		(end 153.504919 28.856764)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.429721 120.850714)
		(end 199.387058 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.510632 82.062082)
		(end 166.114838 81.700179)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.746824 63.219843)
		(end 213.761218 63.198814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.934328 68.800526)
		(end 202.945072 68.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.673628 68.015613)
		(end 143.721939 68.00723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.362972 51.501987)
		(end 174.10372 51.97875)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.756753 26.25879)
		(end 93.792266 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.071135 28.269369)
		(end 154.053206 28.315435)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.606956 70.996422)
		(end 112.344833 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.638421 120.700243)
		(end 111.604611 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.079855 31.94201)
		(end 94.073603 31.991663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.744103 118.503649)
		(end 199.770741 118.54529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.576922 68.289016)
		(end 139.610733 68.324529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.584032 67.865236)
		(end 161.11179 67.76986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.443207 76.114382)
		(end 203.487005 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.101292 67.996421)
		(end 113.114035 67.996259)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.868534 26)
		(end 153.131464 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.130476 68.995432)
		(end 154.130476 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.831232 120.850714)
		(end 111.789806 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.85871 78.144005)
		(end 139.850327 78.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.707181 28.907093)
		(end 198.659113 28.895561)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.104812 118.227612)
		(end 189.146789 118.201509)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.095679 26.852416)
		(end 97.104062 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.54141 68.255206)
		(end 139.576922 68.289016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.34326 70.900507)
		(end 199.298433 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.746771 120.548858)
		(end 199.718537 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.288848 118.399455)
		(end 106.31294 118.391149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.095607 65.309408)
		(end 166.114847 65.292698)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.707181 118.085732)
		(end 198.755761 118.076592)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.773608 78.424549)
		(end 139.751562 78.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.949824 28.84692)
		(end 106.839072 28.79896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.985947 70.991611)
		(end 97.937283 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.34582 69.997409)
		(end 111.34582 68.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.11558 89.587866)
		(end 127.108732 90.12413)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.148414 28.90181)
		(end 199.100067 28.91211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.933881 120.588947)
		(end 153.903714 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.228282 28.169806)
		(end 195.69826 28.087939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.937283 120.982031)
		(end 97.888972 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.978809 61.762406)
		(end 174.222899 62.239949)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.895624 28.126649)
		(end 199.884707 28.17486)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.92792 26.662447)
		(end 142.945567 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.819504 120.99164)
		(end 143.770604 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.335008 120.140427)
		(end 108.326625 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.150156 94.484434)
		(end 123.35697 93.989606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.186449 118.076592)
		(end 107.235421 118.069866)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.103587 67.769849)
		(end 90.631346 67.865226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.747314 68.054815)
		(end 97.793872 68.039434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.085746 90.685599)
		(end 124.106286 90.149684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.44643 65.986033)
		(end 119.877068 65.666384)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.143264 26.662447)
		(end 97.160911 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.558604 26.095914)
		(end 153.602401 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.141289 78.144011)
		(end 157.135287 78.095346)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.809324 120.850714)
		(end 79.767898 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.102871 65.650646)
		(end 177.122939 65.666352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.011652 70.51101)
		(end 142.987483 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.453718 66.859602)
		(end 87.94026 67.085221)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.68837 76.361663)
		(end 199.718537 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.384701 28.789415)
		(end 197.882317 28.601703)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.389267 120.664731)
		(end 157.35724 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.400544 120.850714)
		(end 203.359118 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.21546 80.144556)
		(end 132.741074 80.394723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.945072 120.236581)
		(end 202.934329 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.542416 68.400318)
		(end 111.572583 68.361662)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.570086 28.029988)
		(end 103.544677 28.028037)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.697195 76.705427)
		(end 188.712576 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.620694 28.815348)
		(end 97.577477 28.791353)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.421471 78.953409)
		(end 153.374213 78.966487)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.616513 70.703821)
		(end 79.582703 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.718537 70.592525)
		(end 199.68837 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.210193 120.824481)
		(end 185.168767 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.777119 62.239966)
		(end 123.021208 61.762424)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.611162 68.705421)
		(end 185.624239 68.752679)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.534373 68.193017)
		(end 157.574462 68.164783)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.069216 28.529466)
		(end 143.040552 28.489194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.922525 118.085732)
		(end 152.971105 118.076592)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.575005 32.231845)
		(end 185.554331 32.27742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.08607 76.946403)
		(end 97.089677 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.344598 119.013218)
		(end 108.345821 119.062647)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.106611 56.868687)
		(end 124.106286 56.843206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.577579 26.058397)
		(end 203.624138 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.251641 61.249992)
		(end 123.261468 61.22648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.786137 67.940039)
		(end 205.811487 67.93744)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.033022 118.632267)
		(end 154.053207 118.67739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.073736 93.989575)
		(end 82.280553 94.4844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.074054 68.848832)
		(end 94.080056 68.897497)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.637866 28.791334)
		(end 153.594648 28.815329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.034561 26.571872)
		(end 154.054432 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.141289 68.848838)
		(end 157.149672 68.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.589558 76.026361)
		(end 107.636815 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.234764 68.22318)
		(end 143.273419 68.193013)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.284561 118.463395)
		(end 97.315183 118.42459)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.914145 26)
		(end 216.677074 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.945567 26.616699)
		(end 142.965437 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.486221 26.076044)
		(end 143.531969 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.037885 70.552436)
		(end 143.011652 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.895937 78.192321)
		(end 199.885193 78.240163)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.73448 118.145904)
		(end 152.780325 118.127385)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.915133 115.150779)
		(end 202.916387 115.100737)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.578352 95.490831)
		(end 128.584582 95.501948)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.92792 70.333974)
		(end 142.912539 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.281147 80.40721)
		(end 164.258917 80.394751)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.102083 78.966488)
		(end 112.054826 78.95341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.719625 70.769659)
		(end 93.68097 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.357239 68.361662)
		(end 157.389267 68.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.967783 61.739404)
		(end 173.978798 61.762383)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.697195 68.705423)
		(end 188.712576 68.658864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.441735 68.568294)
		(end 111.463781 68.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.162123 76.289022)
		(end 143.197635 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.90432 70.144005)
		(end 199.895937 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.463782 120.464769)
		(end 111.441736 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.284665 28.927254)
		(end 107.23542 28.922959)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.115291 28.174878)
		(end 97.104374 28.126667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.77074 28.447535)
		(end 199.744103 28.489176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.240255 60.726486)
		(end 169.248869 60.702503)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.316626 70.938024)
		(end 189.270878 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.43348 88.443677)
		(end 81.429912 88.46891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.389267 70.668309)
		(end 157.357239 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.421471 70.953405)
		(end 153.374214 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.361578 70.703821)
		(end 185.326066 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.036308 79.897476)
		(end 208.53888 79.696994)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.683373 78.938028)
		(end 107.636815 78.953409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.827018 28.881665)
		(end 152.780325 28.86544)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.869522 26.999012)
		(end 139.869522 31.842064)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.34326 78.900511)
		(end 199.298433 78.920381)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.111028 76.015617)
		(end 199.15887 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.026469 68.658863)
		(end 94.04185 68.705421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.84787 83.318004)
		(end 121.511959 82.899924)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.917693 76.092336)
		(end 111.96252 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.916386 31.89205)
		(end 202.915132 31.842008)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.624138 26.043016)
		(end 203.671395 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.421669 118.992193)
		(end 102.447144 118.992843)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.089677 120.091763)
		(end 97.08607 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.504919 28.856764)
		(end 153.458628 28.874103)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.980579 70.769659)
		(end 107.941924 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.397597 70.878461)
		(end 143.354934 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.425537 26.168362)
		(end 139.465626 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.60416 67.997621)
		(end 189.653191 67.996417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.022976 80.133237)
		(end 179.000139 80.144545)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.965438 68.56829)
		(end 142.987483 68.524492)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.149225 70.592525)
		(end 108.119058 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.261336 55.166045)
		(end 127.257125 55.191178)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.816213 70.991611)
		(end 203.767549 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.026468 26.662447)
		(end 94.041849 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.229396 70.991611)
		(end 153.180495 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.686331 64.913072)
		(end 84.704692 64.930743)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.495718 78.769664)
		(end 157.458589 78.737637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.381992 118.351758)
		(end 97.418017 118.317909)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.148012 70.878461)
		(end 217.104214 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.168148 118.064309)
		(end 153.217486 118.067345)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.397597 68.114378)
		(end 143.441395 68.092332)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.229258 28.447553)
		(end 97.204713 28.404646)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.075655 94.507701)
		(end 128.307468 94.991321)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.980579 78.769663)
		(end 107.941924 78.79983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.642759 26.365241)
		(end 139.672926 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.958149 78.287422)
		(end 202.945072 78.240164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.556373 118.823037)
		(end 147.086395 118.904904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.770603 76.001232)
		(end 143.819504 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.117706 118.391149)
		(end 99.141797 118.399456)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.356633 70.144005)
		(end 111.350631 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.410441 26.029939)
		(end 189.458283 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.645065 76.138551)
		(end 153.686491 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.134885 75.997625)
		(end 93.183786 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.871092 28.087939)
		(end 192.341071 28.169806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.346808 26)
		(end 107.395839 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.975941 114.807552)
		(end 202.994306 114.760998)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.584302 92.378231)
		(end 81.71316 92.898827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.558264 120.420971)
		(end 185.536218 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.02945 113.4909)
		(end 168.415438 95.501999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.406629 114.807552)
		(end 111.424994 114.760998)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.05322 70.703821)
		(end 108.017708 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.037479 70.920377)
		(end 184.991731 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.234359 118.155686)
		(end 189.279736 118.136079)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.731449 118.677408)
		(end 188.751634 118.632285)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.730223 26.616699)
		(end 188.750093 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.022966 33.490968)
		(end 157.739706 33.028065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.252685 26.058397)
		(end 199.298433 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.073603 31.991663)
		(end 94.064873 32.040941)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.073521 28.593379)
		(end 151.562208 28.431565)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.822541 120.548858)
		(end 188.796308 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.453664 80.133237)
		(end 87.430827 80.144545)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.235421 118.069866)
		(end 107.284666 118.065571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.815389 28.789415)
		(end 106.313005 28.601703)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.141895 70.63118)
		(end 203.111728 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.654178 31.842064)
		(end 185.652924 31.892106)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.68097 78.799826)
		(end 93.640881 78.82806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.350631 68.897502)
		(end 111.356633 68.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.057262 78.511016)
		(end 203.033093 78.468352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.801762 78.985609)
		(end 184.753097 78.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.054927 76.752684)
		(end 94.065671 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.880512 118.914887)
		(end 142.889031 118.866194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.945172 26.043016)
		(end 184.991731 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.670554 78.996427)
		(end 203.914144 78.996427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.765235 26.226762)
		(end 153.802363 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.226392 120.420971)
		(end 157.206522 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.792266 26.2926)
		(end 93.826076 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.775006 70.991611)
		(end 216.726105 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.201872 60.193249)
		(end 215.20925 60.168857)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.819217 26.571872)
		(end 199.839088 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.190675 76.138551)
		(end 217.232101 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.274173 113.986212)
		(end 139.577093 114.428777)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.324183 20.001245)
		(end 73.323913 20.012247)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.916504 68.440401)
		(end 93.942737 68.481827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.182253 68.114378)
		(end 189.226051 68.092332)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.447169 118.992844)
		(end 102.983476 118.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.017707 26.25879)
		(end 108.05322 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.044991 33.028065)
		(end 184.76173 33.490969)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.104811 28.765249)
		(end 189.064176 28.737101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.983502 118.992843)
		(end 103.008977 118.992193)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.487005 70.900507)
		(end 203.443207 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.326066 70.737631)
		(end 185.288937 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.316625 78.938025)
		(end 189.270878 78.920378)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.28016 64.112407)
		(end 167.296623 64.092956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.338254 81.326475)
		(end 131.318187 81.342181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.234764 76.223184)
		(end 143.273419 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.923324 64.512808)
		(end 167.280143 64.112426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.95821 55.191203)
		(end 123.953999 55.16607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.032918 26.043016)
		(end 80.080175 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.000116 80.144556)
		(end 178.52573 80.394723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.761625 80.133241)
		(end 163.275083 79.907622)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.973143 79.055406)
		(end 136.441203 79.12371)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.912969 68.32453)
		(end 188.946779 68.289018)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.91254 120.283838)
		(end 142.899462 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.287423 120.330396)
		(end 108.269776 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.377467 68.289018)
		(end 97.412979 68.255207)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.05435 67.304786)
		(end 180.561365 67.479607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.550675 26.365241)
		(end 79.582703 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.327072 70.592525)
		(end 157.298839 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.469244 28.912129)
		(end 189.420897 28.901828)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.064177 118.25576)
		(end 189.104812 118.227612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.377467 26.2926)
		(end 97.412979 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.97594 32.185235)
		(end 202.959929 32.13782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.863373 63.654549)
		(end 122.177498 63.219864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.899462 68.75268)
		(end 142.912539 68.705423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.83079 61.226456)
		(end 215.024902 60.72651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.654179 119.062666)
		(end 188.655402 119.013237)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.954007 91.826798)
		(end 123.958218 91.801665)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.896471 67.769855)
		(end 206.921424 67.764684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.756754 68.255206)
		(end 93.792266 68.289016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.024983 28.706978)
		(end 188.987328 28.674953)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.985947 26.00481)
		(end 98.034848 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.210193 26.168362)
		(end 185.250282 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.589558 68.026359)
		(end 107.636815 68.039437)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.486222 120.916799)
		(end 143.441395 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.206341 28.000651)
		(end 147.670733 28.028036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.229396 120.988033)
		(end 153.180495 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.809324 70.854292)
		(end 79.767898 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.322925 26)
		(end 93.085854 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.753098 76.001232)
		(end 184.801762 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.441395 78.900508)
		(end 143.397597 78.878462)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.389267 76.324534)
		(end 157.423077 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.558264 76.568294)
		(end 185.578134 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.81414 33.501933)
		(end 203.807629 33.490979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.115292 118.817983)
		(end 97.128581 118.770371)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.089677 70.095341)
		(end 97.08607 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.797327 118.31789)
		(end 153.833351 118.351739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.671276 76.897502)
		(end 217.674883 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.421866 120.376144)
		(end 111.404219 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.058856 33.006653)
		(end 185.045004 33.028043)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.00433 28.865458)
		(end 189.957636 28.881684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.74677 76.440407)
		(end 199.773003 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.272606 70.51101)
		(end 157.248437 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.014051 78.991615)
		(end 198.965151 78.995222)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.871687 120.664731)
		(end 153.837876 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.697196 120.283838)
		(end 188.684118 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.62688 118.103694)
		(end 107.673973 118.118722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.360054 86.82401)
		(end 173.217942 87.341147)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.822541 78.552438)
		(end 188.796308 78.511012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.325116 120.042862)
		(end 79.323913 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.899475 81.700162)
		(end 211.880236 81.683452)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.08607 70.04644)
		(end 97.084867 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.136665 63.654552)
		(end 175.152113 63.674819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.062717 120.982031)
		(end 199.014052 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.149672 78.192322)
		(end 157.141289 78.144011)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.423077 26.2926)
		(end 157.458589 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.680909 51.978786)
		(end 168.421654 51.502023)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.238803 63.198796)
		(end 83.253197 63.219825)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.100537 26.756262)
		(end 154.11128 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.327072 76.400318)
		(end 157.357239 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.753002 118.568352)
		(end 105.777486 118.561286)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.623687 118.193883)
		(end 152.73448 118.145904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.226996 120.507432)
		(end 97.202828 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.817971 91.270589)
		(end 169.820893 91.245274)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.343108 120.188739)
		(end 79.334725 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.874457 28.895561)
		(end 152.827018 28.881665)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.92792 68.658864)
		(end 142.945567 68.613116)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.114806 70.240159)
		(end 97.104062 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.502197 92.898855)
		(end 169.631053 92.378257)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.255643 64.913072)
		(end 176.274004 64.930743)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.111281 70.192317)
		(end 154.100537 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.139722 94.507711)
		(end 123.150146 94.484457)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.585709 67.487311)
		(end 181.100989 67.636016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.913579 28.087936)
		(end 149.888303 28.08469)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.111756 79.222994)
		(end 160.583997 79.127617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.131229 90.711059)
		(end 127.179109 91.245225)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.160911 78.379724)
		(end 97.143264 78.333976)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.870726 120.042862)
		(end 142.869523 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.910322 68.897501)
		(end 199.913929 68.946401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.037868 63.219846)
		(end 129.351993 63.654532)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.143264 78.333976)
		(end 97.127883 78.287417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.111028 68.015616)
		(end 199.15887 68.026359)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.640881 78.82806)
		(end 93.599455 78.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.87704 81.326476)
		(end 119.4464 81.006826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.903375 118.063717)
		(end 198.952804 118.064309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.550675 76.361663)
		(end 79.582703 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.730362 67.304791)
		(end 162.754233 67.295872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.683641 79.35682)
		(end 161.658985 79.350382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.180781 70.424549)
		(end 97.160911 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.444739 26.00481)
		(end 107.493404 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.751562 76.524496)
		(end 139.773608 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.295802 75.997625)
		(end 112.344833 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.777088 84.752872)
		(end 122.764914 84.730484)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.111028 120.973648)
		(end 199.062717 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.462324 118.568359)
		(end 145.981233 118.703854)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.084867 76.995434)
		(end 94.084867 77.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.117723 28.601703)
		(end 98.61534 28.789415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.421471 26.043016)
		(end 153.468029 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.102083 76.026361)
		(end 112.149925 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.252685 70.938024)
		(end 199.206127 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.52682 80.681286)
		(end 210.065825 80.407222)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.558263 26.571872)
		(end 185.578133 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.544651 28.028036)
		(end 103.009044 28.000651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.988347 78.511014)
		(end 153.962114 78.55244)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.599455 78.854292)
		(end 93.556792 78.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178.020905 66.297966)
		(end 178.04247 66.311544)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.797172 120.464769)
		(end 199.773004 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.837876 26.2926)
		(end 153.871686 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.134885 78.995218)
		(end 93.085854 78.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.673374 68.800522)
		(end 188.684118 68.75268)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.278382 114.627661)
		(end 157.305647 114.585695)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.086436 28.087939)
		(end 146.556415 28.169806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.41298 120.734053)
		(end 97.377467 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.673374 70.192317)
		(end 188.664991 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.087459 26.709005)
		(end 154.100537 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.82367 120.982031)
		(end 216.775006 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.23245 70.985609)
		(end 93.183786 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.345821 119.062647)
		(end 108.345821 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.116786 53.531812)
		(end 214.935505 53.027071)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.747314 120.934446)
		(end 97.701566 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.23832 80.133237)
		(end 133.215483 80.144545)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.897176 65.650646)
		(end 120.310932 65.309425)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.817746 78.878465)
		(end 107.773948 78.900511)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.245742 79.696981)
		(end 133.748316 79.897461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.148119 92.353321)
		(end 173.153608 92.378206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.556792 76.114382)
		(end 93.599455 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.694352 114.585751)
		(end 139.721617 114.627717)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.968442 70.991611)
		(end 138.919541 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.655058 90.685599)
		(end 215.675598 90.149684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.185893 33.501943)
		(end 82.799905 51.490844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.91612 75.996422)
		(end 198.965151 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.792924 70.938024)
		(end 157.747176 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.774097 79.010445)
		(end 91.748647 79.011746)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.174791 118.503649)
		(end 108.201429 118.54529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.01063 118.588197)
		(end 154.033022 118.632267)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.244794 113.4909)
		(end 122.630782 95.501999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.13173 31.89205)
		(end 157.130476 31.842008)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.471147 68.164782)
		(end 199.511236 68.193016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.086089 27.979625)
		(end 97.084866 27.930196)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.319052 51.978773)
		(end 128.307454 52.001464)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.636553 92.353322)
		(end 169.738659 91.826823)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.246901 26.00481)
		(end 112.295802 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.909696 32.407148)
		(end 93.880356 32.447706)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.127883 26.709005)
		(end 97.143264 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.550297 118.155667)
		(end 153.594649 118.177495)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.90432 68.848836)
		(end 199.910322 68.897501)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.206127 68.039437)
		(end 199.252686 68.054818)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.030454 67.295858)
		(end 180.054326 67.304778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.809993 118.177495)
		(end 107.85321 118.20149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.032245 61.739398)
		(end 123.251631 61.250016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.874362 67.642473)
		(end 115.899019 67.636035)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.202828 120.464769)
		(end 97.180782 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.065671 78.192317)
		(end 94.054927 78.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.673973 118.118722)
		(end 107.720264 118.13606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.295802 78.995224)
		(end 112.246901 78.991616)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.096286 120.627602)
		(end 143.066119 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.443207 78.878466)
		(end 203.400544 78.854298)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.326066 68.255206)
		(end 185.361578 68.289016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.415967 79.127607)
		(end 135.888209 79.222983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.008822 78.379722)
		(end 93.988952 78.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.50492 118.13606)
		(end 153.550297 118.155667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.180495 78.995222)
		(end 153.131464 78.996426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.636991 51.502012)
		(end 122.630761 51.490895)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.27806 26.010812)
		(end 153.326371 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.400544 76.138551)
		(end 203.443207 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.850327 76.800526)
		(end 139.85871 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.935496 53.027047)
		(end 214.926272 53.003292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.04185 76.705427)
		(end 94.054927 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.636241 118.091033)
		(end 143.684588 118.080733)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.807622 33.490968)
		(end 203.524362 33.028065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.802364 68.25521)
		(end 153.837876 68.28902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.281462 76.400318)
		(end 97.311629 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.645065 68.138549)
		(end 153.686491 68.164782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.328604 120.962904)
		(end 93.280762 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.750093 26.571872)
		(end 188.772139 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.37576 120.236581)
		(end 111.365017 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.104214 26.095914)
		(end 217.148012 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.799376 67.865236)
		(end 115.327134 67.76986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.933881 76.400318)
		(end 153.962114 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.808714 32.185291)
		(end 139.790349 32.231845)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.739693 33.028043)
		(end 157.72584 33.006652)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.577135 32.564066)
		(end 139.274214 33.006632)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.352137 67.764678)
		(end 115.874337 67.642479)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.012516 70.468347)
		(end 153.988347 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34582 26.999012)
		(end 108.34582 27.930177)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.042362 28.881665)
		(end 106.995669 28.86544)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.68836 87.88967)
		(end 169.572837 87.365952)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.05322 68.28902)
		(end 108.087031 68.324533)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.334725 120.140427)
		(end 79.328723 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.941924 68.193016)
		(end 107.980579 68.223183)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.345821 119.993831)
		(end 111.345821 115.150779)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.558604 78.900511)
		(end 153.513777 78.920381)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.869523 76.995434)
		(end 139.869523 77.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.773608 70.424549)
		(end 139.751562 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.719237 76.015617)
		(end 203.767549 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.188874 76.658869)
		(end 157.206521 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.043604 66.598107)
		(end 210.065834 66.585649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.592049 114.449473)
		(end 139.665013 114.545193)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.534396 51.978773)
		(end 82.522798 52.001464)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.671395 26.029939)
		(end 203.719237 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.340981 79.35037)
		(end 135.316324 79.356808)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.634983 70.192317)
		(end 185.624239 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.605544 55.747593)
		(end 215.602621 55.722278)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.669075 57.404977)
		(end 215.675923 56.868713)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.183786 120.988033)
		(end 93.134885 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.471147 26.168362)
		(end 199.511236 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.683374 68.054818)
		(end 107.729121 68.072465)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.684118 68.75268)
		(end 188.697195 68.705423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.148012 26.11796)
		(end 217.190675 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.132342 118.387347)
		(end 143.166648 118.351758)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.270878 120.916799)
		(end 189.226051 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.803381 118.703854)
		(end 197.322289 118.568358)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.424994 114.760998)
		(end 111.445668 114.715423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.080458 75.997625)
		(end 158.129489 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.48795 120.507432)
		(end 111.463782 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.988347 68.481831)
		(end 154.012516 68.524495)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.850775 68.400314)
		(end 188.880941 68.361658)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.096285 70.63118)
		(end 143.066118 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.897915 78.966483)
		(end 184.850073 78.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.125588 118.963922)
		(end 154.129254 119.013218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.468167 70.920377)
		(end 93.422419 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.026469 76.658869)
		(end 94.04185 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.912969 76.324534)
		(end 188.946779 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.899462 76.752684)
		(end 142.912539 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.373119 28.889149)
		(end 189.326026 28.874121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.203691 70.51101)
		(end 108.177458 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.518041 28.920025)
		(end 189.469244 28.912129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.912539 26.709005)
		(end 142.92792 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.671395 70.966482)
		(end 203.624138 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.84113 68.026356)
		(end 97.888972 68.015613)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.496544 66.585636)
		(end 118.957538 66.311573)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.141289 70.144005)
		(end 157.135287 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.684588 28.912129)
		(end 143.636241 28.901828)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.601528 85.253439)
		(end 214.590513 85.23046)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.44474 76.001232)
		(end 107.493404 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.913929 70.04644)
		(end 199.910322 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.224993 76.001232)
		(end 80.273894 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.441395 120.896929)
		(end 143.397598 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.661745 65.666368)
		(end 165.681812 65.650662)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.286479 118.723456)
		(end 108.302107 118.770352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.512994 26.095914)
		(end 93.556791 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.099839 118.42459)
		(end 143.132342 118.387347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.921449 67.764678)
		(end 207.443649 67.642479)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.346809 67.99642)
		(end 107.395839 67.997623)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.215514 66.848283)
		(end 133.238351 66.859591)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.044962 113.9648)
		(end 185.058815 113.986191)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.292019 82.480035)
		(end 83.9352 82.880417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.357504 59.62691)
		(end 215.473025 59.103192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.982893 68.007234)
		(end 158.031558 68.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.080056 76.897502)
		(end 94.083663 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.388325 118.111178)
		(end 98.435018 118.127403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.031557 76.001232)
		(end 158.080458 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.313508 120.824481)
		(end 143.273419 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.098164 26.168362)
		(end 189.13959 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.162136 28.315453)
		(end 97.144208 28.269387)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.654179 77.997409)
		(end 185.652975 78.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.134885 67.997619)
		(end 93.183786 68.001227)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.704197 67.997619)
		(end 184.753098 68.001227)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.383491 28.928516)
		(end 107.334063 28.929108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.084867 76.995434)
		(end 97.08607 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.41429 79.505532)
		(end 115.89901 79.356827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.899462 70.240159)
		(end 142.888718 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.13959 76.138551)
		(end 189.182253 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.804732 28.922959)
		(end 198.75576 28.916233)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.680947 95.01407)
		(end 168.692545 94.991379)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.316626 120.934446)
		(end 189.270878 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.919943 70.095341)
		(end 202.916336 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.43861 79.513228)
		(end 116.414314 79.505539)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.652313 118.387329)
		(end 199.684817 118.424571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.767549 70.985609)
		(end 203.719237 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.422419 26.058397)
		(end 93.468167 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.098786 57.430467)
		(end 124.099762 57.405002)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.712576 26.662447)
		(end 188.730223 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.528852 120.824481)
		(end 97.488763 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.588463 28.889149)
		(end 143.54137 28.874121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.013639 70.938024)
		(end 216.967081 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.334953 118.155667)
		(end 199.379305 118.177495)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.373119 118.103713)
		(end 189.420897 118.091033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.257121 55.191203)
		(end 127.182031 55.722229)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.541371 118.11874)
		(end 143.588463 118.103713)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.477212 94.991356)
		(end 214.709023 94.507734)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.771717 118.823037)
		(end 101.301739 118.904904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.080175 70.966482)
		(end 80.032918 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.037885 76.440407)
		(end 143.066118 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.037479 78.920377)
		(end 184.991731 78.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.188875 120.330396)
		(end 157.173494 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.807419 32.54339)
		(end 93.792493 32.564045)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.363184 68.039434)
		(end 189.410442 68.026356)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.686286 82.079772)
		(end 84.309489 82.461412)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.625786 120.962904)
		(end 143.578528 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.782063 59.651672)
		(end 123.788186 59.626935)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.054826 76.039438)
		(end 112.102083 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.801762 70.985609)
		(end 184.753098 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.886739 70.966482)
		(end 157.839482 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.229259 118.545308)
		(end 97.255896 118.503667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.790768 28.283176)
		(end 191.765955 28.288983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.346808 78.996426)
		(end 98.083878 78.996423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.44474 70.991611)
		(end 107.395839 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.549891 68.223183)
		(end 199.58702 68.25521)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.918744 64.092938)
		(end 83.935208 64.11239)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.888261 118.908153)
		(end 149.913537 118.904907)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.34326 68.092335)
		(end 199.387058 68.114381)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.979922 28.922977)
		(end 143.930677 28.927272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.46644 81.342197)
		(end 211.446372 81.326491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.673933 78.737637)
		(end 111.638421 78.703827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.79366 51.501987)
		(end 82.534408 51.97875)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.895785 120.896929)
		(end 79.851987 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.438224 84.752877)
		(end 128.194135 85.230419)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.288865 28.593379)
		(end 105.777552 28.431565)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.968442 120.988033)
		(end 138.919541 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.180495 75.997625)
		(end 153.229396 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.327082 28.08469)
		(end 101.301806 28.087936)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.880335 70.144005)
		(end 142.874333 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.421647 51.502012)
		(end 168.415417 51.490895)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.991731 76.054819)
		(end 185.037479 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.674883 26.949981)
		(end 217.676087 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.125666 68.897501)
		(end 154.129273 68.946401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.011047 68.568294)
		(end 203.033093 68.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.851987 120.874883)
		(end 79.809324 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.251316 79.011753)
		(end 205.225866 79.010452)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.455364 28.028037)
		(end 193.429955 28.029988)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.092136 94.991343)
		(end 174.103734 95.014034)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.638208 114.428777)
		(end 111.941129 113.986211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.098164 78.828061)
		(end 189.058075 78.799827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.206127 76.039438)
		(end 199.252685 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.793872 76.039438)
		(end 97.841129 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.822524 63.219846)
		(end 175.136649 63.654532)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.71988 64.112409)
		(end 130.076701 64.512791)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.816214 68.001232)
		(end 203.865114 67.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.458283 26.019195)
		(end 189.506594 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.160416 78.240164)
		(end 157.149672 78.192322)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.860311 94.507701)
		(end 174.092124 94.991321)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.273419 26.196595)
		(end 143.313508 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.226051 70.900507)
		(end 189.182253 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.201429 118.54529)
		(end 108.225974 118.588197)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.400544 70.854292)
		(end 203.359118 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.441735 70.424549)
		(end 111.421865 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.307443 52.001487)
		(end 128.075632 52.485109)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.942737 78.51101)
		(end 93.916504 78.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.202827 70.468347)
		(end 97.180781 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.895785 26.095914)
		(end 79.940612 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.085742 56.307241)
		(end 124.084116 56.28181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.427415 26.365241)
		(end 185.457582 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.622998 114.90318)
		(end 185.634185 114.951958)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.984257 81.00681)
		(end 85.553619 81.326459)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.032216 85.253439)
		(end 123.021201 85.23046)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.633875 57.965707)
		(end 215.668097 57.430492)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.394455 91.24525)
		(end 81.397378 91.270565)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.069322 118.065571)
		(end 153.118719 118.063717)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.313713 64.913071)
		(end 212.69051 64.531431)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.050175 118.145923)
		(end 190.160927 118.193883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.750094 68.56829)
		(end 188.772139 68.524492)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.033315 91.270589)
		(end 124.036237 91.245274)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.037479 76.072466)
		(end 185.082306 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.869522 27.930196)
		(end 142.869522 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.45859 120.734053)
		(end 157.423077 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.555259 26.00481)
		(end 189.60416 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.85871 68.848832)
		(end 139.864712 68.897497)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.464499 28.765231)
		(end 199.422522 28.791334)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.755171 113.49091)
		(end 184.761682 113.501864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.858104 70.63118)
		(end 93.826076 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.102823 81.342197)
		(end 176.689067 81.683418)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.130476 76.995434)
		(end 157.13168 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.198237 76.007234)
		(end 112.246901 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.046108 85.766381)
		(end 169.036281 85.742869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.70116 70.552436)
		(end 139.672927 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.870726 26.949981)
		(end 142.874333 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.914145 120.992844)
		(end 203.865114 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.721939 120.982031)
		(end 143.673628 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.302804 120.283838)
		(end 108.287423 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.111729 120.588947)
		(end 203.083495 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.991732 120.934446)
		(end 184.945173 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.261478 61.226456)
		(end 123.45559 60.72651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.888718 70.192317)
		(end 142.880335 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.54141 78.737632)
		(end 139.504281 78.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.622532 26.2926)
		(end 199.656342 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.411536 118.103694)
		(end 153.458629 118.118722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.310845 26.226762)
		(end 217.347974 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.712576 78.333976)
		(end 188.697195 78.287417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.255896 118.503667)
		(end 97.284561 118.463395)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.461142 67.295858)
		(end 88.485014 67.304778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.624138 76.039438)
		(end 203.671395 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.405351 118.177514)
		(end 143.449703 118.155686)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.558604 120.896929)
		(end 153.513778 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.686491 78.828064)
		(end 153.645065 78.854297)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.095679 76.848838)
		(end 97.104062 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178.525707 80.394736)
		(end 178.503477 80.407194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.425537 78.82806)
		(end 139.384111 78.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.353852 70.240159)
		(end 79.343108 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.449324 70.63118)
		(end 217.417296 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.793872 78.953406)
		(end 97.747313 78.938025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.858104 78.631181)
		(end 93.826076 78.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.315881 70.240159)
		(end 108.302804 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.796308 76.481833)
		(end 188.822541 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.956395 80.394736)
		(end 86.934165 80.407194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.811451 79.055411)
		(end 205.786101 79.052812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.942737 70.51101)
		(end 93.916504 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.005694 114.761054)
		(end 94.024059 114.807608)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.511236 70.799826)
		(end 199.471147 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.062716 68.007233)
		(end 199.111028 68.015616)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.27219 120.796248)
		(end 217.232101 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.688369 26.365241)
		(end 199.718536 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.173494 120.283838)
		(end 157.160416 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.260335 33.028065)
		(end 138.977074 33.490969)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.427416 78.631181)
		(end 185.395388 78.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.656891 76.800526)
		(end 217.665274 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.079856 115.050889)
		(end 94.083613 115.100793)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.868775 90.711056)
		(end 169.870401 90.685624)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.871982 76.015617)
		(end 216.919824 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.582703 26.328112)
		(end 79.616513 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.101014 67.636023)
		(end 181.12567 67.642461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.512994 70.900507)
		(end 93.468167 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.860409 76.138551)
		(end 107.901835 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.868535 120.992844)
		(end 143.819504 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.059716 79.907612)
		(end 209.036331 79.897485)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.479491 26.403896)
		(end 217.507724 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.160911 26.616699)
		(end 97.180781 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.532948 79.897471)
		(end 179.509563 79.907598)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.839583 78.240159)
		(end 139.826506 78.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.558604 76.092336)
		(end 153.602402 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.014052 76.001232)
		(end 199.062716 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.789806 26.168362)
		(end 111.831232 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.423077 120.700243)
		(end 157.389267 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.916336 68.946403)
		(end 202.919943 68.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.632565 63.674837)
		(end 167.648014 63.65457)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.334725 70.144005)
		(end 79.328723 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.471147 120.824481)
		(end 199.429721 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.417296 70.668309)
		(end 217.383486 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.672927 120.588947)
		(end 139.64276 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.488056 64.092938)
		(end 175.50452 64.11239)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 223.663814 20)
		(end 73.336185 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.502177 54.093991)
		(end 169.495424 54.069418)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.935436 89.027136)
		(end 172.901214 89.562351)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.084867 119.062666)
		(end 97.08609 119.013237)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.160968 28.79896)
		(end 190.050175 28.846939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.783174 79.052804)
		(end 182.757824 79.055403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.15047 32.040885)
		(end 157.141739 31.991607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.280374 26.226762)
		(end 203.319029 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.084867 69.997409)
		(end 97.084867 68.995429)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.226391 68.568294)
		(end 157.248437 68.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.280564 94.484424)
		(end 82.290988 94.507678)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.72658 76.193017)
		(end 153.765235 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.098164 70.828059)
		(end 189.058075 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 223.674841 20.00027)
		(end 223.663839 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.252823 76.072466)
		(end 139.29765 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.570278 76.138551)
		(end 97.612941 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.689154 26.226762)
		(end 79.727809 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.659113 28.895561)
		(end 198.611674 28.881665)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.257835 66.311557)
		(end 132.71883 66.585621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.615888 76.138551)
		(end 157.658551 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.534373 78.799831)
		(end 157.495718 78.769664)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.802364 70.737631)
		(end 153.765235 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.034848 70.995218)
		(end 97.985947 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.900161 118.424571)
		(end 153.930783 118.463377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.295288 82.062082)
		(end 211.899494 81.700179)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.206521 76.613121)
		(end 157.226391 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.665936 118.063735)
		(end 189.715334 118.065589)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.558815 67.982392)
		(end 138.101332 67.996252)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.577108 114.428798)
		(end 139.592034 114.449453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.222488 28.431565)
		(end 190.711175 28.59338)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.886036 118.964807)
		(end 102.421643 118.992192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.672917 118.908153)
		(end 195.698193 118.904907)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.683373 76.054819)
		(end 107.729121 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.130476 31.842008)
		(end 157.130476 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.585652 79.505526)
		(end 180.561356 79.513215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.937283 76.007234)
		(end 97.985947 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.727393 78.51101)
		(end 139.70116 78.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.673375 120.188739)
		(end 188.664992 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.958149 68.705427)
		(end 202.97353 68.658868)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.150123 52.508419)
		(end 123.139699 52.485165)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.29765 68.092331)
		(end 139.341448 68.114377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.089677 78.095342)
		(end 97.08607 78.046442)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.868535 70.996422)
		(end 143.819504 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.399954 118.203428)
		(end 144.902338 118.39114)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.503266 62.726859)
		(end 174.516567 62.748595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.160911 70.379722)
		(end 97.143264 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.072079 76.658869)
		(end 154.08746 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.991731 70.938024)
		(end 184.945173 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.031558 68.001232)
		(end 158.080458 67.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.916998 28.605514)
		(end 188.884494 28.568272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.310904 81.683435)
		(end 119.897148 81.342213)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.987483 68.524492)
		(end 143.011652 68.481829)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.797172 70.468347)
		(end 199.773003 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.053207 118.67739)
		(end 154.071135 118.723456)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.010629 28.404627)
		(end 153.986084 28.447535)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.940612 26.076044)
		(end 79.98636 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.738663 91.826798)
		(end 169.742874 91.801665)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.85871 76.848838)
		(end 139.864712 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.820927 85.742845)
		(end 214.601539 85.253463)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.615316 28.789424)
		(end 98.59168 28.79895)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.226391 70.424549)
		(end 157.206521 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.982291 70.737631)
		(end 188.946779 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.457583 78.592525)
		(end 185.427416 78.631181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.326066 120.734053)
		(end 185.288937 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.827019 118.111159)
		(end 152.874457 118.097264)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.885193 76.752684)
		(end 199.895937 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.871687 68.324533)
		(end 153.903714 68.361661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.119643 114.545137)
		(end 203.192564 114.449473)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.919824 120.962904)
		(end 216.871982 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.558264 70.424549)
		(end 185.536218 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.425537 70.828059)
		(end 139.384111 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.416027 67.86523)
		(end 136.441212 67.86912)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.197635 26.25879)
		(end 143.234763 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.578134 68.613115)
		(end 185.595781 68.658863)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.870726 68.946399)
		(end 142.874333 68.897498)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.920143 31.941954)
		(end 202.916386 31.89205)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.441184 79.010451)
		(end 158.898667 78.996591)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.173493 68.705427)
		(end 157.188874 68.658868)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.345821 119.993831)
		(end 108.344617 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.458283 70.977226)
		(end 189.410441 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.02303 66.859602)
		(end 179.509572 67.085221)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.4645 118.227594)
		(end 199.505135 118.255742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.926478 118.399464)
		(end 145.437791 118.561278)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.463781 26.528074)
		(end 111.48795 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.968441 26.00481)
		(end 139.017106 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.851585 28.901828)
		(end 97.803807 28.889149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.173493 26.709005)
		(end 157.188874 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.535801 60.702485)
		(end 173.544415 60.726468)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.710424 118.136079)
		(end 97.756715 118.11874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.748384 61.249998)
		(end 173.967772 61.73938)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.119642 32.44765)
		(end 203.090303 32.407092)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.873895 68.114382)
		(end 111.917693 68.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.024887 86.266351)
		(end 214.830774 85.766405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.114866 65.292681)
		(end 166.510659 64.930778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.622532 76.289022)
		(end 199.656342 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.979146 66.297968)
		(end 119.425544 66.000724)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.226051 78.900508)
		(end 189.182253 78.878462)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.761232 63.198793)
		(end 214.052751 62.748635)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.048695 118.351739)
		(end 108.083001 118.387329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.719926 92.923449)
		(end 81.875199 93.436787)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.709034 94.507711)
		(end 214.719458 94.484457)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.102084 68.02636)
		(end 112.149926 68.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.958149 76.705427)
		(end 202.97353 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.837876 120.700243)
		(end 153.802364 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.445667 32.277364)
		(end 111.424993 32.231789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.462341 28.424491)
		(end 145.437857 28.431557)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.808079 83.79405)
		(end 174.51656 84.244208)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.149672 68.800526)
		(end 157.160416 68.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.089756 118.963941)
		(end 97.095856 118.914887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.209247 28.28317)
		(end 104.684097 28.174347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.94117 33.006631)
		(end 111.63825 32.564066)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.073707 53.003261)
		(end 82.064484 53.027016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.327072 26.403896)
		(end 157.357239 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.58702 78.737636)
		(end 199.549891 78.769663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.967081 26.043016)
		(end 217.013639 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.504495 82.880436)
		(end 175.488032 82.899887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 207.468297 79.35682)
		(end 207.443641 79.350382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.279735 28.856783)
		(end 189.234358 28.837176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.880335 26.852416)
		(end 142.888718 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.374214 68.026359)
		(end 153.421471 68.039437)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.897128 81.342197)
		(end 119.87706 81.326491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.727809 120.796248)
		(end 79.689154 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.182322 118.632285)
		(end 97.204714 118.588216)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.057262 68.481833)
		(end 203.083495 68.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.481958 118.072818)
		(end 107.530755 118.080714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.298839 78.552442)
		(end 157.272606 78.511016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.636815 70.953405)
		(end 107.589558 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.982893 76.007234)
		(end 158.031557 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.034848 120.99164)
		(end 97.985948 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.29664 64.092936)
		(end 167.63255 63.674857)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.149224 78.592529)
		(end 108.119058 78.631185)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.295802 67.997625)
		(end 112.344833 67.996421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.143264 76.658869)
		(end 97.160911 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.011652 68.481829)
		(end 143.037885 68.440403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.694352 32.407148)
		(end 139.665012 32.447706)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.945649 79.688057)
		(end 116.438634 79.513236)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.900236 89.587866)
		(end 172.893388 90.12413)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.937283 68.00723)
		(end 97.985948 68.001228)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.468167 120.916799)
		(end 93.42242 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.126104 120.874883)
		(end 185.082306 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.880941 78.631182)
		(end 188.850774 78.592526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.214575 58.523914)
		(end 127.218143 58.549146)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.561775 62.239966)
		(end 168.805864 61.762424)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.253229 78.552438)
		(end 97.226996 78.511012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.5355 118.227612)
		(end 97.577477 118.201509)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.664991 26.852416)
		(end 188.673374 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.634185 114.951958)
		(end 185.642916 115.001236)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.363446 54.639521)
		(end 127.26134 55.16602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.871686 26.328112)
		(end 153.903713 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.988347 70.51101)
		(end 153.962114 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.19258 114.449453)
		(end 203.207506 114.428798)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.034848 75.997625)
		(end 98.083879 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.119058 78.631185)
		(end 108.08703 78.668313)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.31909 95.014057)
		(end 128.578345 95.49082)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.915132 76.995434)
		(end 202.916336 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.458589 78.737637)
		(end 157.423077 78.703827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.659067 28.028921)
		(end 188.655401 27.979625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.192377 113.501875)
		(end 93.475637 113.964778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.216825 67.940039)
		(end 114.242175 67.93744)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.711062 120.766081)
		(end 111.673934 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.853977 28.927254)
		(end 198.804732 28.922959)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.424581 86.824004)
		(end 169.417203 86.799612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.610733 68.324529)
		(end 139.64276 68.361657)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.252823 70.920377)
		(end 139.207075 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.00017 66.848283)
		(end 179.023007 66.859591)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.347974 76.255212)
		(end 217.383486 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.966906 70.468347)
		(end 93.942737 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.421865 68.613121)
		(end 111.441735 68.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.343657 70.668309)
		(end 97.311629 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.533339 67.98109)
		(end 137.558789 67.982391)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34582 69.997409)
		(end 108.344617 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.129489 75.996422)
		(end 184.655166 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.572583 76.361663)
		(end 111.604611 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.553598 81.326475)
		(end 85.533531 81.342181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.384111 120.850714)
		(end 139.341448 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.576922 78.703821)
		(end 139.54141 78.737632)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.42993 28.02999)
		(end 192.896419 28.084687)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.065803 80.40721)
		(end 210.043573 80.394751)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.202827 26.528074)
		(end 97.226995 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.336185 126.992844)
		(end 223.663814 126.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.750094 120.420971)
		(end 188.730223 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.916998 118.387347)
		(end 188.951304 118.351758)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.334063 28.929108)
		(end 107.284665 28.927254)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.272606 76.481833)
		(end 157.298839 76.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.083612 31.892106)
		(end 94.079855 31.94201)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.280762 76.015617)
		(end 93.328604 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.975112 60.726492)
		(end 82.169225 61.226438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.332155 93.461037)
		(end 169.340153 93.436841)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.917693 78.900512)
		(end 111.873895 78.878466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.35197 83.338294)
		(end 129.037845 83.772979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.078609 67.764673)
		(end 90.103562 67.769844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.659068 118.963941)
		(end 188.665168 118.914887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.383486 26.2926)
		(end 217.417296 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.643019 53.003261)
		(end 173.633796 53.027016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.819504 26.001203)
		(end 143.868534 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.917693 26.095914)
		(end 111.96252 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.90432 76.848838)
		(end 199.910322 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.313508 26.168362)
		(end 143.354934 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.822541 70.552436)
		(end 188.796308 70.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.243246 120.734053)
		(end 203.207733 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.850074 70.977226)
		(end 184.801762 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.449703 118.155686)
		(end 143.49508 118.136079)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.289576 118.13606)
		(end 199.334953 118.155667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.149672 70.192317)
		(end 157.141289 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.040552 28.489194)
		(end 143.013914 28.447553)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.63307 70.287416)
		(end 217.617689 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.129273 26.949981)
		(end 154.130476 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.804733 118.069866)
		(end 198.853978 118.065571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.919943 76.897502)
		(end 202.925945 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.29765 78.900507)
		(end 139.252823 78.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.119058 76.361663)
		(end 108.149225 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.867657 118.387329)
		(end 153.900161 118.424571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.811125 120.330396)
		(end 139.793478 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.646147 76.752684)
		(end 217.656891 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.347974 70.737631)
		(end 217.310845 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.664991 76.848838)
		(end 188.673374 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.427151 87.365933)
		(end 127.31163 87.889651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.555259 78.991612)
		(end 189.506595 78.98561)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.890941 56.843181)
		(end 169.870399 56.307267)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.949824 118.145904)
		(end 106.995669 118.127385)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.479491 120.588947)
		(end 217.449324 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.575398 86.82401)
		(end 127.433286 87.341147)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.485816 76.440407)
		(end 185.512049 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.206127 78.953409)
		(end 199.158869 78.966487)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.718537 68.400317)
		(end 199.74677 68.440405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.026469 70.333974)
		(end 94.008822 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.002142 118.067345)
		(end 199.05127 118.072818)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.002803 58.549171)
		(end 173.091434 59.078105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.430858 66.848283)
		(end 87.453695 66.859591)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.253212 63.219846)
		(end 83.567337 63.654532)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.504536 64.112409)
		(end 175.861357 64.512791)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.649367 26.90108)
		(end 185.652974 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.826506 70.287416)
		(end 139.811125 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.129254 119.013218)
		(end 154.130477 119.062647)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.395388 76.324534)
		(end 185.427416 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.415411 51.490884)
		(end 158.029491 33.501944)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.222911 62.239971)
		(end 174.235085 62.262359)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.168767 68.138545)
		(end 185.210193 68.164778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.354934 68.138546)
		(end 143.397597 68.114378)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.634983 68.800521)
		(end 185.643366 68.848832)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.908574 59.078124)
		(end 123.997203 58.549191)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.995669 118.127385)
		(end 107.042363 118.111159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.719435 52.508419)
		(end 214.709011 52.485165)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.987483 26.528074)
		(end 143.011651 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.839583 26.756262)
		(end 139.850326 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.066119 120.588947)
		(end 143.037885 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.916337 120.042862)
		(end 202.915133 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.395839 26.001203)
		(end 107.444739 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.880216 81.683435)
		(end 211.46646 81.342213)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.70116 78.552436)
		(end 139.672927 78.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.534373 76.193017)
		(end 157.574462 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.772139 70.468347)
		(end 188.750093 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.903714 70.63118)
		(end 153.871686 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.080056 70.095341)
		(end 94.074054 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.397598 120.874883)
		(end 143.354934 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.681832 65.650646)
		(end 166.095588 65.309425)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.773948 26.095914)
		(end 107.817745 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.113259 78.966483)
		(end 139.065417 78.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.104062 76.800526)
		(end 97.114806 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.037884 26.443985)
		(end 143.066118 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.886739 76.026361)
		(end 157.934581 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.73448 28.84692)
		(end 152.623728 28.79896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.590502 85.230437)
		(end 214.346412 84.752894)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.030398 79.696981)
		(end 179.532972 79.897461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.893387 56.868691)
		(end 172.900238 57.404956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.316299 79.356815)
		(end 134.80102 79.505519)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.718852 66.585633)
		(end 132.741082 66.598092)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.801762 26.010812)
		(end 184.850073 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.869522 31.842064)
		(end 139.868268 31.892106)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.129273 70.04644)
		(end 154.125666 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.011047 26.571872)
		(end 203.033093 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.934582 120.973648)
		(end 157.88674 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.13168 70.04644)
		(end 157.130476 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.024058 32.185291)
		(end 94.005693 32.231845)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.397597 76.114382)
		(end 143.441395 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.658989 70.095341)
		(end 188.655382 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.76375 80.694877)
		(end 164.742185 80.681299)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.139381 118.962853)
		(end 195.672892 118.908156)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.92139 79.22817)
		(end 206.896437 79.222999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.792924 120.934446)
		(end 157.747176 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.014052 70.991611)
		(end 198.965151 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.018725 118.703854)
		(end 151.537633 118.568358)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.98937 118.588216)
		(end 143.013915 118.545308)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.880357 114.545193)
		(end 93.909696 114.585751)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.64276 76.361663)
		(end 139.672927 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.441736 120.420971)
		(end 111.421866 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.967081 76.039438)
		(end 217.013639 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.811125 70.333974)
		(end 139.793478 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.374214 70.966482)
		(end 153.326372 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.326312 28.126649)
		(end 108.315395 28.17486)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.816213 76.001232)
		(end 203.865114 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.653426 56.281784)
		(end 215.605546 55.747618)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.506595 68.00723)
		(end 189.55526 68.001228)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.963767 91.24525)
		(end 172.96669 91.270565)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.57008 88.468929)
		(end 215.566512 88.443697)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.786076 79.05281)
		(end 205.251341 79.011755)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.742164 80.681286)
		(end 164.281169 80.407222)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.671396 68.02636)
		(end 203.719238 68.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.751633 28.360576)
		(end 188.731448 28.315453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.903714 120.627602)
		(end 153.871687 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.17298 28.881684)
		(end 144.125542 28.895579)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.287423 76.658869)
		(end 108.302804 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.363184 26.043016)
		(end 189.410441 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.731925 62.748617)
		(end 129.023445 63.198775)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.240328 118.285884)
		(end 143.279521 118.25576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.767549 120.982031)
		(end 203.719238 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.086763 118.770352)
		(end 154.100052 118.817965)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.858392 93.989575)
		(end 128.065209 94.4844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.375861 68.039433)
		(end 93.42242 68.054814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.000768 88.468929)
		(end 123.9972 88.443697)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.888719 120.188739)
		(end 142.880336 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.381992 28.641104)
		(end 97.347686 28.605514)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.468167 68.07246)
		(end 93.512994 68.092331)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.100067 28.91211)
		(end 199.05127 28.920007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.882276 118.39114)
		(end 198.384659 118.203428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.119487 28.077956)
		(end 154.110968 28.126649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.041777 55.191203)
		(end 172.966687 55.722229)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.011047 78.424555)
		(end 202.991177 78.379728)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.207075 78.938024)
		(end 139.160517 78.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.558264 68.568288)
		(end 185.578134 68.613115)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.261349 91.826798)
		(end 127.363457 92.353296)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.869522 26.999012)
		(end 142.870726 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.991177 26.616699)
		(end 203.011047 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.569141 80.14456)
		(end 209.546304 80.133252)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.60416 75.997625)
		(end 189.653191 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.441873 120.464769)
		(end 79.419827 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.449669 114.545193)
		(end 185.479008 114.585751)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.13168 26.949981)
		(end 157.135287 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.347974 26.25879)
		(end 217.383486 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.493726 32.365126)
		(end 111.468597 32.321847)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.505135 118.255742)
		(end 199.544328 118.285865)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.139688 52.485142)
		(end 122.907875 52.001522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.670692 118.964807)
		(end 148.206299 118.992192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.726021 64.93076)
		(end 120.744383 64.913089)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.119058 120.627602)
		(end 108.087031 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.853872 28.529466)
		(end 188.825208 28.489194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.609381 32.137876)
		(end 185.59337 32.185291)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.298433 76.072466)
		(end 199.34326 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.305647 32.407092)
		(end 157.278382 32.365126)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.001481 67.940039)
		(end 160.026831 67.93744)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.669789 81.700162)
		(end 176.273996 82.062065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.751561 26.528074)
		(end 139.773607 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.238276 113.501863)
		(end 112.244788 113.490911)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.578134 120.376144)
		(end 185.558264 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.684117 26.756262)
		(end 188.697195 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.173923 68.324534)
		(end 203.207733 68.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.095855 28.077975)
		(end 97.089755 28.028921)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.965151 67.997623)
		(end 199.014052 68.001231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.206521 70.379722)
		(end 157.188874 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.148012 120.874883)
		(end 217.104214 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.668098 57.430467)
		(end 215.669074 57.405002)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.632526 83.318004)
		(end 167.296615 82.899924)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.903713 26.365241)
		(end 153.93388 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.054432 70.379722)
		(end 154.034562 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.334987 114.545137)
		(end 157.407908 114.449473)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.897916 70.966482)
		(end 184.850074 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.468029 78.938028)
		(end 153.421471 78.953409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.873895 78.878466)
		(end 111.831232 78.854298)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.719468 94.484434)
		(end 214.926282 93.989606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.673933 68.255211)
		(end 111.711062 68.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.582703 76.324534)
		(end 79.616513 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.495718 70.769659)
		(end 157.458589 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.282478 92.898852)
		(end 173.289231 92.923425)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.231086 65.986033)
		(end 165.661724 65.666384)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.817962 55.722252)
		(end 169.74287 55.191228)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.347024 68.946403)
		(end 111.350631 68.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.92792 120.330396)
		(end 142.91254 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.404218 70.333974)
		(end 111.388837 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.011651 26.485411)
		(end 143.037884 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.504582 92.923449)
		(end 127.659855 93.436787)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.363184 76.039438)
		(end 189.410441 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.458283 78.977227)
		(end 189.410441 78.966484)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.346823 118.561278)
		(end 197.858136 118.399463)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.942737 120.507432)
		(end 93.916505 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.066118 78.592526)
		(end 143.037885 78.552438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.44638 81.006811)
		(end 119.425536 80.99215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.492275 26.443985)
		(end 79.520508 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.495463 82.880434)
		(end 121.138642 82.480052)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.119783 65.309408)
		(end 85.533539 65.65063)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.612941 68.114378)
		(end 97.656739 68.092332)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.912969 70.668309)
		(end 188.880941 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.119664 78.14401)
		(end 154.111281 78.192321)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.463781 68.524496)
		(end 111.48795 68.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.658953 118.823033)
		(end 104.684031 118.818501)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.509595 67.085231)
		(end 179.53298 67.095358)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.773003 70.51101)
		(end 199.74677 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.054928 120.236581)
		(end 94.04185 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.615298 118.203428)
		(end 99.117682 118.39114)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.326625 120.188739)
		(end 108.315882 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.658551 76.114382)
		(end 157.702349 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.958149 70.287416)
		(end 202.945072 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.363008 95.490831)
		(end 174.369238 95.501948)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.997196 88.443672)
		(end 123.908565 87.914738)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.594648 28.815329)
		(end 153.550296 28.837157)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.066119 68.400314)
		(end 143.096285 68.361658)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.75576 28.916233)
		(end 198.707181 28.907093)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.341039 67.642467)
		(end 135.86324 67.764668)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.899522 65.292681)
		(end 212.295315 64.930778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.888718 26.804104)
		(end 142.899461 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.636241 28.901828)
		(end 143.588463 28.889149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.14174 115.00118)
		(end 157.15047 114.951902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.334213 84.730462)
		(end 214.066058 84.266006)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.988951 26.571872)
		(end 94.008821 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.243245 78.737637)
		(end 203.207733 78.703827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.288937 70.769659)
		(end 185.250282 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.653191 120.992844)
		(end 189.60416 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.901835 68.164782)
		(end 107.941924 68.193016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.772139 26.528074)
		(end 188.796307 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.114048 67.996258)
		(end 113.656564 67.982399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.2422 67.937437)
		(end 114.77414 67.869133)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.79035 114.761054)
		(end 139.808715 114.807608)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.166648 118.351758)
		(end 143.202673 118.317909)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.368628 79.127613)
		(end 206.343443 79.123723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.589558 70.966482)
		(end 107.541716 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.127883 70.287416)
		(end 97.114806 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.27219 76.193017)
		(end 217.310845 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.656342 78.668313)
		(end 199.622532 78.703825)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.081255 82.899905)
		(end 213.064791 82.880453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.057262 120.507432)
		(end 203.033094 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.082306 26.095914)
		(end 185.126103 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.863265 67.764673)
		(end 135.888218 67.769844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.356634 120.140427)
		(end 111.350632 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.269776 70.379722)
		(end 108.249906 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.675597 56.843181)
		(end 215.655055 56.307267)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.73189 84.24423)
		(end 128.718589 84.265967)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.799932 95.501959)
		(end 93.185852 113.490899)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.229395 78.991615)
		(end 153.180495 78.995222)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.928864 118.723474)
		(end 142.946793 118.677408)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.913929 68.946401)
		(end 199.915132 68.995432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.874304 79.350376)
		(end 115.352103 79.228175)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.301764 118.904907)
		(end 101.32704 118.908153)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.65896 79.350376)
		(end 161.136759 79.228175)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.550331 114.545137)
		(end 111.623252 114.449473)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.915132 27.930177)
		(end 199.913909 27.979606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.910322 76.897502)
		(end 199.913929 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.013639 120.934446)
		(end 216.967081 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.104062 68.800522)
		(end 97.114806 68.75268)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.915132 26.999012)
		(end 202.916336 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.674883 70.04644)
		(end 217.671276 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.06522 94.484424)
		(end 128.075644 94.507678)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.064503 93.965796)
		(end 82.073727 93.989551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.119058 68.361661)
		(end 108.149225 68.400317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.054432 68.613119)
		(end 154.072079 68.658867)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.58702 76.255212)
		(end 199.622532 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.888971 26.019195)
		(end 97.937282 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.665274 26.852416)
		(end 217.671276 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.353852 76.752684)
		(end 79.366929 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.64276 68.361657)
		(end 139.672927 68.400312)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.767898 26.168362)
		(end 79.809324 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.202827 68.524492)
		(end 97.226996 68.481829)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.421685 28.000651)
		(end 101.886077 28.028036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.643048 93.989575)
		(end 173.849865 94.4844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.204714 118.588216)
		(end 97.229259 118.545308)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.582778 83.318006)
		(end 83.567329 83.338273)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.119057 26.365241)
		(end 108.149224 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.017106 26.010812)
		(end 139.065417 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.03624 91.245248)
		(end 124.084117 90.711081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.913909 27.979606)
		(end 199.910243 28.028902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.118719 118.063717)
		(end 153.168148 118.064309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.514182 26.443985)
		(end 111.542416 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.354742 28.029988)
		(end 149.329333 28.028037)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.770603 26.00481)
		(end 143.819504 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.280761 78.977226)
		(end 93.23245 78.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.792266 70.703821)
		(end 93.756754 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.57009 58.523908)
		(end 215.631595 57.991139)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.542417 120.588947)
		(end 111.514183 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.323913 126.980596)
		(end 73.324183 126.991598)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.05322 76.289022)
		(end 108.08703 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.361578 120.700243)
		(end 185.326066 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.04185 120.283838)
		(end 94.026469 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.895188 118.227594)
		(end 107.935823 118.255742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.946779 120.700243)
		(end 188.912969 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.901835 70.828059)
		(end 107.860409 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.23245 120.982031)
		(end 93.183786 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.128313 76.324534)
		(end 143.162123 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.177512 63.219843)
		(end 122.191906 63.198814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.27806 78.985613)
		(end 153.229395 78.991615)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.026795 79.055411)
		(end 160.001445 79.052812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.065418 70.977226)
		(end 139.017106 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.624239 78.240159)
		(end 185.611162 78.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.963636 79.897471)
		(end 87.940251 79.907598)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.817746 76.114382)
		(end 107.860409 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.096285 76.361663)
		(end 143.128313 76.324534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.175273 32.13782)
		(end 157.161657 32.089663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.168147 28.928516)
		(end 153.118719 28.929108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.652975 68.946397)
		(end 185.654179 68.995428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.096624 28.929126)
		(end 98.047195 28.928534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.747314 76.054819)
		(end 97.793872 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.465626 120.796248)
		(end 139.425537 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.90432 78.14401)
		(end 199.895937 78.192321)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.438667 67.47962)
		(end 116.945682 67.3048)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.652975 120.042862)
		(end 185.649368 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.878827 64.531414)
		(end 176.255625 64.913054)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.85816 118.399455)
		(end 197.882252 118.391149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.926292 93.989582)
		(end 214.935515 93.965827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.54137 28.874121)
		(end 143.495079 28.856783)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.384111 76.138551)
		(end 139.425537 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.441873 26.528074)
		(end 79.466042 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.719237 26.019195)
		(end 203.767549 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.01942 70.769659)
		(end 188.982291 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.351375 59.651672)
		(end 215.357498 59.626935)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.808715 114.807608)
		(end 139.824726 114.855023)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.034848 67.997621)
		(end 98.083879 67.996417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.969545 79.696985)
		(end 116.945673 79.688065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.541716 68.015616)
		(end 107.589558 68.026359)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.341029 118.823037)
		(end 192.871051 118.904904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.22786 120.464769)
		(end 108.203692 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.768174 27.999999)
		(end 148.231867 27.999999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.182253 78.878462)
		(end 189.13959 78.854294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.383486 120.700243)
		(end 217.347974 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.209231 118.709667)
		(end 105.234044 118.70386)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.988347 26.485411)
		(end 154.012515 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.793658 118.992192)
		(end 149.329266 118.964807)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.229396 76.001232)
		(end 153.27806 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.230324 114.715423)
		(end 157.253254 114.67094)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.839583 76.752684)
		(end 139.850327 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.826505 26.709005)
		(end 139.839583 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.359118 68.164783)
		(end 203.400544 68.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.317934 79.011748)
		(end 182.7832 79.052801)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.141739 31.991607)
		(end 157.135487 31.941954)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.490404 79.907612)
		(end 117.467019 79.897485)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.792923 26.058397)
		(end 157.839482 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.889031 118.866194)
		(end 142.899948 118.817983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.183786 68.001227)
		(end 93.23245 68.007229)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.615888 70.854292)
		(end 157.574462 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.937713 89.001729)
		(end 172.935438 89.027111)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.033306 55.722252)
		(end 123.958214 55.191228)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.356633 76.848838)
		(end 111.365016 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.747176 26.076044)
		(end 157.792923 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.800996 79.505526)
		(end 134.7767 79.513215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.468167 78.920377)
		(end 93.422419 78.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.125666 76.897502)
		(end 154.129273 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.753097 26.00481)
		(end 184.801762 26.010812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.102083 70.966482)
		(end 112.054826 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.173922 78.668314)
		(end 203.141895 78.631186)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.646147 120.236581)
		(end 217.63307 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.96252 26.076044)
		(end 112.008267 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.770604 68.001228)
		(end 143.819504 67.997621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.645065 26.142129)
		(end 153.686491 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.013639 26.058397)
		(end 217.059387 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.58702 70.737631)
		(end 199.549891 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.479008 32.407148)
		(end 185.449668 32.447706)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.473179 66.311557)
		(end 86.934174 66.585621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.865114 70.995218)
		(end 203.816213 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.886739 78.966488)
		(end 157.839482 78.95341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.531271 118.818501)
		(end 146.556348 118.823033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.654179 119.993831)
		(end 185.652975 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.610732 70.668309)
		(end 139.576922 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.280762 68.015612)
		(end 93.328604 68.026355)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.346431 62.239966)
		(end 214.59052 61.762424)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.412979 68.255207)
		(end 97.450108 68.22318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.904439 65.309408)
		(end 131.318195 65.65063)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.683373 26.058397)
		(end 107.729121 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.569195 66.848287)
		(end 210.043581 66.59812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.516546 84.24423)
		(end 174.503245 84.265967)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.177458 76.440407)
		(end 108.203691 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.207075 70.938024)
		(end 139.160517 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.100067 118.080714)
		(end 199.148414 118.091015)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.839482 78.95341)
		(end 157.792923 78.938029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.600042 26.616699)
		(end 217.617689 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.962115 120.548858)
		(end 153.933881 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.429721 70.854292)
		(end 199.387058 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.988952 70.424549)
		(end 93.966906 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.073504 118.399455)
		(end 152.097596 118.391149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.903718 59.103167)
		(end 123.90857 59.07815)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.083001 118.387329)
		(end 108.115505 118.424571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.665013 114.545193)
		(end 139.694352 114.585751)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.860409 26.142129)
		(end 107.901835 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.595781 70.333974)
		(end 185.578134 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.654179 119.993831)
		(end 188.654179 119.062666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.701161 120.548858)
		(end 139.672927 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.529012 82.079771)
		(end 166.510651 82.0621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.67284 79.222988)
		(end 181.647887 79.228159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.111815 67.769855)
		(end 161.136768 67.764684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.831852 118.064327)
		(end 143.88128 118.063735)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.20965 114.760998)
		(end 157.230324 114.715423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.875206 93.436812)
		(end 81.883205 93.461007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.903714 76.361663)
		(end 153.933881 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.697893 118.770371)
		(end 188.71352 118.723474)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.945071 26.756262)
		(end 202.958149 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.100537 70.240159)
		(end 154.08746 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.689154 70.769659)
		(end 79.652025 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.231841 28)
		(end 148.206366 28.00065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.236249 66.297966)
		(end 132.257814 66.311544)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.712576 120.330396)
		(end 188.697196 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34582 77.997414)
		(end 108.344617 78.046444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.570278 68.138546)
		(end 97.612941 68.114378)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.793674 28.00065)
		(end 148.768199 28)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.673374 26.804104)
		(end 188.684117 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.016497 28)
		(end 193.991022 28.00065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.366929 26.709005)
		(end 79.38231 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.584284 54.614611)
		(end 81.578795 54.639496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.885951 78.996585)
		(end 183.343435 79.010444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.856735 68.658867)
		(end 199.872116 68.705426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.387058 78.878465)
		(end 199.34326 78.900511)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.910198 118.097282)
		(end 189.957637 118.111178)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.367434 83.318006)
		(end 129.351985 83.338273)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.207733 76.289022)
		(end 203.243245 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.243284 28.874103)
		(end 199.196192 28.88913)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.361791 32.564066)
		(end 185.05887 33.006632)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.655402 119.013237)
		(end 188.659068 118.963941)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.888271 120.588947)
		(end 93.858104 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.327159 67.769855)
		(end 115.352112 67.764684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.01942 120.766081)
		(end 188.982292 120.734053)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.652025 70.737631)
		(end 79.616513 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.846403 92.378232)
		(end 123.851892 92.353347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.913929 26.949981)
		(end 199.915132 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.033094 120.464769)
		(end 203.011048 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.578528 78.953406)
		(end 143.531969 78.938025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.52432 113.964778)
		(end 203.807581 113.501874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.354934 76.138551)
		(end 143.397597 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.065417 78.977226)
		(end 139.017106 78.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.763802 66.297968)
		(end 165.2102 66.000724)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.912539 78.287417)
		(end 142.899462 78.24016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.494864 28.737101)
		(end 97.455671 28.706978)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.888718 68.800522)
		(end 142.899462 68.75268)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.966978 118.632285)
		(end 142.98937 118.588216)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.083879 120.992844)
		(end 98.034848 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.103622 28.084687)
		(end 103.570111 28.02999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.252685 76.054819)
		(end 199.298433 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.251377 67.981095)
		(end 205.786111 67.940042)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.822541 76.440407)
		(end 188.850774 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.652975 70.04644)
		(end 185.649368 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.457583 70.592525)
		(end 185.427416 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.778559 28.28317)
		(end 196.253409 28.174347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.101295 78.996585)
		(end 137.558779 79.010444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.988347 76.481833)
		(end 154.012516 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.27806 76.007234)
		(end 153.326372 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.223323 67.47962)
		(end 162.730338 67.3048)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.377002 114.903124)
		(end 111.390618 114.854967)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.098164 68.164779)
		(end 189.13959 68.138546)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.514183 68.440407)
		(end 111.542416 68.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.507724 70.552436)
		(end 217.479491 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.549891 70.769659)
		(end 199.511236 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.091438 59.07813)
		(end 173.09629 59.103148)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.781852 88.443672)
		(end 169.693221 87.914738)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.773003 76.481833)
		(end 199.797172 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.946779 70.703821)
		(end 188.912969 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.817746 70.878461)
		(end 107.773948 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.065671 68.800521)
		(end 94.074054 68.848832)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.649368 68.897497)
		(end 185.652975 68.946397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.449668 32.447706)
		(end 185.376747 32.54337)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178.52576 66.598104)
		(end 179.000147 66.848272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.549589 62.262376)
		(end 168.561763 62.239989)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.05322 78.703825)
		(end 108.017708 78.737636)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.108731 56.868691)
		(end 127.115582 57.404956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.485038 67.304786)
		(end 88.992053 67.479607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.622997 32.089719)
		(end 185.609381 32.137876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.616513 26.2926)
		(end 79.652025 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.986084 28.447535)
		(end 153.959447 28.489176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.074054 78.144005)
		(end 94.065671 78.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.765235 78.769663)
		(end 153.72658 78.79983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.374214 76.026361)
		(end 153.421471 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.130476 69.997409)
		(end 157.130476 68.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.602402 78.878465)
		(end 153.558604 78.900511)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.399957 120.376144)
		(end 79.38231 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.347024 70.04644)
		(end 111.34582 69.997409)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.997207 58.549166)
		(end 124.000775 58.523933)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.965151 78.995222)
		(end 198.91612 78.996426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.652975 76.946403)
		(end 185.654179 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.450442 62.262381)
		(end 128.718597 62.726837)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.611162 120.283838)
		(end 185.595781 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.91612 26)
		(end 198.965151 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.347974 120.734053)
		(end 217.310845 120.766081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.095679 68.848833)
		(end 97.104062 68.800522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.677685 28.424491)
		(end 99.653201 28.431557)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.538857 79.696985)
		(end 208.514985 79.688065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.134885 70.995218)
		(end 93.085854 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.05322 26.2926)
		(end 108.08703 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.761689 113.501875)
		(end 185.044949 113.964778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.652025 76.255212)
		(end 79.689154 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.198946 79.505532)
		(end 161.683666 79.356827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.110968 28.126649)
		(end 154.100051 28.17486)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.281389 84.265984)
		(end 168.268088 84.244248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.08607 78.046442)
		(end 97.084867 77.997411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.344833 26)
		(end 138.87051 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.531969 26.058397)
		(end 143.578528 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.377001 32.089663)
		(end 111.365814 32.040885)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.19192 63.198793)
		(end 122.483439 62.748635)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.130476 26.999012)
		(end 154.130476 27.930177)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.910198 28.895579)
		(end 189.86213 28.907111)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.671276 70.095341)
		(end 217.665274 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.611674 28.881665)
		(end 198.564981 28.86544)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.248438 120.464769)
		(end 157.226392 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.746746 114.670996)
		(end 139.769676 114.715479)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.130476 76.995434)
		(end 154.130476 77.997414)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.340161 93.436817)
		(end 169.495431 92.923477)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.649168 115.050889)
		(end 185.652925 115.100793)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.318167 81.342197)
		(end 130.904411 81.683418)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.65319 78.996423)
		(end 189.60416 78.99522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.633869 89.027131)
		(end 215.631594 89.001749)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.993887 118.709667)
		(end 151.0187 118.70386)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.269776 26.616699)
		(end 108.287423 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.206521 26.616699)
		(end 157.226391 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.533957 120.507432)
		(end 217.507724 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.089677 76.897502)
		(end 97.095679 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.207733 26.2926)
		(end 203.243245 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.376731 32.54339)
		(end 185.361805 32.564045)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.130476 69.997409)
		(end 154.129273 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.344833 67.996421)
		(end 113.101279 67.996421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.578528 68.039434)
		(end 143.625786 68.026356)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.141895 78.631186)
		(end 203.111728 78.592531)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.839583 68.752679)
		(end 139.850327 68.800521)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.623705 28.79895)
		(end 152.600069 28.789424)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.130476 26.999012)
		(end 157.13168 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.121216 64.531413)
		(end 121.138651 64.512827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.914145 75.996422)
		(end 216.677074 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.868269 115.100793)
		(end 139.869523 115.150835)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.137869 28.907093)
		(end 107.089801 28.895561)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.826506 120.283838)
		(end 139.811125 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.083663 78.04644)
		(end 94.080056 78.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.047195 28.928534)
		(end 97.997857 28.925498)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.704711 64.930761)
		(end 85.100505 65.292664)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.046005 91.826798)
		(end 173.148113 92.353296)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.977033 113.501875)
		(end 139.260293 113.964778)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.122959 65.666367)
		(end 177.553599 65.986017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.408343 118.193883)
		(end 198.519136 118.145904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.365814 32.040885)
		(end 111.357083 31.991607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.374213 78.966487)
		(end 153.326371 78.97723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.071135 118.723456)
		(end 154.086763 118.770352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.729121 70.920377)
		(end 107.683373 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.726105 120.99164)
		(end 216.677074 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.975016 118.285865)
		(end 108.012671 118.31789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.917693 68.092336)
		(end 111.96252 68.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.356633 68.848838)
		(end 111.365016 68.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.334245 62.262376)
		(end 214.346419 62.239989)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.833351 28.641085)
		(end 153.797326 28.674934)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.311625 87.889676)
		(end 127.306773 87.914693)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.302804 70.287416)
		(end 108.287423 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.146789 118.201509)
		(end 189.190007 118.177514)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.43283 118.067345)
		(end 107.481958 118.072818)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.871686 76.324534)
		(end 153.903714 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.290965 52.485132)
		(end 82.280541 52.508386)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.326625 68.800525)
		(end 108.335008 68.848836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.880335 68.848833)
		(end 142.888718 68.800522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.731448 28.315453)
		(end 188.71352 28.269387)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.915132 69.997409)
		(end 202.915132 68.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.610732 26.328112)
		(end 139.642759 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.255896 28.489194)
		(end 97.229258 28.447553)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.536217 26.528074)
		(end 185.558263 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.020077 118.069866)
		(end 153.069322 118.065571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.853873 118.463395)
		(end 188.884495 118.42459)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.625785 76.026361)
		(end 143.673627 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.528852 68.164779)
		(end 97.570278 68.138546)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.008822 76.613121)
		(end 94.026469 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.793478 76.613121)
		(end 139.811125 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.631311 79.127607)
		(end 90.103553 79.222983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.014979 32.277364)
		(end 202.994305 32.231789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.647921 67.764673)
		(end 181.672874 67.769844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.130477 119.993831)
		(end 157.130477 115.150779)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.09976 89.587862)
		(end 124.098784 89.562397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.429721 68.138549)
		(end 199.471147 68.164782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.22786 78.468351)
		(end 108.203691 78.511014)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.873895 70.878461)
		(end 111.831232 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.715438 28.529448)
		(end 199.684816 28.568253)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.727393 70.51101)
		(end 139.70116 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.721939 68.00723)
		(end 143.770604 68.001228)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.062716 70.985609)
		(end 199.014052 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.850073 78.977226)
		(end 184.801762 78.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.826076 70.668309)
		(end 93.792266 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.580172 120.420971)
		(end 217.558126 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.893714 90.149662)
		(end 172.914256 90.685576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.870726 76.946403)
		(end 142.874333 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.404218 26.662447)
		(end 111.421865 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.654178 26.999012)
		(end 185.654178 31.842064)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.966905 26.528074)
		(end 93.988951 26.571872)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.27219 70.799826)
		(end 217.232101 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.326625 78.192321)
		(end 108.315881 78.240163)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.211807 87.365933)
		(end 173.096286 87.889651)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.669072 89.587862)
		(end 215.668096 89.562397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.704197 120.99164)
		(end 184.655166 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.819504 78.99522)
		(end 143.770603 78.991612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.916121 120.992844)
		(end 189.653191 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.817746 120.874883)
		(end 107.773948 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.005122 80.992133)
		(end 85.984278 81.006795)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.904144 118.914868)
		(end 199.910244 118.963922)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.519136 118.145904)
		(end 198.564981 118.127385)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.578316 51.501987)
		(end 128.319064 51.97875)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.550675 70.63118)
		(end 79.520508 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34101 76.897502)
		(end 108.344617 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.280374 76.223184)
		(end 203.319029 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.646147 70.240159)
		(end 217.63307 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.096295 59.103173)
		(end 173.211818 59.626891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.562184 28.431557)
		(end 151.537699 28.424491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.408361 28.79895)
		(end 198.384725 28.789424)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.054293 79.688052)
		(end 180.030422 79.696971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.026469 120.330396)
		(end 94.008822 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.162123 120.700243)
		(end 143.128313 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.665274 70.144005)
		(end 217.656891 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.410441 76.026361)
		(end 189.458283 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.138668 64.512808)
		(end 121.495487 64.112426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.182321 28.360576)
		(end 97.162136 28.315453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.383486 70.703821)
		(end 217.347974 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.726105 75.997625)
		(end 216.775006 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.202673 118.317909)
		(end 143.240328 118.285884)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.069321 28.927254)
		(end 153.020076 28.922959)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.128907 118.904904)
		(end 104.658928 118.823037)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.916504 76.440407)
		(end 93.942737 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.748292 79.897471)
		(end 133.724907 79.907598)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.816214 120.988033)
		(end 203.767549 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.149925 70.977226)
		(end 112.102083 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.789806 78.828065)
		(end 111.749717 78.799831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.180495 67.997623)
		(end 153.229396 68.001231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.176329 26.010812)
		(end 80.224993 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.634983 78.192317)
		(end 185.624239 78.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.895937 70.192317)
		(end 199.885193 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.784539 66.848287)
		(end 164.258925 66.59812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.287423 70.333974)
		(end 108.269776 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.361578 68.289016)
		(end 185.395389 68.324529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.37576 70.240159)
		(end 111.365016 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.82367 76.007234)
		(end 216.871982 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.376312 28.79896)
		(end 144.265519 28.846939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.589558 120.962904)
		(end 107.541716 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.278382 32.365126)
		(end 157.253253 32.321847)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.99202 79.513223)
		(end 88.485005 79.688043)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.017708 76.255212)
		(end 108.05322 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.080458 70.995218)
		(end 158.031557 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.48795 78.511016)
		(end 111.463781 78.468352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.544328 118.285865)
		(end 199.581983 118.31789)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.756714 28.874121)
		(end 97.710423 28.856783)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.012516 78.468351)
		(end 153.988347 78.511014)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.182037 91.270591)
		(end 127.257129 91.801615)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.441395 26.095914)
		(end 143.486221 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.681784 81.342197)
		(end 165.661716 81.326491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.384111 70.854292)
		(end 139.341448 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.310951 65.309408)
		(end 120.330191 65.292698)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.74677 26.443985)
		(end 199.773003 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.323913 69.997409)
		(end 79.323913 26.999012)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.495718 76.223184)
		(end 157.534373 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.991732 68.054814)
		(end 185.037479 68.07246)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.365016 26.804104)
		(end 111.375759 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.578133 26.616699)
		(end 185.59578 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.34326 76.092336)
		(end 199.387058 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.773948 120.896929)
		(end 107.729122 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34582 27.930177)
		(end 108.344597 27.979606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.210221 66.00071)
		(end 165.231065 65.986048)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.897916 68.026355)
		(end 184.945173 68.039433)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.850073 26.019195)
		(end 184.897915 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.458589 68.255211)
		(end 157.495718 68.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.997857 118.067363)
		(end 98.047196 118.064327)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.395388 26.328112)
		(end 185.427415 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.87051 70.996422)
		(end 125.608387 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.689048 81.683435)
		(end 176.669808 81.700145)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.549557 84.730462)
		(end 168.281402 84.266006)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.137869 118.085732)
		(end 107.186449 118.076592)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.945173 68.039433)
		(end 184.991732 68.054814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.387058 76.114382)
		(end 199.429721 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.036232 55.747593)
		(end 124.033309 55.722278)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.984307 65.986032)
		(end 86.005151 66.000693)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.68097 70.799826)
		(end 93.640881 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.966466 86.290364)
		(end 81.798135 86.79957)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 207.983659 67.487317)
		(end 208.007955 67.479628)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.423077 78.703827)
		(end 157.389266 78.668314)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.23245 78.985609)
		(end 93.183785 78.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.652925 115.100793)
		(end 185.654179 115.150835)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.870398 56.307241)
		(end 169.868772 56.28181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.468597 32.321847)
		(end 111.445667 32.277364)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.816213 26.00481)
		(end 203.865114 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.690528 64.531413)
		(end 212.707963 64.512827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.934143 80.407207)
		(end 86.473149 80.68127)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.966684 55.722254)
		(end 172.963762 55.747569)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.556792 68.114377)
		(end 93.599455 68.138545)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.397597 26.11796)
		(end 143.441395 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.034848 26.001203)
		(end 98.083878 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.036363 67.095372)
		(end 209.059748 67.085245)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.727809 76.193017)
		(end 79.767898 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.298433 68.072465)
		(end 199.34326 68.092335)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.11326 76.026361)
		(end 139.160517 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.910322 78.095345)
		(end 199.90432 78.14401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.326371 26.019195)
		(end 153.374213 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.331901 89.562376)
		(end 81.330925 89.587841)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.465626 70.799826)
		(end 139.425537 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.366124 89.027136)
		(end 81.331902 89.562351)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.383492 118.064309)
		(end 107.43283 118.067345)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.850327 70.192317)
		(end 139.839583 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.298839 120.548858)
		(end 157.272606 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.080458 120.99164)
		(end 158.031558 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.897916 120.962904)
		(end 184.850074 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.065418 76.015617)
		(end 139.11326 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.767549 76.007234)
		(end 203.816213 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.811512 67.937437)
		(end 206.343452 67.869133)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.673933 70.737631)
		(end 111.638421 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.135288 120.091763)
		(end 157.131681 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.125695 67.642467)
		(end 181.647896 67.764668)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.128313 70.668309)
		(end 143.096285 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.111281 78.192321)
		(end 154.100537 78.240163)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.131464 70.996422)
		(end 143.868535 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.458589 70.737631)
		(end 157.423077 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.429721 76.138551)
		(end 199.471147 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.340931 28.028902)
		(end 108.334831 28.077956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.63307 120.283838)
		(end 217.617689 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.375759 26.756262)
		(end 111.388837 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.343108 70.192317)
		(end 79.334725 70.144005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.994305 32.231789)
		(end 202.97594 32.185235)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.977067 33.49098)
		(end 138.970555 33.501932)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.280374 70.769659)
		(end 203.243245 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.054927 78.240159)
		(end 94.04185 78.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.015742 65.986033)
		(end 211.44638 65.666384)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.865114 67.997625)
		(end 203.914145 67.996421)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.941924 76.193017)
		(end 107.980579 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.915133 119.062647)
		(end 199.915133 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.839031 118.193883)
		(end 106.949824 118.145904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.869523 77.997411)
		(end 142.869523 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.250282 68.193012)
		(end 185.288937 68.223179)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.741051 80.394736)
		(end 132.718821 80.407194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.579102 118.091015)
		(end 107.62688 118.103694)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.860618 28.02999)
		(end 101.327107 28.084687)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.962114 26.443985)
		(end 153.988347 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.97654 83.794047)
		(end 167.962146 83.773018)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.323913 26.999012)
		(end 79.325116 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.535778 86.290364)
		(end 173.367447 86.79957)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.017708 70.737631)
		(end 107.980579 70.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.084867 68.995429)
		(end 97.08607 68.946399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.851987 70.878461)
		(end 79.809324 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.965438 120.420971)
		(end 142.945567 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.305647 114.585695)
		(end 157.334987 114.545137)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.135287 76.897502)
		(end 157.141289 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.912539 68.705423)
		(end 142.92792 68.658864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.443207 70.878461)
		(end 203.400544 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.316358 67.636023)
		(end 135.341014 67.642461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.160415 26.756262)
		(end 157.173493 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.617689 120.330396)
		(end 217.600042 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.665046 28.837176)
		(end 97.620694 28.815348)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.359118 120.824481)
		(end 203.319029 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.100524 65.292681)
		(end 85.119763 65.309391)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.969601 67.295862)
		(end 117.467027 67.095382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.423077 68.289022)
		(end 157.458589 68.255211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.072079 78.333979)
		(end 154.054432 78.379727)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.952804 118.064309)
		(end 199.002142 118.067345)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.915133 119.993831)
		(end 199.913929 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.595781 78.333975)
		(end 185.578134 78.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.801762 68.007229)
		(end 184.850074 68.015612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.721617 114.627717)
		(end 139.746746 114.670996)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.871419 118.770352)
		(end 199.884708 118.817965)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.746745 32.321903)
		(end 139.721617 32.365182)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.684072 28.174342)
		(end 104.658995 28.16981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.580172 26.571872)
		(end 217.600042 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.916336 76.946403)
		(end 202.919943 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.885133 81.700162)
		(end 130.48934 82.062065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.35724 120.627602)
		(end 157.327073 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.536218 78.468347)
		(end 185.512049 78.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.797326 28.674934)
		(end 153.759671 28.706959)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.940228 79.907608)
		(end 87.453687 80.133226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.354934 78.854294)
		(end 143.313508 78.828061)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.08703 70.668309)
		(end 108.05322 70.703821)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.855791 118.723456)
		(end 199.871419 118.770352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.934581 78.977231)
		(end 157.886739 78.966488)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.710423 28.856783)
		(end 97.665046 28.837176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.375861 70.953405)
		(end 93.328604 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.713166 92.898852)
		(end 81.719919 92.923425)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.570278 78.854294)
		(end 97.528852 78.828061)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.514183 120.548858)
		(end 111.48795 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.59578 26.662447)
		(end 185.611161 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.423077 76.289022)
		(end 157.458589 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.765235 70.769659)
		(end 153.72658 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.81355 28.916251)
		(end 189.764578 28.922977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.109058 90.149662)
		(end 127.1296 90.685576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.757799 79.055406)
		(end 182.225859 79.12371)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.535499 28.765249)
		(end 97.494864 28.737101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.677668 118.568359)
		(end 100.196577 118.703854)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.366929 70.287416)
		(end 79.353852 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.85826 115.001236)
		(end 139.864512 115.050889)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.738547 61.226462)
		(end 173.748374 61.249974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.982893 78.985614)
		(end 157.934581 78.977231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.926396 115.00118)
		(end 202.935126 114.951902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178.042491 66.311557)
		(end 178.503486 66.585621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.811125 76.658869)
		(end 139.826506 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.072079 70.333974)
		(end 154.054432 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.395839 75.997625)
		(end 107.44474 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.207076 68.054814)
		(end 139.252823 68.07246)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.966489 60.702485)
		(end 81.975103 60.726468)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.873896 120.874883)
		(end 111.831232 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.789806 120.824481)
		(end 111.749717 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.05127 28.920007)
		(end 199.002142 28.92548)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.074054 70.144005)
		(end 94.065671 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.673686 28.126667)
		(end 188.665167 28.077975)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.915132 76.995434)
		(end 199.915132 77.997414)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.446401 65.666368)
		(end 211.466468 65.650662)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.742878 91.80164)
		(end 169.817968 91.270614)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.419827 76.568294)
		(end 79.441873 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.272606 26.485411)
		(end 157.298838 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.316626 68.054815)
		(end 189.363184 68.039434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.542416 78.592531)
		(end 111.514183 78.552442)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.555259 76.001232)
		(end 189.60416 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.29765 26.095914)
		(end 139.341447 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.465626 76.193017)
		(end 139.504281 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.00142 79.05281)
		(end 159.466685 79.011755)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.384683 118.203419)
		(end 198.408319 118.193893)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.55639 28.16981)
		(end 146.531312 28.174342)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.874411 28.028921)
		(end 142.870745 27.979625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.645274 28.02999)
		(end 147.111763 28.084687)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.873895 26.11796)
		(end 111.917693 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.542416 26.403896)
		(end 111.572583 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.34582 77.997415)
		(end 111.34582 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.131465 67.99642)
		(end 153.180495 67.997623)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.196192 118.103694)
		(end 199.243285 118.118722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.850774 76.400318)
		(end 188.880941 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.162123 78.703823)
		(end 143.128312 78.66831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.959447 28.489176)
		(end 153.930782 28.529448)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.179111 91.24525)
		(end 127.182034 91.270565)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.131731 115.100737)
		(end 157.135488 115.050833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.125542 28.895579)
		(end 144.077474 28.907111)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.718576 84.265989)
		(end 128.450422 84.730444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.98636 26.058397)
		(end 80.032918 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.493726 114.627661)
		(end 111.520991 114.585695)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.216764 79.05281)
		(end 113.682029 79.011755)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.556792 70.878461)
		(end 93.512994 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.888718 78.192318)
		(end 142.880335 78.144007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.326372 120.973648)
		(end 153.278061 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.160516 26.043016)
		(end 139.207075 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.634185 32.040941)
		(end 185.622997 32.089719)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.513777 68.072465)
		(end 153.558604 68.092335)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.915133 119.993831)
		(end 202.915133 115.150779)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.770603 70.991611)
		(end 143.721939 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.86213 118.08575)
		(end 189.910198 118.097282)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.098783 89.562372)
		(end 124.064559 89.027156)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.534373 26.196595)
		(end 157.574462 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.269637 79.688052)
		(end 134.245766 79.696971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.858103 26.365241)
		(end 93.88827 26.403896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.38231 70.333974)
		(end 79.366929 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.131224 56.281787)
		(end 127.129598 56.307219)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.841129 76.026361)
		(end 97.888971 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.858259 31.991663)
		(end 139.849529 32.040941)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.782513 118.067363)
		(end 143.831852 118.064327)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.684118 76.752684)
		(end 188.697195 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.91612 70.996422)
		(end 189.653191 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.311629 78.631182)
		(end 97.281462 78.592526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.354934 70.854292)
		(end 143.313508 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.655167 67.996416)
		(end 184.704197 67.997619)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.441246 67.982398)
		(end 159.466696 67.981097)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.323913 119.993831)
		(end 79.323913 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.334832 118.914868)
		(end 108.340932 118.963922)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.555505 93.436817)
		(end 123.710775 92.923477)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.916504 70.552436)
		(end 93.888271 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.622532 68.28902)
		(end 199.656343 68.324533)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.583972 79.127613)
		(end 160.558787 79.123723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.865114 120.99164)
		(end 203.816214 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.032918 70.953405)
		(end 79.98636 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.280762 120.973648)
		(end 93.23245 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.03791 114.67094)
		(end 203.063038 114.627661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.512049 78.51101)
		(end 185.485816 78.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.701566 78.920378)
		(end 97.656739 78.900508)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.658552 120.874883)
		(end 157.615888 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.083879 70.996422)
		(end 98.034848 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.487005 26.095914)
		(end 203.531832 26.076044)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.225833 79.123713)
		(end 182.200649 79.127603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.27806 70.985609)
		(end 153.229396 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.34101 120.091763)
		(end 108.335008 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.839482 70.953405)
		(end 157.792924 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.160517 78.953405)
		(end 139.113259 78.966483)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.119058 70.63118)
		(end 108.08703 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.343409 79.010445)
		(end 183.317959 79.011746)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.955037 33.028043)
		(end 111.941184 33.006652)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.558604 68.092335)
		(end 153.602402 68.114381)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.624138 70.953405)
		(end 203.57758 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.776676 79.513223)
		(end 134.269661 79.688043)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.935822 28.737083)
		(end 107.895187 28.765231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.790349 32.231845)
		(end 139.769675 32.27742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.65659 67.982398)
		(end 113.68204 67.981097)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.11128 26.804104)
		(end 154.119663 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.344617 68.946401)
		(end 108.34582 68.995432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.341447 26.11796)
		(end 139.384111 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.319029 26.196595)
		(end 203.359118 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.76564 28.837157)
		(end 107.720263 28.856764)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.933881 68.400317)
		(end 153.962114 68.440405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.897916 76.026361)
		(end 184.945173 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.173923 76.324534)
		(end 203.207733 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.68837 120.627602)
		(end 199.656343 120.664731)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.168767 70.854292)
		(end 185.126104 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.617689 76.658869)
		(end 217.63307 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.973531 120.330396)
		(end 202.95815 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.885193 26.756262)
		(end 199.895936 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.665012 32.447706)
		(end 139.592091 32.54337)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.104062 78.192318)
		(end 97.095679 78.144007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.388837 78.287422)
		(end 111.37576 78.240164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.492275 76.440407)
		(end 79.520508 76.400318)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.106612 90.124152)
		(end 124.099761 89.587887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.268551 118.67739)
		(end 108.286479 118.723456)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.421683 95.490856)
		(end 168.680935 95.014093)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.684817 118.424571)
		(end 199.715439 118.463377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.692556 94.991356)
		(end 168.924367 94.507734)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.42242 68.054814)
		(end 93.468167 68.07246)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.880941 68.361658)
		(end 188.912969 68.32453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.512994 68.092331)
		(end 93.556792 68.114377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.811124 26.662447)
		(end 139.826505 26.709005)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.747176 78.920383)
		(end 157.702349 78.900512)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.533278 79.011748)
		(end 136.998544 79.052801)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.91612 78.996426)
		(end 189.65319 78.996423)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.749717 68.193017)
		(end 111.789806 68.164783)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.846935 89.001724)
		(end 169.785428 88.468954)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.366184 53.027047)
		(end 123.35696 53.003292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.659113 118.097264)
		(end 198.707181 118.085732)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.253229 120.548858)
		(end 97.226996 120.507432)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.831232 70.854292)
		(end 111.789806 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.985948 68.001228)
		(end 98.034848 67.997621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.295802 120.99164)
		(end 112.246902 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.111728 76.400318)
		(end 203.141895 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.149673 120.188739)
		(end 157.14129 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.718537 120.588947)
		(end 199.68837 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.302804 76.705427)
		(end 108.315881 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.874333 76.897502)
		(end 142.880335 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.054827 120.949827)
		(end 112.008268 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.676087 119.993831)
		(end 217.674883 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.37576 68.752684)
		(end 111.388837 68.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.747176 68.072466)
		(end 157.792924 68.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.884419 57.404977)
		(end 169.891267 56.868713)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.421209 92.353322)
		(end 215.523315 91.826823)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.643366 68.848832)
		(end 185.649368 68.897497)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.979094 80.694877)
		(end 118.957529 80.681299)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.423077 70.703821)
		(end 157.389267 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.344945 90.685602)
		(end 81.346571 90.711033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.96252 120.916799)
		(end 111.917693 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.286833 54.093991)
		(end 215.28008 54.069418)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.937283 70.985609)
		(end 97.888971 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.916504 78.552436)
		(end 93.888271 78.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.87051 26)
		(end 138.919541 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.119736 81.683435)
		(end 85.100496 81.700145)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.128312 26.328112)
		(end 143.162123 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.13168 68.946403)
		(end 157.135287 68.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.888278 28.084687)
		(end 149.354767 28.02999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.438255 62.239971)
		(end 128.450429 62.262359)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.796308 120.507432)
		(end 188.77214 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.524349 33.028043)
		(end 203.510496 33.006652)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.064775 82.880434)
		(end 212.707954 82.480052)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.037909 32.321847)
		(end 203.014979 32.277364)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.238767 83.79405)
		(end 82.947248 84.244208)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.289217 54.069391)
		(end 173.282465 54.093963)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.173493 76.705427)
		(end 157.188874 76.658869)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.468598 114.67094)
		(end 111.493726 114.627661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.080175 26.029939)
		(end 80.128017 26.019195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.57758 120.934446)
		(end 203.531832 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.506273 32.365182)
		(end 185.479008 32.407148)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.945072 68.752684)
		(end 202.958149 68.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.869523 119.062666)
		(end 142.870746 119.013237)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.282458 54.093988)
		(end 173.153602 54.614586)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.016397 67.487311)
		(end 89.531677 67.636016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.79857 28.447553)
		(end 188.774025 28.404646)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.226996 68.481829)
		(end 97.253229 68.440403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.979923 118.069884)
		(end 144.028895 118.07661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.649368 76.897502)
		(end 185.652975 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.652025 120.734053)
		(end 79.616513 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.016481 118.992844)
		(end 194.552788 118.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.792924 68.054819)
		(end 157.839482 68.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.054826 70.953405)
		(end 112.008268 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.782046 87.341166)
		(end 123.639933 86.824029)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.615888 26.142129)
		(end 157.658551 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.802364 78.737636)
		(end 153.765235 78.769663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.719839 82.880436)
		(end 129.703376 82.899887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.013915 118.545308)
		(end 143.040552 118.503667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.13959 70.854292)
		(end 189.098164 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.226391 76.568294)
		(end 157.248437 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.202827 78.468348)
		(end 97.180781 78.42455)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.173493 78.287422)
		(end 157.160416 78.240164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.180781 76.568294)
		(end 97.202827 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.941924 70.799826)
		(end 107.901835 70.828059)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.721939 78.98561)
		(end 143.673627 78.977227)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.411536 28.88913)
		(end 153.363758 28.90181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.310845 120.766081)
		(end 217.27219 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.884707 28.17486)
		(end 199.871418 28.222472)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.726105 70.995218)
		(end 216.677074 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.496767 62.726854)
		(end 122.764921 62.262399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.424993 32.231789)
		(end 111.406628 32.185235)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.96252 68.072466)
		(end 112.008268 68.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.180495 120.99164)
		(end 153.131465 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.982893 26.010812)
		(end 158.031557 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.965151 70.995218)
		(end 198.91612 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.534434 95.014057)
		(end 82.793689 95.49082)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.080175 76.026361)
		(end 80.128017 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.080458 78.995224)
		(end 158.031557 78.991616)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.149925 78.977231)
		(end 112.102083 78.966488)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.773948 76.092336)
		(end 107.817746 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.22584 79.010451)
		(end 204.683323 78.996591)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.350631 26.90108)
		(end 111.356633 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.111027 26.019195)
		(end 199.158869 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.600027 118.203419)
		(end 152.623663 118.193893)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.320155 28.765249)
		(end 143.27952 28.737101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.338303 65.666367)
		(end 131.768943 65.986017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.698219 118.904904)
		(end 196.22824 118.823037)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.839482 26.043016)
		(end 157.886739 26.029939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.095679 70.144005)
		(end 97.089677 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.965437 76.568294)
		(end 142.987483 76.524496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.103528 79.222988)
		(end 90.078575 79.228159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.589557 78.966487)
		(end 107.541715 78.97723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.419827 26.571872)
		(end 79.441873 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.27806 68.007233)
		(end 153.326372 68.015616)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.130477 119.993831)
		(end 154.129273 120.042862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.103708 51.978773)
		(end 174.09211 52.001464)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.712576 70.333974)
		(end 188.697195 70.287416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.232101 26.168362)
		(end 217.27219 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.899932 118.080733)
		(end 97.948729 118.072836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.129601 90.685602)
		(end 127.131227 90.711033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.248365 28.360558)
		(end 108.225973 28.404627)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.965437 26.571872)
		(end 142.987483 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.180782 68.56829)
		(end 97.202827 68.524492)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.546281 80.133241)
		(end 209.059739 79.907622)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.198237 26.010812)
		(end 112.246901 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.658551 78.878466)
		(end 157.615888 78.854298)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.704666 82.062083)
		(end 84.686304 82.079754)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.875182 53.556026)
		(end 81.719912 54.069366)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.463781 78.468352)
		(end 111.441735 78.424555)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.826506 68.705421)
		(end 139.839583 68.752679)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.034562 68.568293)
		(end 154.054432 68.613119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.114806 76.752684)
		(end 97.127883 76.705427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.988348 120.507432)
		(end 153.962115 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.759768 60.726492)
		(end 127.953881 61.226438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.191884 83.794047)
		(end 122.17749 83.773018)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.919541 120.99164)
		(end 138.87051 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.326372 70.977226)
		(end 153.27806 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.064873 114.951958)
		(end 94.073604 115.001236)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.415715 92.378232)
		(end 215.421204 92.353347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.089677 68.897498)
		(end 97.095679 68.848833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.457583 120.588947)
		(end 185.427416 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.946314 114.903124)
		(end 202.95993 114.854967)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.893712 56.843185)
		(end 172.893387 56.868666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178.503508 66.585633)
		(end 178.525738 66.598092)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.031558 120.988033)
		(end 157.982893 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.160911 120.376144)
		(end 97.143264 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.789778 80.992133)
		(end 131.768934 81.006795)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.272606 68.481833)
		(end 157.298839 68.440407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.032918 76.039438)
		(end 80.080175 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.659018 67.642473)
		(end 161.683675 67.636035)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.817677 28.360558)
		(end 199.795285 28.404627)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.655166 120.992844)
		(end 158.129489 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.130476 77.997415)
		(end 157.130476 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.074054 120.140427)
		(end 94.065671 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.792923 78.938029)
		(end 157.747176 78.920383)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.643366 70.144005)
		(end 185.634983 70.192317)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.343656 78.66831)
		(end 97.311629 78.631182)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.754257 67.295862)
		(end 163.251683 67.095382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.495718 26.226762)
		(end 157.534373 26.196595)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.686491 120.824481)
		(end 153.645065 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 208.514961 79.688057)
		(end 208.007946 79.513236)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.645065 70.854292)
		(end 153.602402 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.083495 78.552442)
		(end 203.057262 78.511016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.872116 68.705426)
		(end 199.885193 68.752683)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.445668 114.715423)
		(end 111.468598 114.67094)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.058075 68.193013)
		(end 189.098164 68.164779)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.883213 93.461031)
		(end 82.064494 93.965772)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.816872 85.253439)
		(end 168.805857 85.23046)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.375861 78.953405)
		(end 93.328603 78.966483)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.872116 120.283838)
		(end 199.856735 120.330396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.928864 28.269387)
		(end 142.913236 28.222491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.865114 78.995224)
		(end 203.816213 78.991616)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.820953 61.249992)
		(end 214.83078 61.22648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.612941 76.114382)
		(end 97.656739 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.963691 67.095367)
		(end 88.461119 67.295849)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.341448 120.874883)
		(end 139.29765 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.59337 32.185291)
		(end 185.575005 32.231845)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.458589 26.25879)
		(end 157.495718 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.506595 120.982031)
		(end 189.458284 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.541716 120.973648)
		(end 107.493405 120.982031)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.753098 68.001227)
		(end 184.801762 68.007229)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.913929 76.946403)
		(end 199.915132 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.957637 118.111178)
		(end 190.00433 118.127403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.511236 78.79983)
		(end 199.471147 78.828064)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.135488 115.050833)
		(end 157.14174 115.00118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.063038 114.627661)
		(end 203.090303 114.585695)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.765914 118.703861)
		(end 191.790727 118.709667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.697892 28.222491)
		(end 188.684603 28.174878)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.945173 70.953405)
		(end 184.897916 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.9079 94.991356)
		(end 123.139711 94.507734)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.865114 26.001203)
		(end 203.914145 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.977023 66.859606)
		(end 117.99986 66.848298)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.190675 70.854292)
		(end 217.148012 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.712576 76.658869)
		(end 188.730223 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.361764 114.428798)
		(end 185.37669 114.449453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.485816 70.552436)
		(end 185.457583 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.567169 118.067363)
		(end 189.616508 118.064327)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.226996 78.511012)
		(end 97.202827 78.468348)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.93388 26.403896)
		(end 153.962114 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.129273 120.042862)
		(end 154.125666 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.013639 76.054819)
		(end 217.059387 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.367473 63.674839)
		(end 129.703384 64.092919)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.991177 76.613121)
		(end 203.011047 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.98636 70.938024)
		(end 79.940612 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.880942 120.627602)
		(end 188.850775 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.901835 76.164784)
		(end 107.941924 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.785424 88.468929)
		(end 169.781856 88.443697)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178.503455 80.407207)
		(end 178.042461 80.68127)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.566719 59.651672)
		(end 169.572842 59.626935)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.253254 114.67094)
		(end 157.278382 114.627661)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.750093 78.42455)
		(end 188.730223 78.379724)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.13168 76.946403)
		(end 157.135287 76.897502)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.361578 26.2926)
		(end 185.395388 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.278061 120.982031)
		(end 153.229396 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.68331 78.99659)
		(end 204.670566 78.996428)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.574434 80.992133)
		(end 177.55359 81.006795)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.249905 26.571872)
		(end 108.269776 26.616699)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.273978 82.062083)
		(end 176.255616 82.079754)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.173493 70.287416)
		(end 157.160416 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.747176 120.916799)
		(end 157.702349 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.399957 76.613121)
		(end 79.419827 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.631598 57.991114)
		(end 215.633873 57.965732)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.638421 68.289022)
		(end 111.673933 68.255211)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.567169 28.925498)
		(end 189.518041 28.920025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.73865 55.166045)
		(end 169.636542 54.639547)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.673627 70.977226)
		(end 143.625785 70.966482)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.656581 67.869124)
		(end 91.188522 67.937429)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.995669 28.86544)
		(end 106.949824 28.84692)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.883188 53.531806)
		(end 81.87519 53.556002)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.883442 57.430467)
		(end 169.884418 57.405002)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.578528 120.949827)
		(end 143.53197 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.899947 28.174878)
		(end 142.88903 28.126667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.083663 76.946403)
		(end 94.084867 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.747176 70.920377)
		(end 157.702349 70.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.730223 70.379722)
		(end 188.712576 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.065671 70.192317)
		(end 94.054927 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.066079 62.726854)
		(end 214.334233 62.262399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.790762 60.168839)
		(end 81.79814 60.193231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.656343 120.664731)
		(end 199.622532 120.700243)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.826076 76.324534)
		(end 93.858104 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.850326 26.804104)
		(end 139.858709 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.47565 113.9648)
		(end 93.489503 113.986191)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.198237 70.985609)
		(end 112.149925 70.977226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.636815 68.039437)
		(end 107.683374 68.054818)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.513777 76.072466)
		(end 153.558604 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.578314 118.992192)
		(end 195.113922 118.964807)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.711062 76.223184)
		(end 111.749717 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.796307 26.485411)
		(end 188.82254 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.037479 120.916799)
		(end 184.991732 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.896394 28.08469)
		(end 192.871118 28.087936)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.346808 70.996422)
		(end 98.083879 70.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.096285 26.365241)
		(end 143.128312 26.328112)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.168767 26.142129)
		(end 185.210193 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178.04244 80.681283)
		(end 178.020875 80.694861)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.506595 76.007234)
		(end 189.555259 76.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.825208 118.503667)
		(end 188.853873 118.463395)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.273419 78.799827)
		(end 143.234764 78.76966)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.246997 28.424491)
		(end 191.222513 28.431557)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.124817 93.436817)
		(end 215.280087 92.923477)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.104214 70.900507)
		(end 217.059387 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.720479 118.255742)
		(end 153.759672 118.285865)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.599455 26.142129)
		(end 93.640881 26.168362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.797172 78.468351)
		(end 199.773003 78.511014)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.742215 66.31156)
		(end 164.76378 66.297982)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.479491 70.592525)
		(end 217.449324 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.570278 120.850714)
		(end 97.528852 120.824481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.09568 120.140427)
		(end 97.089677 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.90016 28.568253)
		(end 153.867657 28.605496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.465626 68.193012)
		(end 139.504281 68.223179)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.100051 28.17486)
		(end 154.086762 28.222472)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.340137 53.556031)
		(end 169.332138 53.531836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.284666 118.065571)
		(end 107.334063 118.063717)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.309471 82.46143)
		(end 84.292036 82.480016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.04185 68.705421)
		(end 94.054927 68.752679)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.920144 115.050833)
		(end 202.926396 115.00118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.933881 70.592525)
		(end 153.903714 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.935126 32.040885)
		(end 202.926395 31.991607)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.924344 52.485142)
		(end 168.692531 52.001522)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.315411 118.080714)
		(end 153.363758 118.091015)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.653568 84.752877)
		(end 82.409479 85.230419)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.759671 28.706959)
		(end 153.720478 28.737083)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.987483 76.524496)
		(end 143.011652 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.53197 70.938024)
		(end 143.486222 70.920377)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.572583 78.631186)
		(end 111.542416 78.592531)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.797172 76.524496)
		(end 199.819218 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.684118 120.236581)
		(end 188.673375 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.059771 67.085235)
		(end 209.546312 66.859617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.326065 26.25879)
		(end 185.361578 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.27506 79.907612)
		(end 163.251675 79.897485)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.971104 28.916233)
		(end 152.922525 28.907093)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.926395 31.991607)
		(end 202.920143 31.941954)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.074053 26.852416)
		(end 94.080055 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.2742 33.006653)
		(end 139.260348 33.028043)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.379304 28.815329)
		(end 199.334952 28.837157)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.831851 28.928534)
		(end 143.782513 28.925498)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.719625 68.223179)
		(end 93.756754 68.255206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.704197 78.995218)
		(end 184.655166 78.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.435018 28.865458)
		(end 98.388324 28.881684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.376705 114.449473)
		(end 185.449669 114.545193)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.57833 28.00065)
		(end 194.552855 28)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.958222 91.80164)
		(end 124.033312 91.270614)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.546335 66.859606)
		(end 209.569172 66.848298)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.730223 78.379724)
		(end 188.712576 78.333976)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.965151 26.001203)
		(end 199.014051 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.775006 76.001232)
		(end 216.82367 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.253368 118.818496)
		(end 196.778518 118.709672)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.671276 26.90108)
		(end 217.674883 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.13168 78.046446)
		(end 157.130476 77.997415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.702349 70.900507)
		(end 157.658551 70.878461)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.60416 120.99164)
		(end 189.55526 120.988033)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.98636 120.934446)
		(end 79.940612 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.850074 76.015617)
		(end 184.897916 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.856735 78.333979)
		(end 199.839088 78.379727)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.514183 78.552442)
		(end 111.48795 78.511016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.645257 118.962855)
		(end 147.670666 118.964806)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.70116 76.440407)
		(end 139.727393 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.756715 118.11874)
		(end 97.803807 118.103713)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.622532 70.703821)
		(end 199.58702 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.819217 78.424553)
		(end 199.797172 78.468351)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.528852 78.828061)
		(end 97.488763 78.799827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.768963 65.986032)
		(end 131.789807 66.000693)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.066118 70.592525)
		(end 143.037885 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.962168 63.219843)
		(end 167.976562 63.198814)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.311639 59.103173)
		(end 127.427162 59.626891)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.255598 82.079772)
		(end 175.878801 82.461412)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.302804 68.705426)
		(end 108.315881 68.752683)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.544635 118.964806)
		(end 103.570044 118.962855)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.520508 76.400318)
		(end 79.550675 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.962089 32.321903)
		(end 93.936961 32.365182)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.326066 78.737632)
		(end 185.288937 78.769659)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.344617 70.04644)
		(end 108.34101 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.486222 68.072462)
		(end 143.53197 68.054815)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.149672 76.800526)
		(end 157.160416 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.344597 27.979606)
		(end 108.340931 28.028902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.634983 76.800526)
		(end 185.643366 76.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.320156 118.227612)
		(end 143.362133 118.201509)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.012516 76.524496)
		(end 154.034562 76.568294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.011047 70.424549)
		(end 202.991177 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.249906 68.568293)
		(end 108.269776 68.613119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.310845 76.223184)
		(end 217.347974 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.7034 64.092938)
		(end 129.719864 64.11239)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.374214 120.962904)
		(end 153.326372 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.667869 93.461031)
		(end 127.84915 93.965772)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 216.726105 26.001203)
		(end 216.775006 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.672926 26.403896)
		(end 139.70116 26.443985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.327073 120.588947)
		(end 157.298839 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.243245 68.255211)
		(end 203.280374 68.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.377467 70.703821)
		(end 97.343657 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.017708 78.737636)
		(end 107.980579 78.769663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.153057 89.001729)
		(end 127.150782 89.027111)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.896377 118.908156)
		(end 193.429888 118.962853)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.811125 78.333975)
		(end 139.793478 78.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.252823 68.07246)
		(end 139.29765 68.092331)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.963728 61.249998)
		(end 128.183116 61.73938)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.556792 78.878461)
		(end 93.512994 78.900507)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.864712 76.897502)
		(end 139.868319 76.946403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.198237 68.007234)
		(end 112.246902 68.001232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.549891 26.226762)
		(end 199.587019 26.25879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.665936 28.929126)
		(end 189.616507 28.928534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.683373 70.938024)
		(end 107.636815 70.953405)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.895937 68.800525)
		(end 199.90432 68.848836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.000778 58.523908)
		(end 124.062283 57.991139)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.963702 85.742851)
		(end 127.953875 85.766363)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.789806 76.164784)
		(end 111.831232 76.138551)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.113259 26.029939)
		(end 139.160516 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.357084 115.00118)
		(end 111.365814 114.951902)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.673628 120.973648)
		(end 143.625786 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.136626 83.338294)
		(end 174.822501 83.772979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.868535 75.996422)
		(end 153.131464 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.916121 67.99642)
		(end 198.965151 67.997623)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.488015 82.899907)
		(end 175.152105 83.317986)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.243285 118.118722)
		(end 199.289576 118.13606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.531402 114.670996)
		(end 185.554332 114.715479)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.313508 68.164779)
		(end 143.354934 68.138546)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.272606 78.511016)
		(end 157.248437 78.468352)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.346809 120.992844)
		(end 98.083879 120.992844)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.850774 70.592525)
		(end 188.822541 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.464221 60.702479)
		(end 123.632552 60.193273)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.718536 78.592529)
		(end 199.68837 78.631185)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.788192 59.62691)
		(end 123.903713 59.103192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.340886 28.895579)
		(end 98.292818 28.907111)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.767549 78.985614)
		(end 203.719237 78.977231)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.578134 70.379722)
		(end 185.558264 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.08746 70.287416)
		(end 154.072079 70.333974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.935224 64.112409)
		(end 84.292045 64.512791)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.328723 70.095341)
		(end 79.325116 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.874457 118.097264)
		(end 152.922525 118.085732)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.655382 120.042862)
		(end 188.654179 119.993831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.493404 70.985609)
		(end 107.44474 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.177458 68.440405)
		(end 108.203691 68.481831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.665274 120.140427)
		(end 217.656891 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.458284 68.015613)
		(end 189.506595 68.00723)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198.519136 28.84692)
		(end 198.408384 28.79896)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.719238 68.015617)
		(end 203.767549 68.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.880356 32.447706)
		(end 93.807435 32.54337)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.630755 51.490884)
		(end 112.244835 33.501944)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.28456 28.529466)
		(end 97.255896 28.489194)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.528852 26.168362)
		(end 97.570278 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.96252 76.072466)
		(end 112.008268 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.168767 76.138551)
		(end 185.210193 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.008821 26.616699)
		(end 94.026468 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.600042 70.379722)
		(end 217.580172 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.458629 118.118722)
		(end 153.50492 118.13606)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.232101 120.824481)
		(end 217.190675 120.850714)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.572584 120.627602)
		(end 111.542417 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.57879 54.639521)
		(end 81.476684 55.16602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.14129 120.140427)
		(end 157.135288 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.645065 120.850714)
		(end 153.602402 120.874883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.649368 120.091763)
		(end 185.643366 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.674883 120.042862)
		(end 217.671276 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.135287 68.897502)
		(end 157.141289 68.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.930782 28.529448)
		(end 153.90016 28.568253)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.080055 26.90108)
		(end 94.083662 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.919943 68.897502)
		(end 202.925945 68.848838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.864711 26.90108)
		(end 139.868318 26.949981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.203692 120.507432)
		(end 108.177459 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.578807 92.353321)
		(end 81.584296 92.378206)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.980579 76.223184)
		(end 108.017708 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.127883 68.705423)
		(end 97.143264 68.658864)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.011048 120.420971)
		(end 202.991178 120.376144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.130477 115.150779)
		(end 157.131731 115.100737)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.504281 76.223184)
		(end 139.54141 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.542416 70.592525)
		(end 111.514183 70.552436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.493404 76.007234)
		(end 107.541716 76.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.488763 76.193017)
		(end 97.528852 76.164784)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.404218 68.658868)
		(end 111.421865 68.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.658551 68.114382)
		(end 157.702349 68.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.839049 28.79895)
		(end 106.815413 28.789424)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.036297 61.249992)
		(end 169.046124 61.22648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.702349 68.092336)
		(end 157.747176 68.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.322925 70.996422)
		(end 80.273894 70.995218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.330924 89.587866)
		(end 81.324076 90.12413)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.473016 87.88967)
		(end 215.357493 87.365952)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.868319 70.04644)
		(end 139.864712 70.095341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.773948 78.900511)
		(end 107.729121 78.920381)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.638421 78.703827)
		(end 111.60461 78.668314)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.104214 76.092336)
		(end 217.148012 76.114382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.686491 70.828059)
		(end 153.645065 70.854292)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.12291 81.326475)
		(end 177.102843 81.342181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.489367 64.930761)
		(end 130.885161 65.292664)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.143264 68.658864)
		(end 97.160911 68.613116)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.234085 28.288982)
		(end 105.209272 28.283176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.655166 75.996422)
		(end 184.704197 75.997625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.882293 28.601694)
		(end 197.858202 28.593387)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.36894 54.614611)
		(end 127.363451 54.639496)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.316689 67.996253)
		(end 92.329433 67.996415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.063038 32.365126)
		(end 203.037909 32.321847)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.556383 67.642467)
		(end 90.078584 67.764668)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.418017 118.317909)
		(end 97.455672 118.285884)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.101242 78.996427)
		(end 112.344832 78.996427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.531832 120.916799)
		(end 203.487005 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.912968 26.328112)
		(end 188.946779 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.427416 70.63118)
		(end 185.395388 70.668309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.63307 26.709005)
		(end 217.646147 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.08746 76.705427)
		(end 154.100537 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.328604 76.026361)
		(end 93.375861 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.643365 26.852416)
		(end 185.649367 26.90108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.884494 28.568272)
		(end 188.853872 28.529466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.347686 28.605514)
		(end 97.315182 28.568272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.474292 66.598107)
		(end 118.496522 66.585649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.100537 78.240163)
		(end 154.08746 78.28742)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.727393 120.507432)
		(end 139.701161 120.548858)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.934582 68.015617)
		(end 157.982893 68.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.764901 84.730462)
		(end 122.496746 84.266006)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.292818 118.08575)
		(end 98.340886 118.097282)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.008267 26.058397)
		(end 112.054826 26.043016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.925945 76.848838)
		(end 202.934328 76.800526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.327065 118.908156)
		(end 101.860576 118.962853)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.665167 28.077975)
		(end 188.659067 28.028921)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.273894 75.997625)
		(end 80.322925 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.92792 78.333976)
		(end 142.912539 78.287417)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.040069 32.137876)
		(end 94.024058 32.185291)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.819218 70.424549)
		(end 199.797172 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.192606 32.54337)
		(end 203.119642 32.44765)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.675924 90.124152)
		(end 215.669073 89.587887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.323913 20.012272)
		(end 73.323913 126.980571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.617689 70.333974)
		(end 217.600042 70.379722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.548406 80.694877)
		(end 210.526841 80.681299)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.280073 54.069394)
		(end 215.1248 53.556056)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.729121 76.072466)
		(end 107.773948 76.092336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.860277 52.485132)
		(end 173.849853 52.508386)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.394447 55.747595)
		(end 81.34657 56.281762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.258895 80.394739)
		(end 163.784508 80.144571)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.966906 78.468347)
		(end 93.942737 78.51101)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.446352 81.326476)
		(end 211.015712 81.006826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.987329 118.317909)
		(end 189.024984 118.285884)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.146789 28.791353)
		(end 189.104811 28.765249)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.85188 54.639522)
		(end 123.846391 54.614637)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.162123 68.289018)
		(end 143.197635 68.255207)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.326624 26.804104)
		(end 108.335007 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.942737 68.481827)
		(end 93.966906 68.524491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.581982 28.674934)
		(end 199.544327 28.706959)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.422419 76.054819)
		(end 93.468167 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.15209 83.318006)
		(end 175.136641 83.338273)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.880336 120.140427)
		(end 142.874333 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.397597 78.878462)
		(end 143.354934 78.854294)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.094127 82.46143)
		(end 130.076692 82.480016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.987328 28.674953)
		(end 188.951304 28.641104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.295802 70.995218)
		(end 112.246901 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.913237 118.770371)
		(end 142.928864 118.723474)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.795285 28.404627)
		(end 199.77074 28.447535)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.270878 76.072466)
		(end 189.316626 76.054819)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.577477 118.201509)
		(end 97.620695 118.177514)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.270878 78.920378)
		(end 189.226051 78.900508)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.218147 58.549171)
		(end 127.306778 59.078105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.045992 55.166045)
		(end 173.041781 55.191178)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.463781 76.524496)
		(end 111.48795 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.011652 120.507432)
		(end 142.987484 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.793478 70.379722)
		(end 139.773608 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.124793 53.556031)
		(end 215.116794 53.531836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.412979 76.255212)
		(end 97.450108 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.945173 120.949827)
		(end 184.897916 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.034562 120.420971)
		(end 154.012516 120.464769)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.624139 120.949827)
		(end 203.57758 120.934446)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.864712 120.091763)
		(end 139.85871 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 223.676087 126.980571)
		(end 223.676087 20.012272)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.868268 31.892106)
		(end 139.864511 31.94201)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.946792 28.315453)
		(end 142.928864 28.269387)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.280762 70.977226)
		(end 93.23245 70.985609)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.344833 75.996422)
		(end 138.87051 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.418016 28.674953)
		(end 97.381992 28.641104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.849843 52.508409)
		(end 173.643029 53.003237)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.415444 95.501988)
		(end 168.421677 95.490867)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.033093 70.468347)
		(end 203.011047 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.477873 87.914713)
		(end 215.473021 87.889695)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.817746 68.114381)
		(end 107.860409 68.138549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.200623 79.127607)
		(end 181.672865 79.222983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.665047 118.155686)
		(end 97.710424 118.136079)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.693217 87.914713)
		(end 169.688365 87.889695)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.655054 56.307241)
		(end 215.653428 56.28181)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.528852 70.828059)
		(end 97.488763 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.798571 118.545308)
		(end 188.825208 118.503667)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.458589 76.255212)
		(end 157.495718 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.910243 28.028902)
		(end 199.904143 28.077956)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.776733 67.479615)
		(end 134.801029 67.487304)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.655401 27.979625)
		(end 188.654178 27.930196)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.507724 120.548858)
		(end 217.479491 120.588947)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.724939 67.085231)
		(end 133.748324 67.095358)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.136793 67.764678)
		(end 161.658993 67.642479)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.444518 93.436812)
		(end 173.452517 93.461007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.88674 68.02636)
		(end 157.934582 68.015617)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.55526 68.001228)
		(end 189.60416 67.997621)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.388324 28.881684)
		(end 98.340886 28.895579)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.47668 55.166045)
		(end 81.472469 55.191178)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.788175 87.365927)
		(end 123.782052 87.34119)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.054927 68.752679)
		(end 94.065671 68.800521)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.480863 28.846939)
		(end 98.435018 28.865458)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.111728 68.400318)
		(end 203.141895 68.361662)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.637027 95.490856)
		(end 122.896279 95.014093)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.410442 120.962904)
		(end 189.363184 120.949827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.377467 76.289022)
		(end 97.412979 76.255212)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.327072 68.400318)
		(end 157.357239 68.361662)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.957559 66.31156)
		(end 118.979124 66.297982)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.934779 52.508419)
		(end 168.924355 52.485165)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.441873 70.468347)
		(end 79.419827 70.424549)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.111281 120.188739)
		(end 154.100538 120.236581)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.555481 53.556031)
		(end 123.547482 53.531836)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.444739 78.991615)
		(end 107.395839 78.995222)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.389266 78.668314)
		(end 157.357239 78.631186)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.362133 118.201509)
		(end 143.405351 118.177514)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.95993 114.854967)
		(end 202.975941 114.807552)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.773608 76.568294)
		(end 139.793478 76.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.180495 26.001203)
		(end 153.229395 26.00481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.966977 28.360576)
		(end 142.946792 28.315453)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.369244 95.501959)
		(end 184.755164 113.490899)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.57758 76.054819)
		(end 203.624138 76.039438)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.934581 76.015617)
		(end 157.982893 76.007234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.801053 67.487311)
		(end 135.316333 67.636016)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.48795 70.51101)
		(end 111.463781 70.468347)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.513777 70.920377)
		(end 153.468029 70.938024)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.104375 118.866194)
		(end 97.115292 118.817983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.772139 76.524496)
		(end 188.796308 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.930783 118.463377)
		(end 153.959447 118.503649)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.487005 76.092336)
		(end 203.531832 76.072466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.125666 120.091763)
		(end 154.119664 120.140427)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.114806 120.236581)
		(end 97.104063 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.488763 68.193013)
		(end 97.528852 68.164779)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.315881 68.752683)
		(end 108.326625 68.800525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.634982 26.804104)
		(end 185.643365 26.852416)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.343108 26.804104)
		(end 79.353852 26.756262)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.114051 78.996422)
		(end 138.101308 78.996584)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.547474 53.531812)
		(end 123.366193 53.027071)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.015692 81.006811)
		(end 210.994848 80.99215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.558822 67.86913)
		(end 160.584006 67.86524)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.676087 69.997409)
		(end 217.674883 70.04644)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.667844 53.531806)
		(end 127.659846 53.556002)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.08703 76.324534)
		(end 108.119058 76.361663)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.671395 78.966488)
		(end 203.624138 78.95341)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.357083 31.991607)
		(end 111.350831 31.941954)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 207.443674 67.642473)
		(end 207.468331 67.636035)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.701566 68.072462)
		(end 97.747314 68.054815)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.880941 70.63118)
		(end 188.850774 70.592525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.642512 59.626916)
		(end 81.648635 59.651653)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.63254 86.799588)
		(end 123.464207 86.290382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.963759 55.747595)
		(end 172.915882 56.281762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.08703 26.328112)
		(end 108.119057 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.458284 120.973648)
		(end 189.410442 120.962904)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.368401 89.001729)
		(end 81.366126 89.027111)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.014052 120.988033)
		(end 198.965151 120.99164)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.387058 120.874883)
		(end 199.34326 120.896929)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.340932 118.963922)
		(end 108.344598 119.013218)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.562167 118.561278)
		(end 152.07348 118.399463)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.146022 118.065589)
		(end 98.195267 118.069884)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.315411 28.91211)
		(end 153.266614 28.920007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.707937 82.480033)
		(end 212.690502 82.461448)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.280374 68.223184)
		(end 203.319029 68.193017)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.248437 26.528074)
		(end 157.272606 26.485411)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.50954 79.907608)
		(end 179.022999 80.133226)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.54141 76.255212)
		(end 139.576922 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.620695 118.177514)
		(end 97.665047 118.155686)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.335008 78.14401)
		(end 108.326625 78.192321)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.313508 70.828059)
		(end 143.273419 70.799826)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.615888 78.854298)
		(end 157.574462 78.828065)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.85321 28.791334)
		(end 107.809992 28.815329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.356633 26.852416)
		(end 111.365016 26.804104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.803807 28.889149)
		(end 97.756714 28.874121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.080458 26.001203)
		(end 158.129489 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.868319 76.946403)
		(end 139.869523 76.995434)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.128313 120.664731)
		(end 143.096286 120.627602)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.034848 78.99522)
		(end 97.985947 78.991612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.404219 120.330396)
		(end 111.388838 120.283838)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.711151 28.593388)
		(end 190.687059 28.601694)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.594649 118.177495)
		(end 153.637866 118.20149)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.70798 64.512808)
		(end 213.064799 64.112426)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.281423 62.726854)
		(end 168.549577 62.262399)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.316639 78.996585)
		(end 91.774123 79.010444)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 80.224993 26.00481)
		(end 80.273894 26.001203)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.443626 28.169806)
		(end 149.913604 28.087939)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.064475 53.02704)
		(end 81.883196 53.531782)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.201852 86.799588)
		(end 215.033519 86.290382)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.066045 84.265984)
		(end 214.052744 84.244248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.86877 56.281784)
		(end 169.82089 55.747618)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.191285 114.807552)
		(end 157.20965 114.760998)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.605552 91.245248)
		(end 215.653429 90.711081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.251615 85.742845)
		(end 123.032227 85.253463)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.125666 78.095345)
		(end 154.119664 78.14401)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.450108 70.769659)
		(end 97.412979 70.737631)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.865114 75.997625)
		(end 203.914145 75.996422)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.253384 28.174342)
		(end 196.228307 28.16981)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.71352 28.269387)
		(end 188.697892 28.222491)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.173922 26.328112)
		(end 203.207733 26.2926)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.455348 118.964807)
		(end 193.990955 118.992192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.04185 78.287416)
		(end 94.026469 78.333975)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.817745 26.11796)
		(end 107.860409 26.142129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 202.958149 26.709005)
		(end 202.97353 26.662447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.270878 68.072462)
		(end 189.316626 68.054815)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.68837 78.631185)
		(end 199.656342 78.668313)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.600042 120.376144)
		(end 217.580172 120.420971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.279521 118.25576)
		(end 143.320156 118.227612)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.999883 66.848287)
		(end 118.474269 66.59812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.465603 95.01407)
		(end 214.477201 94.991379)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.727393 26.485411)
		(end 139.751561 26.528074)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.160416 120.236581)
		(end 157.149673 120.188739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.183098 85.253445)
		(end 127.963712 85.742827)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.331904 57.430471)
		(end 81.366128 57.965687)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.198237 120.982031)
		(end 112.149926 120.973648)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.065856 66.585636)
		(end 210.52685 66.311573)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.443207 26.11796)
		(end 203.487005 26.095914)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.809324 26.142129)
		(end 79.851987 26.11796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.302804 78.28742)
		(end 108.287423 78.333979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.344617 78.046444)
		(end 108.34101 78.095345)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.086762 28.222472)
		(end 154.071135 28.269369)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.987483 78.468348)
		(end 142.965437 78.42455)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.489322 82.062083)
		(end 130.47096 82.079754)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.326372 76.015617)
		(end 153.374214 76.026361)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.188874 68.658868)
		(end 157.206521 68.613121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.982291 26.25879)
		(end 189.019419 26.226762)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.765235 68.223183)
		(end 153.802364 68.25521)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.34326 120.896929)
		(end 199.298434 120.916799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.959447 118.503649)
		(end 153.986085 118.54529)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.429919 58.523914)
		(end 81.433487 58.549146)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.584588 95.501959)
		(end 138.970508 113.490899)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.269776 68.613119)
		(end 108.287423 68.658867)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.484981 79.688052)
		(end 88.46111 79.696971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.912539 70.287416)
		(end 142.899462 70.240159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.201428 28.447535)
		(end 108.174791 28.489176)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.064873 32.040941)
		(end 94.053685 32.089719)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.425565 66.00071)
		(end 119.446409 65.986048)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.962114 76.440407)
		(end 153.988347 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.701565 26.076044)
		(end 97.747313 26.058397)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.347024 78.046446)
		(end 111.34582 77.997415)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.913929 120.042862)
		(end 199.910322 120.091763)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.946793 118.677408)
		(end 142.966978 118.632285)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.344941 56.307244)
		(end 81.324401 56.843159)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.850774 26.403896)
		(end 188.880941 26.365241)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.504281 120.766081)
		(end 139.465626 120.796248)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.872116 76.705427)
		(end 199.885193 76.752684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.33616 20)
		(end 73.325158 20.00027)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.173923 70.668309)
		(end 203.141895 70.63118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.334986 32.44765)
		(end 157.305647 32.407092)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 217.507724 76.440407)
		(end 217.533957 76.481833)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.891268 90.124152)
		(end 169.884417 89.587887)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.639945 60.168833)
		(end 123.782057 59.651696)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.326066 76.255212)
		(end 185.361578 76.289022)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.581983 118.31789)
		(end 199.618007 118.351739)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.673933 76.255212)
		(end 111.711062 76.223184)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.017106 70.985609)
		(end 138.968442 70.991611)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.849529 114.951958)
		(end 139.85826 115.001236)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.182028 55.722254)
		(end 127.179106 55.747569)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.679843 28.765231)
		(end 153.637866 28.791334)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.820896 91.245248)
		(end 169.868773 90.711081)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.471147 76.164784)
		(end 199.511236 76.193017)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 112.523043 49.098953 0)
		(layer "F.SilkS")
	)
	(gr_text "1S LTO\nBMS"
		(at 99.073043 38.098953 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 194.276957 84.943891 180)
		(layer "F.SilkS")
	)
	(gr_text "UPDI"
		(at 138.642301 95.343891 180)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 205.442355 39.298953 120)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 92.857645 92.843891 180)
		(layer "F.SilkS")
	)
	(gr_text "QWIIC\nµŠup"
		(at 153.457699 32.148953 90)
		(layer "F.SilkS")
	)
	(gr_text "+ -"
		(at 154.342301 101.533891 240)
		(layer "F.SilkS")
	)
	(gr_text "+ -"
		(at 200.126957 101.533891 240)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 184.476957 97.893891 180)
		(layer "F.SilkS")
	)
	(gr_text "QWIIC\nµŠup"
		(at 189.326957 114.843891 270)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 148.492301 84.943891 180)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 184.426957 92.843891 180)
		(layer "F.SilkS")
	)
	(gr_text "UPDI"
		(at 112.573043 51.648953 0)
		(layer "F.SilkS")
	)
	(gr_text "RevC, 2025-11-20\nVlastimil Slinták\nµArt.cz"
		(at 174.592355 61.488953 30)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 138.692301 97.893891 180)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 113.873043 39.298953 120)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 159.657699 39.298953 120)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 178.476957 99.743891 300)
		(layer "F.SilkS")
	)
	(gr_text "1S LTO\nBMS"
		(at 152.142301 108.893891 180)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 204.142355 54.148953 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 204.092355 49.098953 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 132.692301 99.743891 300)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 210.092355 47.248953 120)
		(layer "F.SilkS")
	)
	(gr_text "QWIIC\nµŠup"
		(at 143.542301 114.843891 270)
		(layer "F.SilkS")
	)
	(gr_text "+ -"
		(at 108.557645 101.533891 240)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 164.307699 47.248953 120)
		(layer "F.SilkS")
	)
	(gr_text "RevC, 2025-11-20\nVlastimil Slinták\nµArt.cz"
		(at 168.192301 85.503891 210)
		(layer "F.SilkS")
	)
	(gr_text "QWIIC\nµŠup"
		(at 97.757645 114.843891 270)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 158.307699 49.098953 0)
		(layer "F.SilkS")
	)
	(gr_text "UPDI"
		(at 204.142355 51.648953 0)
		(layer "F.SilkS")
	)
	(gr_text "+ -"
		(at 96.873043 45.458953 60)
		(layer "F.SilkS")
	)
	(gr_text "UPDI"
		(at 92.857645 95.343891 180)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 92.907645 97.893891 180)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 148.507699 62.048953 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 183.126957 107.693891 300)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 137.342301 107.693891 300)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 112.573043 54.148953 0)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 138.642301 92.843891 180)
		(layer "F.SilkS")
	)
	(gr_text "UPDI"
		(at 184.426957 95.343891 180)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 194.292355 62.048953 0)
		(layer "F.SilkS")
	)
	(gr_text "+ -"
		(at 142.657699 45.458953 60)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 91.557645 107.693891 300)
		(layer "F.SilkS")
	)
	(gr_text "1S LTO\nBMS"
		(at 106.357645 108.893891 180)
		(layer "F.SilkS")
	)
	(gr_text "RevC, 2025-11-20\nVlastimil Slinták\nµArt.cz"
		(at 128.807699 61.488953 30)
		(layer "F.SilkS")
	)
	(gr_text "1S LTO\nBMS"
		(at 197.926957 108.893891 180)
		(layer "F.SilkS")
	)
	(gr_text "RevC, 2025-11-20\nVlastimil Slinták\nµArt.cz"
		(at 83.023043 61.488953 30)
		(layer "F.SilkS")
	)
	(gr_text "QWIIC\nµŠup"
		(at 199.242355 32.148953 90)
		(layer "F.SilkS")
	)
	(gr_text "UPDI"
		(at 158.357699 51.648953 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 102.723043 62.048953 0)
		(layer "F.SilkS")
	)
	(gr_text "RevC, 2025-11-20\nVlastimil Slinták\nµArt.cz"
		(at 122.407645 85.503891 210)
		(layer "F.SilkS")
	)
	(gr_text "1S LTO\nBMS"
		(at 190.642355 38.098953 0)
		(layer "F.SilkS")
	)
	(gr_text "QWIIC\nµŠup"
		(at 107.673043 32.148953 90)
		(layer "F.SilkS")
	)
	(gr_text "RevC, 2025-11-20\nVlastimil Slinták\nµArt.cz"
		(at 213.976957 85.503891 210)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 102.707645 84.943891 180)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 86.907645 99.743891 300)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 118.523043 47.248953 120)
		(layer "F.SilkS")
	)
	(gr_text "1S LTO\nBMS"
		(at 144.857699 38.098953 0)
		(layer "F.SilkS")
	)
	(gr_text "+ -"
		(at 188.442355 45.458953 60)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 158.357699 54.148953 0)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.676957 85.743891) (xy 187.276957 85.743891) (xy 187.276957 83.943891) (xy 189.676957 83.943891)
			)
		)
	)
	(zone
		(net 126)
		(net_name "Board_4-Net-(JP1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.692301 87.243891) (xy 145.442301 87.243891) (xy 145.442301 85.583891) (xy 144.192301 85.583891)
				(xy 144.192301 85.743891) (xy 138.692301 85.743891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 107.323043 61.248953) (xy 109.723043 61.248953) (xy 109.723043 63.048953) (xy 107.323043 63.048953)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Board_0-Net-(J2-Pin_1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 93.323043 43.948953) (xy 89.223043 41.548953) (xy 86.423043 46.348953) (xy 88.123043 47.348953)
				(xy 89.023043 45.748953) (xy 91.423043 47.148953)
			)
		)
	)
	(zone
		(net 147)
		(net_name "Board_5-ADC_SP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193.076957 113.943891) (xy 193.076957 107.843891) (xy 191.276957 107.843891) (xy 191.276957 113.943891)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Board_0-Net-(Q1-S)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.723043 59.098953) (xy 95.493043 59.098953) (xy 95.493043 61.548953) (xy 92.723043 61.548953)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.342355 47.248953) (xy 184.792355 48.048953) (xy 182.742355 51.448953) (xy 181.542355 50.748953)
			)
		)
	)
	(zone
		(net 140)
		(net_name "Board_4-VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.792301 91.643891) (xy 137.792301 85.743891) (xy 138.392301 85.743891) (xy 138.392301 87.743891)
				(xy 139.892301 87.743891) (xy 139.892301 91.643891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.557699 47.248953) (xy 139.007699 48.048953) (xy 136.957699 51.448953) (xy 135.757699 50.748953)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 205.226957 99.743891) (xy 203.776957 98.943891) (xy 205.826957 95.543891) (xy 207.026957 96.243891)
			)
		)
	)
	(zone
		(net 57)
		(net_name "Board_2-+BATT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 197.426089 62.449156) (xy 197.042355 62.448953) (xy 197.042355 59.748953) (xy 189.992355 59.748953)
				(xy 189.992355 58.118953) (xy 189.342355 58.118953) (xy 189.342355 62.348953) (xy 187.292355 62.348953)
				(xy 187.292355 68.048953) (xy 190.392355 68.048953) (xy 197.392355 68.048953)
			)
		)
	)
	(zone
		(net 113)
		(net_name "Board_4-+BATT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 145.358567 84.543688) (xy 145.742301 84.543891) (xy 145.742301 87.243891) (xy 152.792301 87.243891)
				(xy 152.792301 88.873891) (xy 153.442301 88.873891) (xy 153.442301 84.643891) (xy 155.492301 84.643891)
				(xy 155.492301 78.943891) (xy 152.392301 78.943891) (xy 145.392301 78.943891)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Board_0-VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.423043 55.348953) (xy 113.423043 61.248953) (xy 112.823043 61.248953) (xy 112.823043 59.248953)
				(xy 111.323043 59.248953) (xy 111.323043 55.348953)
			)
		)
	)
	(zone
		(net 150)
		(net_name "Board_5-Net-(J2-Pin_1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 203.676957 103.043891) (xy 207.776957 105.443891) (xy 210.576957 100.643891) (xy 208.876957 99.643891)
				(xy 207.976957 101.243891) (xy 205.576957 99.843891)
			)
		)
	)
	(zone
		(net 85)
		(net_name "Board_3-+BATT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 99.573911 84.543688) (xy 99.957645 84.543891) (xy 99.957645 87.243891) (xy 107.007645 87.243891)
				(xy 107.007645 88.873891) (xy 107.657645 88.873891) (xy 107.657645 84.643891) (xy 109.707645 84.643891)
				(xy 109.707645 78.943891) (xy 106.607645 78.943891) (xy 99.607645 78.943891)
			)
		)
	)
	(zone
		(net 122)
		(net_name "Board_4-Net-(J2-Pin_1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.892301 103.043891) (xy 161.992301 105.443891) (xy 164.792301 100.643891) (xy 163.092301 99.643891)
				(xy 162.192301 101.243891) (xy 159.792301 99.843891)
			)
		)
	)
	(zone
		(net 56)
		(net_name "Board_1-VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 159.207699 55.348953) (xy 159.207699 61.248953) (xy 158.607699 61.248953) (xy 158.607699 59.248953)
				(xy 157.107699 59.248953) (xy 157.107699 55.348953)
			)
		)
	)
	(zone
		(net 98)
		(net_name "Board_3-Net-(JP1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.907645 87.243891) (xy 99.657645 87.243891) (xy 99.657645 85.583891) (xy 98.407645 85.583891)
				(xy 98.407645 85.743891) (xy 92.907645 85.743891)
			)
		)
	)
	(zone
		(net 90)
		(net_name "Board_3-ADC_LP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.407645 84.843891) (xy 116.507645 84.843891) (xy 116.507645 91.543891) (xy 112.207645 98.943891)
				(xy 109.807645 97.643891) (xy 113.407645 91.043891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.657645 83.343891) (xy 92.657645 81.643891) (xy 98.307645 81.643891) (xy 98.307645 83.343891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 153.107699 61.248953) (xy 155.507699 61.248953) (xy 155.507699 63.048953) (xy 153.107699 63.048953)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.773043 47.248953) (xy 93.223043 48.048953) (xy 91.173043 51.448953) (xy 89.973043 50.748953)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.342355 63.648953) (xy 204.342355 65.348953) (xy 198.692355 65.348953) (xy 198.692355 63.648953)
			)
		)
	)
	(zone
		(net 144)
		(net_name "Board_5-ADC_LN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 207.876957 100.743891) (xy 205.476957 99.343891) (xy 207.926957 95.093891) (xy 208.776957 95.543891)
				(xy 212.376957 97.643891) (xy 210.776957 100.243891) (xy 208.776957 99.143891)
			)
		)
	)
	(zone
		(net 129)
		(net_name "Board_4-Net-(Q1-S)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.492301 87.893891) (xy 155.722301 87.893891) (xy 155.722301 85.443891) (xy 158.492301 85.443891)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Board_1-+BATT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.641433 62.449156) (xy 151.257699 62.448953) (xy 151.257699 59.748953) (xy 144.207699 59.748953)
				(xy 144.207699 58.118953) (xy 143.557699 58.118953) (xy 143.557699 62.348953) (xy 141.507699 62.348953)
				(xy 141.507699 68.048953) (xy 144.607699 68.048953) (xy 151.607699 68.048953)
			)
		)
	)
	(zone
		(net 32)
		(net_name "Board_1-ADC_LN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 134.907699 46.248953) (xy 137.307699 47.648953) (xy 134.857699 51.898953) (xy 134.007699 51.448953)
				(xy 130.407699 49.348953) (xy 132.007699 46.748953) (xy 134.007699 47.848953)
			)
		)
	)
	(zone
		(net 88)
		(net_name "Board_3-ADC_LN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.307645 100.743891) (xy 113.907645 99.343891) (xy 116.357645 95.093891) (xy 117.207645 95.543891)
				(xy 120.807645 97.643891) (xy 119.207645 100.243891) (xy 117.207645 99.143891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 198.892355 61.248953) (xy 201.292355 61.248953) (xy 201.292355 63.048953) (xy 198.892355 63.048953)
			)
		)
	)
	(zone
		(net 118)
		(net_name "Board_4-ADC_LP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 159.192301 84.843891) (xy 162.292301 84.843891) (xy 162.292301 91.543891) (xy 157.992301 98.943891)
				(xy 155.592301 97.643891) (xy 159.192301 91.043891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 159.442301 99.743891) (xy 157.992301 98.943891) (xy 160.042301 95.543891) (xy 161.242301 96.243891)
			)
		)
	)
	(zone
		(net 157)
		(net_name "Board_5-Net-(Q1-S)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.276957 87.893891) (xy 201.506957 87.893891) (xy 201.506957 85.443891) (xy 204.276957 85.443891)
			)
		)
	)
	(zone
		(net 34)
		(net_name "Board_1-ADC_LP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.807699 62.148953) (xy 134.707699 62.148953) (xy 134.707699 55.448953) (xy 139.007699 48.048953)
				(xy 141.407699 49.348953) (xy 137.807699 55.948953)
			)
		)
	)
	(zone
		(net 60)
		(net_name "Board_2-ADC_LN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.692355 46.248953) (xy 183.092355 47.648953) (xy 180.642355 51.898953) (xy 179.792355 51.448953)
				(xy 176.192355 49.348953) (xy 177.792355 46.748953) (xy 179.792355 47.848953)
			)
		)
	)
	(zone
		(net 91)
		(net_name "Board_3-ADC_SP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 101.507645 113.943891) (xy 101.507645 107.843891) (xy 99.707645 107.843891) (xy 99.707645 113.943891)
			)
		)
	)
	(zone
		(net 45)
		(net_name "Board_1-Net-(Q1-S)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.507699 59.098953) (xy 141.277699 59.098953) (xy 141.277699 61.548953) (xy 138.507699 61.548953)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.226957 83.343891) (xy 184.226957 81.643891) (xy 189.876957 81.643891) (xy 189.876957 83.343891)
			)
		)
	)
	(zone
		(net 112)
		(net_name "Board_3-VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.007645 91.643891) (xy 92.007645 85.743891) (xy 92.607645 85.743891) (xy 92.607645 87.743891)
				(xy 94.107645 87.743891) (xy 94.107645 91.643891)
			)
		)
	)
	(zone
		(net 38)
		(net_name "Board_1-Net-(J2-Pin_1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.107699 43.948953) (xy 135.007699 41.548953) (xy 132.207699 46.348953) (xy 133.907699 47.348953)
				(xy 134.807699 45.748953) (xy 137.207699 47.148953)
			)
		)
	)
	(zone
		(net 70)
		(net_name "Board_2-Net-(JP1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.092355 59.748953) (xy 197.342355 59.748953) (xy 197.342355 61.408953) (xy 198.592355 61.408953)
				(xy 198.592355 61.248953) (xy 204.092355 61.248953)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Board_0-Net-(JP1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.523043 59.748953) (xy 105.773043 59.748953) (xy 105.773043 61.408953) (xy 107.023043 61.408953)
				(xy 107.023043 61.248953) (xy 112.523043 61.248953)
			)
		)
	)
	(zone
		(net 42)
		(net_name "Board_1-Net-(JP1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.307699 59.748953) (xy 151.557699 59.748953) (xy 151.557699 61.408953) (xy 152.807699 61.408953)
				(xy 152.807699 61.248953) (xy 158.307699 61.248953)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Board_0-ADC_LN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 89.123043 46.248953) (xy 91.523043 47.648953) (xy 89.073043 51.898953) (xy 88.223043 51.448953)
				(xy 84.623043 49.348953) (xy 86.223043 46.748953) (xy 88.223043 47.848953)
			)
		)
	)
	(zone
		(net 119)
		(net_name "Board_4-ADC_SP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 147.292301 113.943891) (xy 147.292301 107.843891) (xy 145.492301 107.843891) (xy 145.492301 113.943891)
			)
		)
	)
	(zone
		(net 116)
		(net_name "Board_4-ADC_LN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 162.092301 100.743891) (xy 159.692301 99.343891) (xy 162.142301 95.093891) (xy 162.992301 95.543891)
				(xy 166.592301 97.643891) (xy 164.992301 100.243891) (xy 162.992301 99.143891)
			)
		)
	)
	(zone
		(net 146)
		(net_name "Board_5-ADC_LP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.976957 84.843891) (xy 208.076957 84.843891) (xy 208.076957 91.543891) (xy 203.776957 98.943891)
				(xy 201.376957 97.643891) (xy 204.976957 91.043891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 143.892301 85.743891) (xy 141.492301 85.743891) (xy 141.492301 83.943891) (xy 143.892301 83.943891)
			)
		)
	)
	(zone
		(net 94)
		(net_name "Board_3-Net-(J2-Pin_1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.107645 103.043891) (xy 116.207645 105.443891) (xy 119.007645 100.643891) (xy 117.307645 99.643891)
				(xy 116.407645 101.243891) (xy 114.007645 99.843891)
			)
		)
	)
	(zone
		(net 154)
		(net_name "Board_5-Net-(JP1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.476957 87.243891) (xy 191.226957 87.243891) (xy 191.226957 85.583891) (xy 189.976957 85.583891)
				(xy 189.976957 85.743891) (xy 184.476957 85.743891)
			)
		)
	)
	(zone
		(net 63)
		(net_name "Board_2-ADC_SP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 195.492355 33.048953) (xy 195.492355 39.148953) (xy 197.292355 39.148953) (xy 197.292355 33.048953)
			)
		)
	)
	(zone
		(net 101)
		(net_name "Board_3-Net-(Q1-S)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.707645 87.893891) (xy 109.937645 87.893891) (xy 109.937645 85.443891) (xy 112.707645 85.443891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.657645 99.743891) (xy 112.207645 98.943891) (xy 114.257645 95.543891) (xy 115.457645 96.243891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.773043 63.648953) (xy 112.773043 65.348953) (xy 107.123043 65.348953) (xy 107.123043 63.648953)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Board_0-+BATT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 105.856777 62.449156) (xy 105.473043 62.448953) (xy 105.473043 59.748953) (xy 98.423043 59.748953)
				(xy 98.423043 58.118953) (xy 97.773043 58.118953) (xy 97.773043 62.348953) (xy 95.723043 62.348953)
				(xy 95.723043 68.048953) (xy 98.823043 68.048953) (xy 105.823043 68.048953)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Board_0-ADC_SP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 103.923043 33.048953) (xy 103.923043 39.148953) (xy 105.723043 39.148953) (xy 105.723043 33.048953)
			)
		)
	)
	(zone
		(net 66)
		(net_name "Board_2-Net-(J2-Pin_1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.892355 43.948953) (xy 180.792355 41.548953) (xy 177.992355 46.348953) (xy 179.692355 47.348953)
				(xy 180.592355 45.748953) (xy 182.992355 47.148953)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.557699 63.648953) (xy 158.557699 65.348953) (xy 152.907699 65.348953) (xy 152.907699 63.648953)
			)
		)
	)
	(zone
		(net 141)
		(net_name "Board_5-+BATT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 191.143223 84.543688) (xy 191.526957 84.543891) (xy 191.526957 87.243891) (xy 198.576957 87.243891)
				(xy 198.576957 88.873891) (xy 199.226957 88.873891) (xy 199.226957 84.643891) (xy 201.276957 84.643891)
				(xy 201.276957 78.943891) (xy 198.176957 78.943891) (xy 191.176957 78.943891)
			)
		)
	)
	(zone
		(net 84)
		(net_name "Board_2-VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.992355 55.348953) (xy 204.992355 61.248953) (xy 204.392355 61.248953) (xy 204.392355 59.248953)
				(xy 202.892355 59.248953) (xy 202.892355 55.348953)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Board_0-ADC_LP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.023043 62.148953) (xy 88.923043 62.148953) (xy 88.923043 55.448953) (xy 93.223043 48.048953)
				(xy 95.623043 49.348953) (xy 92.023043 55.948953)
			)
		)
	)
	(zone
		(net 62)
		(net_name "Board_2-ADC_LP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.592355 62.148953) (xy 180.492355 62.148953) (xy 180.492355 55.448953) (xy 184.792355 48.048953)
				(xy 187.192355 49.348953) (xy 183.592355 55.948953)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.442301 83.343891) (xy 138.442301 81.643891) (xy 144.092301 81.643891) (xy 144.092301 83.343891)
			)
		)
	)
	(zone
		(net 73)
		(net_name "Board_2-Net-(Q1-S)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.292355 59.098953) (xy 187.062355 59.098953) (xy 187.062355 61.548953) (xy 184.292355 61.548953)
			)
		)
	)
	(zone
		(net 35)
		(net_name "Board_1-ADC_SP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 149.707699 33.048953) (xy 149.707699 39.148953) (xy 151.507699 39.148953) (xy 151.507699 33.048953)
			)
		)
	)
	(zone
		(net 168)
		(net_name "Board_5-VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.576957 91.643891) (xy 183.576957 85.743891) (xy 184.176957 85.743891) (xy 184.176957 87.743891)
				(xy 185.676957 87.743891) (xy 185.676957 91.643891)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 98.107645 85.743891) (xy 95.707645 85.743891) (xy 95.707645 83.943891) (xy 98.107645 83.943891)
			)
		)
	)
	(zone
		(net 149)
		(net_name "Board_5-GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.28)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 204.676941 78.993894)
					(mid 214.203236 84.493891)
					(end 214.20322 95.493894)
				)
				(arc
					(start 203.810915 113.493895)
					(mid 194.284637 118.993896)
					(end 184.758358 113.493895)
				)
				(arc
					(start 174.366053 95.493896)
					(mid 174.366056 84.493888)
					(end 183.892336 78.993894)
				)
			)
		)
	)
	(zone
		(net 121)
		(net_name "Board_4-GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.28)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 158.892285 78.993894)
					(mid 168.41858 84.493891)
					(end 168.418564 95.493894)
				)
				(arc
					(start 158.026259 113.493895)
					(mid 148.499981 118.993896)
					(end 138.973702 113.493895)
				)
				(arc
					(start 128.581397 95.493896)
					(mid 128.5814 84.493888)
					(end 138.10768 78.993894)
				)
			)
		)
	)
	(zone
		(net 9)
		(net_name "Board_0-GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.28)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 92.323059 67.99895)
					(mid 82.796764 62.498953)
					(end 82.79678 51.49895)
				)
				(arc
					(start 93.189085 33.498949)
					(mid 102.715363 27.998948)
					(end 112.241642 33.498949)
				)
				(arc
					(start 122.633947 51.498948)
					(mid 122.633944 62.498956)
					(end 113.107664 67.99895)
				)
			)
		)
	)
	(zone
		(net 37)
		(net_name "Board_1-GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.28)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 138.107715 67.99895)
					(mid 128.58142 62.498953)
					(end 128.581436 51.49895)
				)
				(arc
					(start 138.973741 33.498949)
					(mid 148.500019 27.998948)
					(end 158.026298 33.498949)
				)
				(arc
					(start 168.418603 51.498948)
					(mid 168.4186 62.498956)
					(end 158.89232 67.99895)
				)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Board_2-GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.28)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 183.892371 67.99895)
					(mid 174.366076 62.498953)
					(end 174.366092 51.49895)
				)
				(arc
					(start 184.758397 33.498949)
					(mid 194.284675 27.998948)
					(end 203.810954 33.498949)
				)
				(arc
					(start 214.203259 51.498948)
					(mid 214.203256 62.498956)
					(end 204.676976 67.99895)
				)
			)
		)
	)
	(zone
		(net 93)
		(net_name "Board_3-GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.28)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 113.107629 78.993894)
					(mid 122.633924 84.493891)
					(end 122.633908 95.493894)
				)
				(arc
					(start 112.241603 113.493895)
					(mid 102.715325 118.993896)
					(end 93.189046 113.493895)
				)
				(arc
					(start 82.796741 95.493896)
					(mid 82.796744 84.493888)
					(end 92.323024 78.993894)
				)
			)
		)
	)
	(embedded_fonts no)
)
