(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "LTO Battery Pack")
		(date "2025-08-26")
		(rev "C")
		(company "μArt.cz")
		(comment 1 "Vlastimil Slinták")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 151.6 117.45)
		(grid_origin 151.6 117.45)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VCC")
	(net 2 "GND")
	(footprint "LOGO"
		(layer "F.Cu")
		(at 151.6 110.45)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Parts:LTO_Battery_D19mm"
		(layer "B.Cu")
		(at 141.1 109.2 180)
		(property "Reference" "BT1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1S LTO"
			(at -0.2 -4.2 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at -0.1 -9 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Single-cell battery"
			(at -0.1 -9 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "lto-pack-revC.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 4 0 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -4 0 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/lto_battery_D19mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Parts:SMTSO30"
		(layer "B.Cu")
		(at 163.6 96.2 150)
		(descr "M3X1.5 Tin Plated - Patch round nut")
		(property "Reference" "J2"
			(at 0 4 330)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -4 330)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 330)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 330)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C2915632"
			(at 0 0 150)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "lto-pack-revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -5.5 330)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 150)
			(size 6.2 6.2)
			(drill 4.22)
			(layers "*.Cu" "B.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_paste_margin_ratio -0.02)
		)
		(embedded_fonts no)
	)
	(footprint "Parts:SMTSO30"
		(layer "B.Cu")
		(at 151.6 117.45 180)
		(descr "M3X1.5 Tin Plated - Patch round nut")
		(property "Reference" "J1"
			(at 0 4 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "BATT"
			(at 0 -4 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C2915632"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "lto-pack-revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -5.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 6.2 6.2)
			(drill 4.22)
			(layers "*.Cu" "B.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_paste_margin_ratio -0.02)
		)
		(embedded_fonts no)
	)
	(footprint "Parts:LTO_Battery_D19mm"
		(layer "B.Cu")
		(at 162.1 109.2 180)
		(property "Reference" "BT2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1S LTO"
			(at -0.2 -4.2 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at -0.1 -9 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Single-cell battery"
			(at -0.1 -9 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "lto-pack-revC.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 4 0 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -4 0 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/lto_battery_D19mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Parts:LTO_Battery_D19mm"
		(layer "B.Cu")
		(at 151.6 91 180)
		(property "Reference" "BT3"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1S LTO"
			(at -0.2 -4.2 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at -0.1 -9 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Single-cell battery"
			(at -0.1 -9 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "lto-pack-revC.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 4 0 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -4 0 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Parts.3dshapes/lto_battery_D19mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(gr_line
		(start 141.1 120.2)
		(end 161.884605 120.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.966026 85.699999)
		(end 131.573721 103.7)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.410888 103.699998)
		(mid 171.410887 114.700003)
		(end 161.884605 120.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 141.1 120.2)
		(mid 131.573721 114.7)
		(end 131.573721 103.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.410888 103.699998)
		(end 161.018583 85.699999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 141.966026 85.699999)
		(mid 151.492305 80.199998)
		(end 161.018583 85.699999)
		(layer "Edge.Cuts")
	)
	(gr_text "Rev${REVISION}, ${ISSUE_DATE}\n${COMPANY}, ${COMMENT1}"
		(at 137.7 100.95 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 156.1 119 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 147.1 119 0)
		(layer "F.SilkS")
	)
	(gr_text "${TITLE}\n1S3P  1.5-2.8 V"
		(at 151.6 107.2 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 167.1 99.45 120)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 162.6 91.45 120)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 121.1 122.2) (xy 152.1 68.2) (xy 183.1 122.2)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 161.800962 101.347114) (xy 158.300962 95.284936) (xy 164.430127 91.784936) (xy 167.930127 97.847114)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 121.1 122.2) (xy 183.1 122.2) (xy 152.1 68.2)
			)
		)
	)
	(zone
		(net 1)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 148.1 113.45) (xy 155.1 113.45) (xy 155.1 119.95) (xy 148.1 119.95)
			)
		)
	)
	(embedded_fonts no)
)
