(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "The New Packet Radio (NPR)")
		(date "2025-06-13")
		(rev "B")
		(company "µArt.cz")
		(comment 1 "Vlastimil Slinták (OK5VAS)")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 183.225 135.75)
		(grid_origin 183.225 135.75)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3V3")
	(net 3 "/AVDD")
	(net 4 "Net-(U2-NRST)")
	(net 5 "Net-(U2-PC14)")
	(net 6 "Net-(U2-PC15)")
	(net 7 "/Ethernet/WZNT_DVCC")
	(net 8 "Net-(J5-RD+)")
	(net 9 "Net-(C11-Pad2)")
	(net 10 "Net-(C12-Pad2)")
	(net 11 "Net-(J5-RD-)")
	(net 12 "Net-(J5-TCT)")
	(net 13 "Net-(J5-RCT)")
	(net 14 "Net-(U3-XI{slash}CLKIN)")
	(net 15 "Net-(U3-XO)")
	(net 16 "Net-(U3-1V2O)")
	(net 17 "Net-(U3-TOCAP)")
	(net 18 "/Ethernet/WZNT_AVCC")
	(net 19 "Net-(U4-VCC)")
	(net 20 "+5V")
	(net 21 "Net-(U5-EN)")
	(net 22 "Net-(D1-K)")
	(net 23 "/LED_RX")
	(net 24 "Net-(D2-K)")
	(net 25 "Net-(D3-K)")
	(net 26 "/LED_CON")
	(net 27 "Net-(D4-K)")
	(net 28 "Net-(J8-Pin_2)")
	(net 29 "/TXD")
	(net 30 "/RXD")
	(net 31 "Net-(J3-Pin_3)")
	(net 32 "Net-(J2-Pin_1)")
	(net 33 "/Ethernet/ACT_LED")
	(net 34 "Net-(J2-Pin_3)")
	(net 35 "unconnected-(J2-Pin_5-Pad5)")
	(net 36 "/Ethernet/LINK_LED")
	(net 37 "Net-(J4-Pin_3)")
	(net 38 "/Power/VBUS")
	(net 39 "Net-(J4-Pin_1)")
	(net 40 "Net-(U7-V3)")
	(net 41 "Net-(J5-TD-)")
	(net 42 "unconnected-(J5-NC-Pad7)")
	(net 43 "Net-(J5-TD+)")
	(net 44 "Net-(U5-L2)")
	(net 45 "Net-(U5-L1)")
	(net 46 "Net-(Q1-B)")
	(net 47 "/LED_TX")
	(net 48 "Net-(U1-SIO1)")
	(net 49 "/SPI1_MISO")
	(net 50 "Net-(U1-SIO3)")
	(net 51 "Net-(U2-PH3)")
	(net 52 "Net-(U2-PA2)")
	(net 53 "/Radio/GPIO_{0}")
	(net 54 "/GPIO_{11}")
	(net 55 "/GPIO_{10}")
	(net 56 "Net-(U2-PA5)")
	(net 57 "/Radio/CLK")
	(net 58 "Net-(U2-PA7)")
	(net 59 "/Radio/MOSI")
	(net 60 "Net-(U2-PB3)")
	(net 61 "/SPI1_CLK")
	(net 62 "Net-(U2-PB5)")
	(net 63 "/SPI1_MOSI")
	(net 64 "Net-(U2-PA13)")
	(net 65 "Net-(U2-PA14)")
	(net 66 "Net-(U2-PA15)")
	(net 67 "Net-(U3-TXN)")
	(net 68 "Net-(U3-TXP)")
	(net 69 "Net-(U3-MISO)")
	(net 70 "Net-(U3-RXN)")
	(net 71 "Net-(U3-RXP)")
	(net 72 "Net-(U3-PMODE2)")
	(net 73 "Net-(U3-PMODE1)")
	(net 74 "Net-(U3-PMODE0)")
	(net 75 "Net-(U3-LINKLED)")
	(net 76 "Net-(U3-ACTLED)")
	(net 77 "Net-(U3-EXRES1)")
	(net 78 "Net-(J7-Pin_1)")
	(net 79 "Net-(J9-CC2)")
	(net 80 "Net-(R42-Pad2)")
	(net 81 "Net-(R43-Pad2)")
	(net 82 "Net-(R44-Pad2)")
	(net 83 "/Radio/MISO")
	(net 84 "Net-(U4-SDO)")
	(net 85 "unconnected-(J9-SBU2-PadB8)")
	(net 86 "Net-(U5-FB)")
	(net 87 "Net-(J9-CC1)")
	(net 88 "/SRAM_CS")
	(net 89 "unconnected-(U1-SIO2-Pad3)")
	(net 90 "/RF_SDN")
	(net 91 "/Radio/~{CS}")
	(net 92 "/RF_INT")
	(net 93 "unconnected-(U3-VBG-Pad18)")
	(net 94 "unconnected-(U3-NC-Pad46)")
	(net 95 "unconnected-(U3-SPDLED-Pad24)")
	(net 96 "unconnected-(U3-DUPLED-Pad26)")
	(net 97 "unconnected-(U3-RSVD-Pad23)")
	(net 98 "unconnected-(U3-NC-Pad47)")
	(net 99 "unconnected-(U3-DNC-Pad7)")
	(net 100 "unconnected-(U3-NC-Pad13)")
	(net 101 "unconnected-(U3-NC-Pad12)")
	(net 102 "unconnected-(J9-SBU1-PadA8)")
	(net 103 "Net-(R45-Pad2)")
	(net 104 "Net-(R46-Pad2)")
	(net 105 "Net-(R49-Pad2)")
	(net 106 "Net-(R52-Pad1)")
	(net 107 "/Ethernet/ETH_GND")
	(net 108 "unconnected-(U4-NC-Pad4)")
	(net 109 "unconnected-(U4-NC-Pad14)")
	(net 110 "unconnected-(U4-NC-Pad3)")
	(net 111 "/ETH_INT")
	(net 112 "/Ethernet/~{CS}")
	(net 113 "Net-(U2-PA3)")
	(net 114 "/Ethernet/~{RST}")
	(net 115 "/PA12")
	(net 116 "/PA11")
	(net 117 "/Power/D+")
	(net 118 "/Power/D-")
	(net 119 "unconnected-(U7-~{CTS}-Pad5)")
	(net 120 "unconnected-(U7-~{RTS}-Pad6)")
	(net 121 "unconnected-(U7-~{DTR}-Pad4)")
	(net 122 "Net-(D1-A)")
	(net 123 "/Radio/ANT1")
	(net 124 "/Radio/ANT2")
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 137.8 83.15)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -0.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "Net-(U1-SIO3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 124.8375 76.1 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at -3.15 -0.0625 90)
			(layer "F.SilkS")
		)
		(property "Value" "100u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15008"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 20 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 131.16 94.8)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 1.74 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U3-XO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U3-XI{slash}CLKIN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 140.81 126.005 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 2.395 -0.04 90)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C12246"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "Net-(U3-ACTLED)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Ethernet/ACT_LED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.4315 79.36 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 0.09 -5.8185 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U5-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_CK_RS282G05A3"
		(layer "F.Cu")
		(at 151.0375 76.25 180)
		(descr "https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf")
		(tags "SPST button tactile switch")
		(property "Reference" "SW1"
			(at 0 -2.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "RESET"
			(at 0 3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C483808"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.6 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.9 0 180)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.9 0 180)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(U2-NRST)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 151.2 98.41)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J4"
			(at 0.9 -1.86 0)
			(layer "F.SilkS")
		)
		(property "Value" "SWD"
			(at 0 7.41 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr through_hole exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 153.445 126.64 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R53"
			(at -0.01 0.98 90)
			(layer "F.SilkS")
		)
		(property "Value" "5k1"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "Net-(J9-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 144.325 110.67 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 1.52 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Net-(U7-V3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 133.245 111.03 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0.12 -3.08 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 150.69 95.95)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0.01 -0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(U2-PA14)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "Net-(J4-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 133.445 96.62 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 1.855 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Taiyo-Yuden_MD-3030"
		(layer "F.Cu")
		(at 129.6375 72.18 180)
		(descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-3030, 3.0mmx3.0mm")
		(tags "inductor taiyo-yuden md smd")
		(property "Reference" "L1"
			(at 0 2.13 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5159665"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(U5-L2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "Net-(U5-L1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Taiyo-Yuden_MD-3030.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 130.4295 79.38 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R52"
			(at -0.07 5.5205 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "Net-(R52-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Net-(U5-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 121.41 117.07 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 1.92 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C318577"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J5-TCT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 150.395 126.64 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R51"
			(at 0 -0.87 90)
			(layer "F.SilkS")
		)
		(property "Value" "5k1"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "Net-(J9-CC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 173.7475 42.55)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0.1025 1 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k1"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "Net-(Q1-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/LED_TX")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 132.445 96.62 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 1.955 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 123.3 64.05 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.33 180)
			(layer "F.SilkS")
		)
		(property "Value" "POWER JACK"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C492401"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "Net-(J7-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_901-143_Horizontal"
		(layer "F.Cu")
		(at 174.225 131.25 180)
		(descr "Amphenol RF 901-143 https://www.amphenolrf.com/library/download/link/link_id/593645/parent/901-143/")
		(tags "SMA THT Female Jack Horizontal")
		(property "Reference" "J6"
			(at 3.65 4.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "Antenna"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C411575"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 4.3 -4.5)
			(end -4.3 -4.5)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.3 2.3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(roundrect_rratio 0.087)
			(net 124 "/Radio/ANT2")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54 180)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54 180)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54 180)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54 180)
			(size 2.5 2.5)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-143_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/Parts.3dshapes/Amphenol_901143.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 134.5 76.075 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0.175 -1.85 180)
			(layer "F.SilkS")
		)
		(property "Value" "100u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15008"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 140.7 87.05)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -2.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/SPI1_CLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(U2-PA5)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 140.725 90.6 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 1.825 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/SRAM_CS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.885 100.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at -1.815 -0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "Net-(R43-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 150.65 86.65 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -1.875 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(U2-PH3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 131.4335 79.38 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at 0.07 -5.3665 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Net-(U5-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "Net-(R49-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 126.8275 75.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at -2.35 -0.0225 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 131.29875 113.57 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 4.65125 90)
			(layer "F.SilkS")
		)
		(property "Value" "6.8n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C93654"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J5-RD+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 133.845 92.62 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 1.82 0.005 90)
			(layer "F.SilkS")
		)
		(property "Value" "12p"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U3-XI{slash}CLKIN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 137.545 93.8 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB3"
			(at 2.35 -0.005 90)
			(layer "F.SilkS")
		)
		(property "Value" "600Ω@100MHz"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19330"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 152.975 115.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 1.825 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U4-VCC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 122.4275 71.85 90)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at 0 -1.5275 180)
			(layer "F.SilkS")
		)
		(property "Value" "BSMD0805-100-6V"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C883112"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*polyfuse* *PTC*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(J8-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 143.025 92.93 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.37 -0.025 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.284375 113.55 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 -4.515625 90)
			(layer "F.SilkS")
		)
		(property "Value" "50R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C227387"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J5-RCT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 135.245 111.03 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0.12 -3.18 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.845 96.6 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0.6 -2.645 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/ETH_INT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.885 98.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at -0.015 0.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/Ethernet/~{RST}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 138.81 94.27 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 1.72 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.30625 113.55 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0.1 -3.85625 90)
			(layer "F.SilkS")
		)
		(property "Value" "10R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25139"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(J5-TD-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(U3-TXN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 128.311875 113.55 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at -0.1 4.061875 90)
			(layer "F.SilkS")
		)
		(property "Value" "50R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C227387"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(J5-TD-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 168.7475 38.45)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0.0025 1 0)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C12246"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 125.295 113.55 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at -0.1 3.445 90)
			(layer "F.SilkS")
		)
		(property "Value" "50R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C227387"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(J5-TD+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 140.7 85.05 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 2.775 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(U2-PA2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/TXD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.875 99.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at -1.815 -0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Net-(R42-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 173.225 39.8375 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 2.35 180)
			(layer "F.SilkS")
		)
		(property "Value" "BC847"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C57668"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(D1-K)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_6.3x5.4"
		(layer "F.Cu")
		(at 136.95 69.15 90)
		(descr "SMD capacitor, aluminum electrolytic, Panasonic C55, 6.3x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C36"
			(at -4.3 1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "220u"
			(at 0 4.35 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2833309"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8 0 90)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.8 0 90)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12"
		(layer "F.Cu")
		(at 151.975 133.05)
		(descr "USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf")
		(tags "usb usb-c 2.0 pd")
		(property "Reference" "J9"
			(at 5.775 -0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "TYPE-C-31-M-12"
			(at 0 5.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C165948"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.6)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.6)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -3.25 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A4" smd rect
			(at -2.45 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "/Power/VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" smd rect
			(at -1.25 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "Net-(J9-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "/Power/D+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" smd rect
			(at 0.25 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "/Power/D-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" smd rect
			(at 1.25 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "unconnected-(J9-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
		)
		(pad "A9" smd rect
			(at 2.45 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "/Power/VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" smd rect
			(at 3.25 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" smd rect
			(at 3.25 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B4" smd rect
			(at 2.45 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "/Power/VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" smd rect
			(at 1.75 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "Net-(J9-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.75 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "/Power/D+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" smd rect
			(at -0.75 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "/Power/D-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" smd rect
			(at -1.75 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(J9-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
		)
		(pad "B9" smd rect
			(at -2.45 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "/Power/VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" smd rect
			(at -3.25 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.13)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.05)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.13)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.05)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_HRO_TYPE-C-31-M-12.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/Parts.3dshapes/HRO_TYPE-C-31-M-12.step"
			(offset
				(xyz -4.45 -3.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_6.3x5.4"
		(layer "F.Cu")
		(at 122.5 82.95 -90)
		(descr "SMD capacitor, aluminum electrolytic, Panasonic C55, 6.3x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C31"
			(at -4.1 2.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "220u"
			(at 0 4.35 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2833309"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8 0 270)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 20 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.8 0 270)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 177.5125 124.75 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 2.0875 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "20nH"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C17702828"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "/Radio/ANT1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "/Radio/ANT2")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 136.01 93.8 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB2"
			(at -0.1 1.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "600Ω@100MHz"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19330"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 142.725 51.55 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -0.02 -0.925 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/GPIO_{11}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_3215-2Pin_3.2x1.5mm"
		(layer "F.Cu")
		(at 147.025 81.6125 180)
		(descr "SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf")
		(tags "SMD SMT Crystal")
		(property "Reference" "Y1"
			(at 0 1.4125 0)
			(layer "F.SilkS")
		)
		(property "Value" "NX3215SA-32.768k"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C156244"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.25 0 180)
			(size 1 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U2-PC15)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.25 0 180)
			(size 1 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(U2-PC14)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3215-2Pin_3.2x1.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 152 90.65)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 1.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "Net-(U2-PB3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/Radio/CLK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.865 105.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at 1.815 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Net-(U3-PMODE1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.875 106.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at 1.815 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "Net-(U3-PMODE0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.925 83.685 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 1.335 -0.025 180)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/SPI1_MISO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(U1-SIO1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 139.81 126.005 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 2.395 0.21 90)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C12246"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Net-(U3-LINKLED)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Ethernet/LINK_LED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 140.125 82.75 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB1"
			(at -1.95 -0.075 180)
			(layer "F.SilkS")
		)
		(property "Value" "600Ω@100MHz"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19330"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/AVDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 140.7 88.95)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -0.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/SPI1_MOSI")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Net-(U2-PA7)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 123.3 67.75 90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J8"
			(at 0 -2.33 180)
			(layer "F.SilkS")
		)
		(property "Value" "POWER SELECT"
			(at 0 7.41 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2937625"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "Net-(J7-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J8-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/Power/VBUS")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 129.3075 111.65 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 1.3 0.3925 180)
			(layer "F.SilkS")
		)
		(property "Value" "10R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25139"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(C12-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(U3-RXN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 176.245 123.35 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0.02 0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "6.8pF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C88896"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "/Radio/ANT2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 149.725 81.6125 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -1.5625 0.025 90)
			(layer "F.SilkS")
		)
		(property "Value" "6p"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C700515"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U2-PC14)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Parts:RF4463F30"
		(layer "F.Cu")
		(at 156.8 116.75 180)
		(property "Reference" "U4"
			(at 1 -2.15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RF4463F30"
			(at -10.2 14.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.nicerf.com/fsk-front-end-module/1w-rf-module-rf4463f30.html"
			(at -11.2 14.2 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1W Si4463 RF Module With Amplifier And LNA"
			(at -11.2 14.2 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5356658"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -8.7 14.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 19 "Net-(U4-VCC)")
			(pinfunction "VCC")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 0 4 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 0 8 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 110 "unconnected-(U4-NC-Pad3)")
			(pinfunction "NC")
			(pintype "free")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 0 12 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 108 "unconnected-(U4-NC-Pad4)")
			(pinfunction "NC")
			(pintype "free")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 0 16 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 90 "/RF_SDN")
			(pinfunction "SDN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0 20 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 92 "/RF_INT")
			(pinfunction "~{IRQ}")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at 0 24 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 91 "/Radio/~{CS}")
			(pinfunction "~{CS}")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at 0 28 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd roundrect
			(at -20 28 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 57 "/Radio/CLK")
			(pinfunction "SCK")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd roundrect
			(at -20 24 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 59 "/Radio/MOSI")
			(pinfunction "SDI")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "11" smd roundrect
			(at -20 20 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 84 "Net-(U4-SDO)")
			(pinfunction "SDO")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "12" smd roundrect
			(at -20 16 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 47 "/LED_TX")
			(pinfunction "GPIO_{1}")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "13" smd roundrect
			(at -20 12 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 53 "/Radio/GPIO_{0}")
			(pinfunction "GPIO_{0}")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
		)
		(pad "14" smd roundrect
			(at -20 8 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 109 "unconnected-(U4-NC-Pad14)")
			(pinfunction "NC")
			(pintype "free")
			(thermal_bridge_angle 45)
		)
		(pad "15" smd roundrect
			(at -20 4 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "16" smd roundrect
			(at -20 0 180)
			(size 3 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 123 "/Radio/ANT1")
			(pinfunction "ANT")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 129.945 96.6 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0.6 -2.995 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/Ethernet/~{CS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 152 89.65)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at 1.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/Radio/MISO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Net-(U4-SDO)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 120.51 127.375 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -2.975 -0.04 180)
			(layer "F.SilkS")
		)
		(property "Value" "1nF/2kV"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C23631"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 107 "/Ethernet/ETH_GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 120.415 117.07 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 1.92 -0.015 90)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C318577"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J5-TCT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 119.41 117.05 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at -1.9 -0.04 90)
			(layer "F.SilkS")
		)
		(property "Value" "10R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25139"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J5-TCT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.495 92.62 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 1.82 0.005 90)
			(layer "F.SilkS")
		)
		(property "Value" "12p"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U3-XO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 133.28 113.57 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0.02 4.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C318577"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J5-RCT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 126.300625 113.55 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0.1 -3.650625 90)
			(layer "F.SilkS")
		)
		(property "Value" "10R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25139"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(J5-TD+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Net-(U3-TXP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
		(layer "F.Cu")
		(at 146.075 88.75 -90)
		(descr "QFN, 32 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_32_05-08-1693.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U2"
			(at -3.35 -2.325 0)
			(layer "F.SilkS")
		)
		(property "Value" "STM32L432KCUx"
			(at 0 3.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l432kc.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M4 MCU, 256KB flash, 64KB RAM, 80 MHz, 1.71-3.6V, 26 GPIO, UFQFPN32"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1337280"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*5x5mm*P0.5mm*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -1.15 -1.15 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1.15 0 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1.15 1.15 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 -1.15 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 1.15 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.15 -1.15 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.15 0 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.15 1.15 270)
			(size 0.93 0.93)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.4375 -1.75 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.4375 -1.25 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U2-PC14)")
			(pinfunction "PC14")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.4375 -0.75 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-PC15)")
			(pinfunction "PC15")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.4375 -0.25 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(U2-NRST)")
			(pinfunction "NRST")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.4375 0.25 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/AVDD")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.4375 0.75 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/GPIO_{10}")
			(pinfunction "PA0")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.4375 1.25 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/GPIO_{11}")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -2.4375 1.75 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(U2-PA2)")
			(pinfunction "USART2_TX")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -1.75 2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "Net-(U2-PA3)")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -1.25 2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/LED_CON")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -0.75 2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(U2-PA5)")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -0.25 2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/SPI1_MISO")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 0.25 2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Net-(U2-PA7)")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 0.75 2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/SRAM_CS")
			(pinfunction "PB0")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 1.25 2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/ETH_INT")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 1.75 2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "17" smd roundrect
			(at 2.4375 1.75 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "18" smd roundrect
			(at 2.4375 1.25 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/Ethernet/~{CS}")
			(pinfunction "PA8")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 2.4375 0.75 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "/RF_INT")
			(pinfunction "PA9")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 2.4375 0.25 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/RF_SDN")
			(pinfunction "PA10")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 2.4375 -0.25 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/PA11")
			(pinfunction "PA11")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 2.4375 -0.75 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "/PA12")
			(pinfunction "PA12")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at 2.4375 -1.25 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U2-PA13)")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at 2.4375 -1.75 270)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(U2-PA14)")
			(pinfunction "PA14")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at 1.75 -2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Net-(U2-PA15)")
			(pinfunction "USART2_RX")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 1.25 -2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "Net-(U2-PB3)")
			(pinfunction "PB3")
			(pintype "bidirectional")
		)
		(pad "27" smd roundrect
			(at 0.75 -2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/Radio/MISO")
			(pinfunction "PB4")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at 0.25 -2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Net-(U2-PB5)")
			(pinfunction "PB5")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at -0.25 -2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/Radio/~{CS}")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at -0.75 -2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/LED_RX")
			(pinfunction "PB7")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at -1.25 -2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(U2-PH3)")
			(pinfunction "PH3")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at -1.75 -2.4375 270)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 0 0 270)
			(size 3.45 3.45)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 138.41 104.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 5.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.225 51.23 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -0.975 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/Radio/GPIO_{0}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(J3-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 129.4255 79.38 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R54"
			(at -0.07 5.6745 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "Net-(R52-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 132.525 83.785)
		(descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOP SO")
		(property "Reference" "U1"
			(at -3.675 -2.685 0)
			(layer "F.SilkS")
		)
		(property "Value" "23LC1024"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/23A102423LC1024-1-Mbit-SPI-Serial-SRAM-with-SDI-SQI-Interface-20005142.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1-Mbit SPI Serial SRAM with SDI and SQI Interface"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C48388"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.625 -1.905)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/SRAM_CS")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.625 -0.635)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(U1-SIO1)")
			(pinfunction "SO")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.625 0.635)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "unconnected-(U1-SIO2-Pad3)")
			(pinfunction "SIO2")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" smd roundrect
			(at -2.625 1.905)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.625 1.905)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/SPI1_MOSI")
			(pinfunction "SI")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 2.625 0.635)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/SPI1_CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.625 -0.635)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "Net-(U1-SIO3)")
			(pinfunction "~{HOLD}")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.625 -1.905)
			(size 1.65 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 159.025 37.05)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D4"
			(at -2.275 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2286"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 164.025 37.05)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 2.125 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2286"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/LED_CON")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:Texas_DRC0010J_ThermalVias"
		(layer "F.Cu")
		(at 129.6375 76.25 -90)
		(descr "Texas DRC0010J, VSON10 3x3mm Body, 0.5mm Pitch,  http://www.ti.com/lit/ds/symlink/tps63000.pdf")
		(tags "Texas VSON10 3x3mm")
		(property "Reference" "U5"
			(at 1.55 -2.4125 180)
			(layer "F.SilkS")
		)
		(property "Value" "TPS63000"
			(at 0.02032 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63000.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 1.8A Switch Current, Adjustable 1.2-5.5V Output Voltage, VSON-10"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C24966"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Texas*DRC0010J*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.25 -1.53 270)
			(size 0.25 0.34)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at -0.25 1.53 270)
			(size 0.25 0.34)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at 0 -0.63 270)
			(size 1.5 1.06)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at 0 0.63 270)
			(size 1.5 1.06)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at 0.25 -1.53 270)
			(size 0.25 0.34)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at 0.25 1.53 270)
			(size 0.25 0.34)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "1" smd roundrect
			(at -1.4 -1 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -1.4 -0.5 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(U5-L2)")
			(pinfunction "L2")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.4 0 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -1.4 0.5 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U5-L1)")
			(pinfunction "L1")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -1.4 1 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+5V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.4 1 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U5-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 1.4 0.5 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U5-EN)")
			(pinfunction "PS/SYNC")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 1.4 0 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U5-EN)")
			(pinfunction "VINA")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 1.4 -0.5 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 1.4 -1 270)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Net-(U5-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at -0.575 0 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 -0.95 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "11" smd custom
			(at 0 0 270)
			(size 1.65 2.4)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.125 -1.1) (xy 0.125 -1.1) (xy 0.125 -1.7) (xy 0.375 -1.7) (xy 0.375 1.7) (xy 0.125 1.7)
						(xy 0.125 1.1) (xy -0.125 1.1) (xy -0.125 1.7) (xy -0.375 1.7) (xy -0.375 -1.7) (xy -0.125 -1.7)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "11" thru_hole circle
			(at 0 0.95 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0.575 0 270)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_DRC0010J.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/Parts.3dshapes/TPS63000.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 169.025 37.05)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 2.125 -0.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2286"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/LED_RX")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 152.825 110.55)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB4"
			(at 0.425 -1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "600Ω@100MHz"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19330"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U4-VCC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 144.325 81.6125 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -1.5625 -0.025 90)
			(layer "F.SilkS")
		)
		(property "Value" "6p"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C700515"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-PC15)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 147.325 110.67 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at -1.52 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/Power/VBUS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 138.41 102.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 5.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "4u7"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C23733"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(U3-TOCAP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 129.3075 113.57 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 4.9425 90)
			(layer "F.SilkS")
		)
		(property "Value" "6.8n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C93654"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(J5-RD-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(C12-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 140.7 86.05)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -2.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/Ethernet/~{RST}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "Net-(U2-PA3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.4375 79.38 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at 0.07 -5.2125 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "Net-(R49-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 138.41 100.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 5.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C318577"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U3-1V2O)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 130.303125 113.55 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0 -4.796875 90)
			(layer "F.SilkS")
		)
		(property "Value" "50R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C227387"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(C12-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J5-RCT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 150.65 85.65)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.575 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 132.4375 75.58 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at -2.43 0.0375 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 141.725 83.05 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 1.55 0.025 270)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/AVDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 166.8 47.05)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 145.325 51.55 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -0.02 -0.925 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/GPIO_{10}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Net-(J2-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 152 88.65)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 1.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Net-(U2-PB5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/Radio/MOSI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:Texas_DRT-3"
		(layer "F.Cu")
		(at 151.975 125.75)
		(descr "Texas Instrument DRT-3 1x0.8mm Pitch 0.7mm http://www.ti.com/lit/ds/symlink/tpd2eusb30.pdf")
		(tags "DRT-3 1x0.8mm Pitch 0.7mm")
		(property "Reference" "U6"
			(at -0.005 1.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "TPD2EUSB30"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2eusb30a.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-Channel ESD Protection for Super-Speed USB 3.0 Interface, DRT-3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C97502"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Texas*DRT*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.35 0.425)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "/Power/D+")
			(pinfunction "D+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.35 0.425)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/Power/D-")
			(pinfunction "D-")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0 -0.425)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Texas_DRT-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 129.825 51.23 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 0.925 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.311875 111.03 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at -1.33 0.711875 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.865 103.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at -1.815 -0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "Net-(R46-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 136.4 89.825 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0.025 -1.4 270)
			(layer "F.SilkS")
		)
		(property "Value" "100u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15008"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 163.7475 38.45)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C12246"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(D3-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.875 101.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at -1.815 -0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "Net-(R44-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 158.7475 38.45)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0.0025 1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C12246"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(D4-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.885 104.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 2.585 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "Net-(U3-PMODE2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 152.975 114.195 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 1.825 -0.005 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U4-VCC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SSOP-10-1EP_3.9x4.9mm_P1mm_EP2.1x3.3mm"
		(layer "F.Cu")
		(at 146.325 116.65 90)
		(descr "SSOP, 10 Pin (http://download.py32.org/%E6%95%B0%E6%8D%AE%E6%89%8B%E5%86%8C/zh-CN/PY32F002A%20%E7%B3%BB%E5%88%97%E6%95%B0%E6%8D%AE%E6%89%8B%E5%86%8C_Rev1.0.pdf#page=44), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SSOP SO ESSOP-10")
		(property "Reference" "U7"
			(at -1.5 -3.6 180)
			(layer "F.SilkS")
		)
		(property "Value" "CH340K"
			(at 0 3.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn.sparkfun.com/assets/5/0/a/8/5/CH340DS1.PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB serial converter, UART, SSOP-10"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C18208922"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*1EP*3.9x4.9mm*P1mm*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 0 90)
			(size 1.69 2.66)
			(layers "F.Paste")
			(roundrect_rratio 0.147929)
		)
		(pad "1" smd roundrect
			(at -2.6375 -2 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "/Power/D+")
			(pinfunction "UD+")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -2.6375 -1 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/Power/D-")
			(pinfunction "UD-")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.6375 0 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.6375 1 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "unconnected-(U7-~{DTR}-Pad4)")
			(pinfunction "~{DTR}")
			(pintype "output+no_connect")
		)
		(pad "5" smd roundrect
			(at -2.6375 2 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "unconnected-(U7-~{CTS}-Pad5)")
			(pinfunction "~{CTS}")
			(pintype "input+no_connect")
		)
		(pad "6" smd roundrect
			(at 2.6375 2 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "unconnected-(U7-~{RTS}-Pad6)")
			(pinfunction "~{RTS}")
			(pintype "output+no_connect")
		)
		(pad "7" smd roundrect
			(at 2.6375 1 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/Power/VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.6375 0 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/RXD")
			(pinfunction "TXD")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at 2.6375 -1 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/TXD")
			(pinfunction "RXD")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.6375 -2 90)
			(size 1.675 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Net-(U7-V3)")
			(pinfunction "V3")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0 0 90)
			(size 2.1 3.3)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-10-1EP_3.9x4.9mm_P1.0mm_EP2.1x3.3mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 138.41 101.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 5.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 174.025 37.05)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at -2.1 0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2286"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 142.725 83.05 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -1.55 -0.025 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(U2-NRST)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 124.725 48.08 90)
		(descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole horizontal IDC box header THT 2x03 2.54mm double row")
		(property "Reference" "J3"
			(at 3.33 9.775 180)
			(layer "F.SilkS")
		)
		(property "Value" "GPIO"
			(at 6.215 11.18 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C34945"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.83 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "+3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 152 112.5 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 1.72 1.52 180)
			(layer "F.SilkS")
		)
		(property "Value" "100u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15008"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 19 "Net-(U4-VCC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-48_7x7mm_P0.5mm"
		(layer "F.Cu")
		(at 131.21 103.2375 90)
		(descr "LQFP, 48 Pin (JEDEC MS-026 variation BBC, 1.40mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MS-026, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-lqfp/05081760_a_lx48.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP CASE-932AA CASE-932-03 C48-1 C48-2 C48-3 C48-5 C48-6 C48-6C PT0048A")
		(property "Reference" "U3"
			(at -3.8125 -4.51 180)
			(layer "F.SilkS")
		)
		(property "Value" "W5500"
			(at 0 5.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://wizwiki.net/wiki/lib/exe/fetch.php/products:w5500:w5500_ds_v109e.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10/100Mb SPI Ethernet controller with TCP/IP stack, LQFP-48"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C32843"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LQFP*7x7mm*P0.5mm*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.1625 -2.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(U3-TXN)")
			(pinfunction "TXN")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -4.1625 -2.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Net-(U3-TXP)")
			(pinfunction "TXP")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -4.1625 -1.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -4.1625 -1.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pinfunction "AVDD")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -4.1625 -0.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(U3-RXN)")
			(pinfunction "RXN")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -4.1625 -0.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "Net-(U3-RXP)")
			(pinfunction "RXP")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -4.1625 0.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "unconnected-(U3-DNC-Pad7)")
			(pinfunction "DNC")
			(pintype "no_connect")
		)
		(pad "8" smd roundrect
			(at -4.1625 0.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pinfunction "AVDD")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -4.1625 1.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at -4.1625 1.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Net-(U3-EXRES1)")
			(pinfunction "EXRES1")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at -4.1625 2.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pinfunction "AVDD")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at -4.1625 2.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "unconnected-(U3-NC-Pad12)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "13" smd roundrect
			(at -2.75 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "unconnected-(U3-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "14" smd roundrect
			(at -2.25 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at -1.75 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pinfunction "AVDD")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at -1.25 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "passive")
		)
		(pad "17" smd roundrect
			(at -0.75 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pinfunction "AVDD")
			(pintype "passive")
		)
		(pad "18" smd roundrect
			(at -0.25 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "unconnected-(U3-VBG-Pad18)")
			(pinfunction "VBG")
			(pintype "passive+no_connect")
		)
		(pad "19" smd roundrect
			(at 0.25 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at 0.75 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(U3-TOCAP)")
			(pinfunction "TOCAP")
			(pintype "passive")
		)
		(pad "21" smd roundrect
			(at 1.25 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pinfunction "AVDD")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 1.75 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U3-1V2O)")
			(pinfunction "1V2O")
			(pintype "output")
		)
		(pad "23" smd roundrect
			(at 2.25 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "unconnected-(U3-RSVD-Pad23)")
			(pinfunction "RSVD")
			(pintype "input+no_connect")
		)
		(pad "24" smd roundrect
			(at 2.75 4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "unconnected-(U3-SPDLED-Pad24)")
			(pinfunction "SPDLED")
			(pintype "output+no_connect")
		)
		(pad "25" smd roundrect
			(at 4.1625 2.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Net-(U3-LINKLED)")
			(pinfunction "LINKLED")
			(pintype "output")
		)
		(pad "26" smd roundrect
			(at 4.1625 2.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "unconnected-(U3-DUPLED-Pad26)")
			(pinfunction "DUPLED")
			(pintype "output+no_connect")
		)
		(pad "27" smd roundrect
			(at 4.1625 1.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "Net-(U3-ACTLED)")
			(pinfunction "ACTLED")
			(pintype "output")
		)
		(pad "28" smd roundrect
			(at 4.1625 1.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "29" smd roundrect
			(at 4.1625 0.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "30" smd roundrect
			(at 4.1625 0.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U3-XI{slash}CLKIN)")
			(pinfunction "XI/CLKIN")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at 4.1625 -0.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U3-XO)")
			(pinfunction "XO")
			(pintype "output")
		)
		(pad "32" smd roundrect
			(at 4.1625 -0.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/Ethernet/~{CS}")
			(pinfunction "~{SCS}")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at 4.1625 -1.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/SPI1_CLK")
			(pinfunction "SCLK")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at 4.1625 -1.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(U3-MISO)")
			(pinfunction "MISO")
			(pintype "output")
		)
		(pad "35" smd roundrect
			(at 4.1625 -2.25 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/SPI1_MOSI")
			(pinfunction "MOSI")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at 4.1625 -2.75 90)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/ETH_INT")
			(pinfunction "~{INT}")
			(pintype "input")
		)
		(pad "37" smd roundrect
			(at 2.75 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/Ethernet/~{RST}")
			(pinfunction "~{RST}")
			(pintype "input")
		)
		(pad "38" smd roundrect
			(at 2.25 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Net-(R42-Pad2)")
			(pinfunction "RSVD")
			(pintype "input")
		)
		(pad "39" smd roundrect
			(at 1.75 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "Net-(R43-Pad2)")
			(pinfunction "RSVD")
			(pintype "input")
		)
		(pad "40" smd roundrect
			(at 1.25 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "Net-(R44-Pad2)")
			(pinfunction "RSVD")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at 0.75 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Net-(R45-Pad2)")
			(pinfunction "RSVD")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at 0.25 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "Net-(R46-Pad2)")
			(pinfunction "RSVD")
			(pintype "input")
		)
		(pad "43" smd roundrect
			(at -0.25 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "Net-(U3-PMODE2)")
			(pinfunction "PMODE2")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at -0.75 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Net-(U3-PMODE1)")
			(pinfunction "PMODE1")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at -1.25 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "Net-(U3-PMODE0)")
			(pinfunction "PMODE0")
			(pintype "input")
		)
		(pad "46" smd roundrect
			(at -1.75 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "unconnected-(U3-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" smd roundrect
			(at -2.25 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "unconnected-(U3-NC-Pad47)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "48" smd roundrect
			(at -2.75 -4.1625 90)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 150.69 105.9)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0.01 0.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U2-PA13)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Net-(J4-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 134.245 111.05 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0.1 -3.18 90)
			(layer "F.SilkS")
		)
		(property "Value" "12k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25752"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Net-(U3-EXRES1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 138.41 103.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 5.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Ethernet/WZNT_AVCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 123.885 102.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at -1.815 -0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Net-(R45-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 128.895 96.6 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0.6 -2.845 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(U3-MISO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/SPI1_MISO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.4375 79.38 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at 0.02 -6.0125 90)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "npr-power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U5-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 142.725 48.08 90)
		(descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole horizontal IDC box header THT 2x03 2.54mm double row")
		(property "Reference" "J2"
			(at 3.43 9.575 180)
			(layer "F.SilkS")
		)
		(property "Value" "GPIO"
			(at 6.215 11.18 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C34945"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.83 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 32 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(J2-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 176.835 37.05 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0.01 -1 0)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C12246"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 131.16 92 -90)
		(descr "SMD3225/4, Crystal, 3.2x2.5mm package, SMD, generated with kicad-footprint-generator make_crystal.py, http://www.txccrystal.com/images/pdf/7m-accuracy.pdf")
		(property "Reference" "Y2"
			(at -2.5 0.86 0)
			(layer "F.SilkS")
		)
		(property "Value" "25MHz"
			(at 0 2.45 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Four pin crystal, GND on pins 2 and 4"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C9006"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1 0.85 270)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 15 "Net-(U3-XO)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.1 0.85 270)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1 -0.85 270)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "Net-(U3-XI{slash}CLKIN)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.1 -0.85 270)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 152 91.65)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Net-(U2-PA15)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/RXD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 144.225 98.45)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "GPIO"
			(at 0 7.41 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr through_hole exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "/PA11")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/PA12")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_RJ:RJ45_Hanrun_HR911105A_Horizontal"
		(layer "F.Cu")
		(at 126.07 119.44)
		(descr "1 Port RJ45 8P8C receptacle, shielded, with magnetics, through hole, 2 LEDs, tab down, http://www.hanrun.com/public/upload/down/2020/09-11/cc11be56d66bb63d5f1eeb85492439c0.pdf")
		(tags "RJ45 Magjack ethernet")
		(property "Reference" "J5"
			(at 13.58 12.21 0)
			(layer "F.SilkS")
		)
		(property "Value" "RJ45_Hanrun_HR911105A_Horizontal"
			(at 4.44 18.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141815_HANRUN-Zhongshan-HanRun-Elec-HR911105A_C12074.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C12074"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RJ45*Hanrun*HR911105A*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.44 6.36 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.275 6.36)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 10.155 6.36)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.167)
			(net 43 "Net-(J5-TD+)")
			(pinfunction "TD+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.26 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J5-TD-)")
			(pinfunction "TD-")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J5-RD+)")
			(pinfunction "RD+")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 3.8 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J5-TCT)")
			(pinfunction "TCT")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 5.08 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J5-RCT)")
			(pinfunction "RCT")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 6.34 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J5-RD-)")
			(pinfunction "RD-")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 7.62 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(J5-NC-Pad7)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "8" thru_hole circle
			(at 8.88 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/Ethernet/ETH_GND")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at -2.185 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0.355 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/Ethernet/LINK_LED")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 8.525 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/Ethernet/ACT_LED")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 11.065 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Ethernet/WZNT_DVCC")
			(pintype "passive")
		)
		(pad "SH" thru_hole circle
			(at -3.305 3.31)
			(size 2.5 2.5)
			(drill 1.63)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/Ethernet/ETH_GND")
			(pintype "passive")
		)
		(pad "SH" thru_hole circle
			(at 12.185 3.31)
			(size 2.5 2.5)
			(drill 1.63)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/Ethernet/ETH_GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Hanrun_HR911105A_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/Parts.3dshapes/HR911105A.STEP"
			(offset
				(xyz 4.5 -3.3 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 178.78 126.175)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0.845 0.975 0)
			(layer "F.SilkS")
		)
		(property "Value" "6.8pF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C88896"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Radio/")
		(sheetfile "npr-radio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "/Radio/ANT1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 131.295 111.65 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 1.8 0.005 90)
			(layer "F.SilkS")
		)
		(property "Value" "10R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25139"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "npr-ethernet.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "Net-(U3-RXP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 157.706316 46.65 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D3.0mm"
		(layer "B.Cu")
		(at 124.225 86.25 180)
		(descr "SMD pad as test Point, diameter 3.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 2.398 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -2.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.4 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D3.0mm"
		(layer "B.Cu")
		(at 177.225 86.25 180)
		(descr "SMD pad as test Point, diameter 3.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 2.398 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -2.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.4 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D3.0mm"
		(layer "B.Cu")
		(at 122.225 41.25 180)
		(descr "SMD pad as test Point, diameter 3.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 2.398 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -2.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.4 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D3.0mm"
		(layer "B.Cu")
		(at 130.225 131.25 180)
		(descr "SMD pad as test Point, diameter 3.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 2.398 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -2.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.4 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D3.0mm"
		(layer "B.Cu")
		(at 177.225 41.25 180)
		(descr "SMD pad as test Point, diameter 3.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 2.398 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -2.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.4 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 149.925 98.95 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D3.0mm"
		(layer "B.Cu")
		(at 167.225 131.25 180)
		(descr "SMD pad as test Point, diameter 3.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 2.398 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -2.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "npr-revB.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.4 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 116.225 35.75)
		(end 183.225 35.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.925 135.75)
		(end 116.225 135.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.225 135.75)
		(end 178.525 135.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.225 135.75)
		(end 116.225 35.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.225 35.75)
		(end 183.225 135.75)
		(layer "Edge.Cuts")
	)
	(gr_text "SWCLK"
		(at 145.425 95.65 315)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 125.87 62.72 45)
		(layer "F.SilkS")
	)
	(gr_text "PA12"
		(at 141.925 104.35 315)
		(layer "F.SilkS")
	)
	(gr_text "USB"
		(at 137.075 60.875 0)
		(layer "F.SilkS")
	)
	(gr_text "RF4463F30\n433 MHz"
		(at 164.9 106.95 270)
		(layer "F.SilkS")
	)
	(gr_text "${TITLE}"
		(at 121.6 57.75 0)
		(layer "F.SilkS")
	)
	(gr_text "EXT 5V"
		(at 123.3 62.75 45)
		(layer "F.SilkS")
	)
	(gr_text "SWDIO"
		(at 145.525 100.85 315)
		(layer "F.SilkS")
	)
	(gr_text "EXT"
		(at 137.075 62.875 0)
		(layer "F.SilkS")
	)
	(gr_text "PA11"
		(at 139.525 96.75 315)
		(layer "F.SilkS")
	)
	(gr_text "RESET"
		(at 148.4 72.85 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 149.025 101.75 315)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 139.825 99.75 315)
		(layer "F.SilkS")
	)
	(gr_text "${COMPANY}, ${COMMENT1}\nRevision ${REVISION}\n${ISSUE_DATE}"
		(at 177 63.55 0)
		(layer "F.SilkS")
	)
	(gr_text "The NPR (New Packet Radio) project enables bidirectional\nIP communication over 70cm ham radio frequencies\n(420-450 MHz) using a custom, open-source protocol\noptimized for point-to-multipoint networking."
		(at 149.725 62.65 0)
		(layer "B.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 183.225 135.75) (xy 183.225 35.75)
		)
		(height 9.2)
		(orientation 1)
		(format
			(prefix "")
			(suffix " mm")
			(units 3)
			(units_format 0)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "100.0 mm"
			(at 191.275 85.75 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 116.225 135.75) (xy 183.225 136.75)
		)
		(height 14.9)
		(orientation 0)
		(format
			(prefix "")
			(suffix " mm")
			(units 3)
			(units_format 0)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "67.0 mm"
			(at 149.725 149.5 0)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 2)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130.4875 75.2) (xy 137.7875 75.2) (xy 137.7875 72.95) (xy 131.9375 72.95) (xy 131.9375 74.3)
				(xy 130.4875 74.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.045 90.7) (xy 138.045 93.45) (xy 135.495 93.45) (xy 135.495 90.7)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(U4-VCC)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 153.175 110.05) (xy 154.525 110.05) (xy 154.525 115.35) (xy 158.625 115.35) (xy 158.625 118.3)
				(xy 153.175 118.3)
			)
		)
	)
	(zone
		(net 44)
		(net_name "Net-(U5-L2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.1875 70.8) (xy 131.1875 73.8) (xy 130.2875 73.8) (xy 130.2875 75.2) (xy 129.9875 75.2) (xy 129.9875 73.8)
				(xy 129.7875 73.8) (xy 129.7875 70.8)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(J8-Pin_2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.5 71.55) (xy 126.7 71.55) (xy 126.7 66.85) (xy 124.7 66.85) (xy 124.7 68.776666) (xy 123.4 70.25)
				(xy 121.5 70.25)
			)
		)
	)
	(zone
		(net 20)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.7875 75.2) (xy 123.55 75.2) (xy 123.55 81.95) (xy 121.501087 81.95) (xy 121.4875 71.95)
				(xy 126.6875 71.95) (xy 126.6875 74) (xy 128.7875 74)
			)
		)
	)
	(zone
		(net 45)
		(net_name "Net-(U5-L1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.4875 70.8) (xy 129.4875 73.8) (xy 129.2875 73.8) (xy 129.2875 75.2) (xy 128.9875 75.2) (xy 128.9875 73.8)
				(xy 128.0875 73.8) (xy 128.0875 70.8)
			)
		)
	)
	(zone
		(net 123)
		(net_name "/Radio/ANT1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 178.025 126.45) (xy 178.625 126.45) (xy 178.625 124.25) (xy 177.738043 124.25)
			)
		)
	)
	(zone
		(net 124)
		(net_name "/Radio/ANT2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 176.425 123.05) (xy 177.025 123.05) (xy 177.225 125.25) (xy 176.425 125.25)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.225 135.75) (xy 183.225 35.75) (xy 116.225 35.75) (xy 116.225 135.75)
			)
		)
	)
	(zone
		(net 78)
		(net_name "Net-(J7-Pin_1)")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.4 68.65) (xy 124.2 68.65) (xy 124.2 63.15) (xy 122.4 63.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Mask")
		(hatch full 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.225 35.75) (xy 181.225 35.75) (xy 181.225 135.75) (xy 183.225 135.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Mask")
		(hatch full 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.225 35.75) (xy 116.225 35.75) (xy 116.225 135.75) (xy 118.225 135.75)
			)
		)
	)
	(embedded_fonts no)
)
