(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.09)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "PocketPico (The GameBoy Emulator)")
		(date "2024-09-02")
		(rev "A")
		(company "μArt.cz")
		(comment 1 "Vlastimil Slinták")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 62.185148 18.1375)
		(grid_origin 62.185148 18.1375)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/XTAL_IN")
	(net 2 "GND")
	(net 3 "Net-(C2-Pad2)")
	(net 4 "+3V3")
	(net 5 "+5V")
	(net 6 "Net-(U1-EN)")
	(net 7 "+BATT")
	(net 8 "+1V1")
	(net 9 "Net-(J1-Pin_1)")
	(net 10 "Net-(J1-Pin_2)")
	(net 11 "VCC")
	(net 12 "Net-(D2-K)")
	(net 13 "Net-(J2-DAT1)")
	(net 14 "/SD_CS")
	(net 15 "Net-(J2-DAT2)")
	(net 16 "/SD_CLK")
	(net 17 "/SD_MOSI")
	(net 18 "/SD_MISO")
	(net 19 "Net-(J3-CC2)")
	(net 20 "Net-(J3-CC1)")
	(net 21 "/USB+")
	(net 22 "/USB-")
	(net 23 "/SWCLK")
	(net 24 "/SWD")
	(net 25 "Net-(U1-L2)")
	(net 26 "Net-(U1-L1)")
	(net 27 "Net-(Q2-D)")
	(net 28 "/LCD_BL")
	(net 29 "/XTAL_OUT")
	(net 30 "Net-(R4-Pad1)")
	(net 31 "Net-(U1-FB)")
	(net 32 "Net-(R6-Pad1)")
	(net 33 "Net-(U2-PROG)")
	(net 34 "Net-(U2-STAT)")
	(net 35 "Net-(U4-~{RUN})")
	(net 36 "Net-(U4-D+)")
	(net 37 "/AMP_SD")
	(net 38 "Net-(U4-D-)")
	(net 39 "Net-(U4-SWCLK)")
	(net 40 "/QSPI_CS")
	(net 41 "Net-(U4-SWDIO)")
	(net 42 "Net-(R26-Pad1)")
	(net 43 "unconnected-(SW3-C-Pad3)")
	(net 44 "/BTN_UP")
	(net 45 "/BTN_RIGHT")
	(net 46 "/BTN_SLCT")
	(net 47 "/BTN_A")
	(net 48 "/BTN_DOWN")
	(net 49 "/BTN_LEFT")
	(net 50 "/BTN_START")
	(net 51 "/BTN_B")
	(net 52 "/AMP_LRC")
	(net 53 "/AMP_DIN")
	(net 54 "/AMP_BCLK")
	(net 55 "/LCD_RS")
	(net 56 "/LCD_RST")
	(net 57 "unconnected-(U5-XR-Pad16)")
	(net 58 "/LCD_SCK")
	(net 59 "unconnected-(U5-YD-Pad13)")
	(net 60 "/LCD_CS")
	(net 61 "unconnected-(U5-YU-Pad15)")
	(net 62 "unconnected-(U5-XL-Pad14)")
	(net 63 "/LCD_SDA")
	(net 64 "/QSPI_CLK")
	(net 65 "/QSPI_SD0")
	(net 66 "/QSPI_SD2")
	(net 67 "/QSPI_SD1")
	(net 68 "/QSPI_SD3")
	(net 69 "unconnected-(U4-GPIO16-Pad27)")
	(net 70 "unconnected-(U4-GPIO29{slash}ADC3-Pad41)")
	(net 71 "unconnected-(U4-GPIO25-Pad37)")
	(net 72 "unconnected-(U4-GPIO23-Pad35)")
	(net 73 "unconnected-(U4-GPIO10-Pad13)")
	(net 74 "unconnected-(U4-GPIO11-Pad14)")
	(net 75 "unconnected-(U4-GPIO24-Pad36)")
	(net 76 "unconnected-(U4-GPIO1-Pad3)")
	(net 77 "unconnected-(U4-GPIO0-Pad2)")
	(net 78 "/AMP_OP")
	(net 79 "/AMP_ON")
	(net 80 "/AMP_GAIN")
	(net 81 "Net-(SW1-C)")
	(net 82 "unconnected-(SW1-A-Pad1)")
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 133.880148 93.8025 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at -1.515 0.145 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/SD_CLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Card:microSD_HC_Molex_104031-0811"
		(layer "F.Cu")
		(at 132.430148 85.0425 -90)
		(descr "1.10mm Pitch microSD Memory Card Connector, Surface Mount, Push-Pull Type, 1.42mm Height, with Detect Switch (https://www.molex.com/pdm_docs/sd/1040310811_sd.pdf)")
		(tags "microSD SD molex")
		(property "Reference" "J2"
			(at 6.945 5.295 0)
			(layer "F.SilkS")
		)
		(property "Value" "Micro_SD_Card"
			(at 0 7.39 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Card:microSD_HC_Molex_104031-0811"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/693072010801.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Micro SD Card Socket"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C585350"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "microSD*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.105 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(J2-DAT2)")
			(pinfunction "DAT2")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -2.005 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/SD_CS")
			(pinfunction "DAT3/CD")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -0.905 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/SD_MOSI")
			(pinfunction "CMD")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.195 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.295 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/SD_CLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.395 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at 3.495 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/SD_MISO")
			(pinfunction "DAT0")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 4.545 -5.45 270)
			(size 0.75 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J2-DAT1)")
			(pinfunction "DAT1")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -5.74 0.7 270)
			(size 1.2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -5.74 4.4 270)
			(size 1.2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "11" smd rect
			(at -5.565 -5.325 270)
			(size 1.55 1.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "11" smd rect
			(at -2.24 5.375 270)
			(size 1.9 1.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "11" smd rect
			(at 3.73 5.375 270)
			(size 1.9 1.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "11" smd rect
			(at 5.755 -5.1 270)
			(size 1.17 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Molex_104031-0811.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/PocketPico.3dshapes/Molex-104031-0811.stp"
			(offset
				(xyz 44.5 -1.7 0.55)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 117.085148 152.7125)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 1.65 0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 78.085148 125.3375)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220p"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C39122"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 72.185148 28.1375)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 100.585148 148.4875 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 1.45 -0.55 180)
			(layer "F.SilkS")
		)
		(property "Value" "5k1"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(J3-CC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 116.895148 126.1375 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at -2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "Net-(R26-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/QSPI_CS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 135.630148 93.8125 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at -1.525 -0.655 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/SD_MISO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 113.685148 153.675 180)
		(descr "SOT, 5 Pin (~), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MCP73831"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in SOT23-5 package"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C14879"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(U2-STAT)")
			(pinfunction "STAT")
			(pintype "tri_state")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "V_{SS}")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "+BATT")
			(pinfunction "V_{BAT}")
			(pintype "power_out")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pinfunction "V_{DD}")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U2-PROG)")
			(pinfunction "PROG")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PocketPico:RP2040-QFN-56"
		(layer "F.Cu")
		(at 102.222648 115.45 180)
		(descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
		(tags "QFN DFN_QFN")
		(property "Reference" "U4"
			(at 0 -5 0)
			(layer "F.SilkS")
		)
		(property "Value" "RP2040"
			(at 0 4.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "PocketPico:RP2040-QFN-56"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2040"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.6375 -0.6375 180)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at -0.6375 0.6375 180)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at 0.6375 -0.6375 180)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at 0.6375 0.6375 180)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "1" smd roundrect
			(at -3.4375 -2.6 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.4375 -2.2 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "unconnected-(U4-GPIO0-Pad2)")
			(pinfunction "GPIO0")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd roundrect
			(at -3.4375 -1.8 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "unconnected-(U4-GPIO1-Pad3)")
			(pinfunction "GPIO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" smd roundrect
			(at -3.4375 -1.4 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/BTN_UP")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -3.4375 -1 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/BTN_DOWN")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -3.4375 -0.6 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/BTN_LEFT")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -3.4375 -0.2 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/BTN_RIGHT")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -3.4375 0.2 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/BTN_A")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -3.4375 0.6 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/BTN_B")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -3.4375 1 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -3.4375 1.4 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/BTN_SLCT")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -3.4375 1.8 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/BTN_START")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -3.4375 2.2 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "unconnected-(U4-GPIO10-Pad13)")
			(pinfunction "GPIO10")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" smd roundrect
			(at -3.4375 2.6 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "unconnected-(U4-GPIO11-Pad14)")
			(pinfunction "GPIO11")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" smd roundrect
			(at -2.6 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/SD_MISO")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -2.2 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/SD_CS")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -1.8 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/SD_CLK")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -1.4 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/SD_MOSI")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -1 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "TESTEN")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at -0.6 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/XTAL_IN")
			(pinfunction "XTAL_IN")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -0.2 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/XTAL_OUT")
			(pinfunction "XTAL_OUT")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 0.2 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "23" smd roundrect
			(at 0.6 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 1 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "Net-(U4-SWCLK)")
			(pinfunction "SWCLK")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 1.4 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "Net-(U4-SWDIO)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 1.8 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U4-~{RUN})")
			(pinfunction "~{RUN}")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 2.2 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "unconnected-(U4-GPIO16-Pad27)")
			(pinfunction "GPIO16")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" smd roundrect
			(at 2.6 3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "/LCD_CS")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at 3.4375 2.6 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "/LCD_SCK")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 3.4375 2.2 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "/LCD_SDA")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 3.4375 1.8 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/LCD_RS")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 3.4375 1.4 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "/LCD_RST")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at 3.4375 1 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "34" smd roundrect
			(at 3.4375 0.6 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/LCD_BL")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 3.4375 0.2 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "unconnected-(U4-GPIO23-Pad35)")
			(pinfunction "GPIO23")
			(pintype "bidirectional+no_connect")
		)
		(pad "36" smd roundrect
			(at 3.4375 -0.2 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "unconnected-(U4-GPIO24-Pad36)")
			(pinfunction "GPIO24")
			(pintype "bidirectional+no_connect")
		)
		(pad "37" smd roundrect
			(at 3.4375 -0.6 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "unconnected-(U4-GPIO25-Pad37)")
			(pinfunction "GPIO25")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" smd roundrect
			(at 3.4375 -1 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "/AMP_DIN")
			(pinfunction "GPIO26/ADC0")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 3.4375 -1.4 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "/AMP_BCLK")
			(pinfunction "GPIO27/ADC1")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at 3.4375 -1.8 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "/AMP_LRC")
			(pinfunction "GPIO28/ADC2")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 3.4375 -2.2 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "unconnected-(U4-GPIO29{slash}ADC3-Pad41)")
			(pinfunction "GPIO29/ADC3")
			(pintype "bidirectional+no_connect")
		)
		(pad "42" smd roundrect
			(at 3.4375 -2.6 180)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "43" smd roundrect
			(at 2.6 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "ADC_AVDD")
			(pintype "power_in")
		)
		(pad "44" smd roundrect
			(at 2.2 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "VREG_VIN")
			(pintype "power_in")
		)
		(pad "45" smd roundrect
			(at 1.8 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pinfunction "VREG_VOUT")
			(pintype "power_out")
		)
		(pad "46" smd roundrect
			(at 1.4 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "Net-(U4-D-)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 1 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U4-D+)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at 0.6 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "USB_VDD")
			(pintype "power_in")
		)
		(pad "49" smd roundrect
			(at 0.2 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "50" smd roundrect
			(at -0.2 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at -0.6 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "/QSPI_SD3")
			(pinfunction "QSPI_SD3")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at -1 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "/QSPI_CLK")
			(pinfunction "QSPI_SCLK")
			(pintype "output")
		)
		(pad "53" smd roundrect
			(at -1.4 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/QSPI_SD0")
			(pinfunction "QSPI_SD0")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at -1.8 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "/QSPI_SD2")
			(pinfunction "QSPI_SD2")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at -2.2 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "/QSPI_SD1")
			(pinfunction "QSPI_SD1")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at -2.6 -3.4375 180)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/QSPI_CS")
			(pinfunction "QSPI_SS_N")
			(pintype "output")
		)
		(pad "57" thru_hole circle
			(at -1.275 -1.275 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at -1.275 0 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at -1.275 1.275 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 0 -1.275 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 0 0 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" smd roundrect
			(at 0 0 180)
			(size 3.2 3.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.045)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 0 1.275 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 1.275 -1.275 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 1.275 0 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 1.275 1.275 180)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/PocketPico.3dshapes/RP2040_QFN_PACKAGE.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 81.585148 125.8875 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 2.05 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/AMP_SD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 101.972648 122.7375 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 2.15 -0.0625 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 72.185148 78.1375)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 110.335148 153.6625 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 1.65 -0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 123.785148 145.0775 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 1.65 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.1sqmm_1x02_P3.6mm_D0.4mm_OD1mm"
		(layer "F.Cu")
		(at 75.485148 127.0375 180)
		(descr "Soldered wire connection, for 2 times 0.1 mm² wires, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.1sqmm")
		(property "Reference" "J1"
			(at 1.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SPEAKER"
			(at 1.8 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x02_P3.6mm_D0.4mm_OD1mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 1.8 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 9 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.6 0 180)
			(size 1.6 1.6)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x02_P3.6mm_D0.4mm_OD1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 130.185148 93.7975 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 2.04 -0.05 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(J2-DAT2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 101.022648 121.5875 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -2.6 0.0125 90)
			(layer "F.SilkS")
		)
		(property "Value" "27.4R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C31439"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/USB+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U4-D+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_CK_RS282G05A3"
		(layer "F.Cu")
		(at 101.185148 96.7375 -90)
		(descr "https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf")
		(tags "SPST button tactile switch")
		(property "Reference" "SW2"
			(at 0 -2.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "RESET"
			(at 0 3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPST_CK_RS282G05A3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C483808"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.6 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.9 0 270)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.9 0 270)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(U4-~{RUN})")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.625148 146.0775 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -1.66 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "Net-(R4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 104.022648 127.0875 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 2.0375 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12"
		(layer "F.Cu")
		(at 102.185148 155.4375)
		(descr "USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf")
		(tags "usb usb-c 2.0 pd")
		(property "Reference" "J3"
			(at -4.4 -5 0)
			(layer "F.SilkS")
		)
		(property "Value" "HRO Type C-31-M-12"
			(at 0 5.1 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0-only 14P Type-C Receptacle connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C165948"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.6)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.6)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -3.25 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A4" smd rect
			(at -2.45 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" smd rect
			(at -1.25 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(J3-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/USB+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" smd rect
			(at 0.25 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/USB-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" smd rect
			(at 1.25 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "A9" smd rect
			(at 2.45 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" smd rect
			(at 3.25 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" smd rect
			(at 3.25 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B4" smd rect
			(at 2.45 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" smd rect
			(at 1.75 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(J3-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.75 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/USB+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" smd rect
			(at -0.75 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/USB-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" smd rect
			(at -1.75 -4.045)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "B9" smd rect
			(at -2.45 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" smd rect
			(at -3.25 -4.045)
			(size 0.6 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.13)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.05)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.13)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.05)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_HRO_TYPE-C-31-M-12.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/PocketPico.3dshapes/USB4085-GF-A-.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 133.985148 104.3375 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 2.1 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/SWCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "Net-(U4-SWCLK)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.635148 148.9275 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -1.65 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "Net-(R6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPDT_PCM12"
		(layer "F.Cu")
		(at 124.235148 155.7125)
		(descr "Ultraminiature Surface Mount Slide Switch, right-angle, https://www.ckswitches.com/media/1424/pcm.pdf")
		(property "Reference" "SW1"
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "PWR"
			(at 0 4.25 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPDT_PCM12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C221841"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.2 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -3.65 -0.78)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" smd rect
			(at -3.65 1.43)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" np_thru_hole circle
			(at -1.5 0.33)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 1.5 0.33)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" smd rect
			(at 3.65 -0.78)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" smd rect
			(at 3.65 1.43)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "1" smd rect
			(at -2.25 -1.43)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "unconnected-(SW1-A-Pad1)")
			(pinfunction "A")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at 0.75 -1.43)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "VCC")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.25 -1.43)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "Net-(SW1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPDT_PCM12.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 103.885148 148.4875 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 1.45 0.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "5k1"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(J3-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 134.185148 148.1375)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H4"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 91.785148 82.1375 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.17 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/LCD_BL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102.907648 108.7125 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -1.665 -0.075 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/XTAL_OUT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.342648 118.0375 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 107.305148 119.22 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 1.4 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 104.522648 106.4875)
		(descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at -0.0375 -2.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "12MHz"
			(at 0 2.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Four pin crystal, GND on pins 2 and 4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C9002"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(C2-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/XTAL_IN")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 132.185148 28.1375)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
	)
	(footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 136.5 108.3 90)
		(descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.00mm single row")
		(property "Reference" "J4"
			(at 0.1 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "SWD"
			(at 0 6.06 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/SWCLK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2 90)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 4 90)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 99.747648 107.5175 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 2.65 -0.0125 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.880148 93.8025 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 2.085 -0.055 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/SD_MOSI")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 122.035148 150.5275 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 1.7 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "Net-(SW1-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.772648 107.9675 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 2.78 -0.0375 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U4-~{RUN})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm"
		(layer "F.Cu")
		(at 109.822648 125.1875 180)
		(descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at -2.1 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "W25Q128JVS"
			(at 0 3.56 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q128jv_dtr%20revc%2003272018%20plus.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "128Mb Serial Flash Memory, Standard/Dual/Quad SPI, SOIC-8"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C97521"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*5.23x5.23mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.6 -1.905 180)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/QSPI_CS")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.6 -0.635 180)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "/QSPI_SD1")
			(pinfunction "DO(IO1)")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.6 0.635 180)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "/QSPI_SD2")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -3.6 1.905 180)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 3.6 1.905 180)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/QSPI_SD0")
			(pinfunction "DI(IO0)")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 3.6 0.635 180)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "/QSPI_CLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 3.6 -0.635 180)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "/QSPI_SD3")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 3.6 -1.905 180)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_5.23x5.23mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/PocketPico.3dshapes/W25Q128JVSIM.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.635148 147.9775 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -1.65 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "Net-(R6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U1-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 98.172648 122.1875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 2 0.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C318573"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 101.922648 106.8625 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -1.625 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "22p"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1555"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:Texas_DRT-3"
		(layer "F.Cu")
		(at 102.185148 148.6725 180)
		(descr "Texas Instrument DRT-3 1x0.8mm Pitch 0.7mm http://www.ti.com/lit/ds/symlink/tpd2eusb30.pdf")
		(tags "DRT-3 1x0.8mm Pitch 0.7mm")
		(property "Reference" "U7"
			(at -0.05 1.235 0)
			(layer "F.SilkS")
		)
		(property "Value" "TPD2EUSB30"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_DRT-3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2eusb30a.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-Channel ESD Protection for Super-Speed USB 3.0 Interface, DRT-3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C97502"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Texas*DRT*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.35 0.425 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/USB+")
			(pinfunction "D+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.35 0.425 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/USB-")
			(pinfunction "D-")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0 -0.425 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Texas_DRT-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 113.685148 149.7 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 -2.45 180)
			(layer "F.SilkS")
		)
		(property "Value" "MMFTP3401"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C596234"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "VCC")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "+BATT")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 78.035148 121.4375)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220p"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C39122"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(J1-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 100.697648 107.5175 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 2.65 0.025 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Taiyo-Yuden_MD-3030"
		(layer "F.Cu")
		(at 120.435148 148.0275 -90)
		(descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-3030, 3.0mmx3.0mm")
		(tags "inductor taiyo-yuden md smd")
		(property "Reference" "L1"
			(at -2.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_Taiyo-Yuden_MD-3030"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5159665"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0 270)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U1-L2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 0 270)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U1-L1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Taiyo-Yuden_MD-3030.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 83.485148 125.8875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 2.04 -0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 122.835148 145.0775 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 1.65 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 124.335148 151.4775 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.65 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 138.785148 103.3375 90)
		(descr "JST SH series connector, SM03B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J5"
			(at 2.2 -2.7 180)
			(layer "F.SilkS")
		)
		(property "Value" "SM03B-SRSS-TB"
			(at 0 3.98 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160403"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/SWCLK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.3 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.3 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/PocketPico.3dshapes/SM03B-SRSS-TB.STEP"
			(offset
				(xyz 0 1.5 -0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 89.485148 81.1375 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "MMFTP3401"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C596234"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/LCD_BL")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(Q2-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 119.635148 137.1375 -90)
		(descr "JST PH series connector, B2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH vertical")
		(property "Reference" "J6"
			(at -4.9375 0.335148 180)
			(layer "F.SilkS")
		)
		(property "Value" "BATT"
			(at 0 4.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C160352"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0.5 270)
			(size 1 5.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "+BATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0.5 270)
			(size 1 5.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -3.4 -1.75 270)
			(size 1.6 3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
		)
		(pad "MP" smd roundrect
			(at 3.4 -1.75 270)
			(size 1.6 3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/PocketPico.3dshapes/B2B-PH-SM4-TB.stp"
			(offset
				(xyz 0 4.25 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 136.630148 93.8025 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 2.085 -0.055 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J2-DAT1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.342648 118.9875 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 2 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_BGA:WLP-9_1.448x1.468mm_Layout3x3_P0.4mm_Ball0.27mm_Pad0.25mm"
		(layer "F.Cu")
		(at 81.585148 123.1375 180)
		(descr "WLP-9, 1.468x1.448mm, 9 Ball, 3x3 Layout, 0.4mm Pitch, https://pdfserv.maximintegrated.com/package_dwgs/21-100168.PDF")
		(tags "BGA 9 0.4")
		(property "Reference" "U3"
			(at 0 1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX98357A"
			(at 0 1.724 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_BGA:WLP-9_1.448x1.468mm_Layout3x3_P0.4mm_Ball0.27mm_Pad0.25mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max98357a-max98357b.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Tiny, Low-Cost, PCM Class D Amplifier with Class AB Performance."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2682619"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin 0.000001)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -0.4 -0.4 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/AMP_SD")
			(pinfunction "~{SD_MODE}")
			(pintype "input")
		)
		(pad "A2" smd circle
			(at 0 -0.4 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "A3" smd circle
			(at 0.4 -0.4 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "/AMP_OP")
			(pinfunction "OUTP")
			(pintype "output")
		)
		(pad "B1" smd circle
			(at -0.4 0 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/AMP_DIN")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "B2" smd circle
			(at 0 0 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "/AMP_GAIN")
			(pinfunction "GAIN")
			(pintype "input+no_connect")
		)
		(pad "B3" smd circle
			(at 0.4 0 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "/AMP_ON")
			(pinfunction "OUTN")
			(pintype "output")
		)
		(pad "C1" smd circle
			(at -0.4 0.4 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "/AMP_BCLK")
			(pinfunction "BCLK")
			(pintype "input")
		)
		(pad "C2" smd circle
			(at 0 0.4 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "C3" smd circle
			(at 0.4 0.4 180)
			(size 0.27 0.27)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/AMP_LRC")
			(pinfunction "LRCLK")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_BGA.3dshapes/WLP-9_1.448x1.468mm_Layout3x3_P0.4mm_Ball0.27mm_Pad0.25mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 108.142648 113.12 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 1.3825 -0.0075 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 116.647648 156.4625 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -2.2875 -0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2286"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.335148 152.7125)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -1.7 -0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 99.122648 122.1875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 2 0.15 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C318573"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 107.122648 106.1125 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.425 0.0625 180)
			(layer "F.SilkS")
		)
		(property "Value" "22p"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1555"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/XTAL_IN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:Texas_DRC0010J_ThermalVias"
		(layer "F.Cu")
		(at 124.335148 148.0075)
		(descr "Texas DRC0010J, VSON10 3x3mm Body, 0.5mm Pitch,  http://www.ti.com/lit/ds/symlink/tps63000.pdf")
		(tags "Texas VSON10 3x3mm")
		(property "Reference" "U1"
			(at 0.95 -2.23 0)
			(layer "F.SilkS")
		)
		(property "Value" "TPS63000"
			(at 0.02032 2.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SON:Texas_DRC0010J_ThermalVias"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps63000.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buck-Boost Converter, 1.8-5.5V Input Voltage, 1.8A Switch Current, Adjustable 1.2-5.5V Output Voltage, VSON-10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C24966"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Texas*DRC0010J*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.25 -1.53)
			(size 0.25 0.34)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at -0.25 1.53)
			(size 0.25 0.34)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at 0 -0.63)
			(size 1.5 1.06)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at 0 0.63)
			(size 1.5 1.06)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at 0.25 -1.53)
			(size 0.25 0.34)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "" smd roundrect
			(at 0.25 1.53)
			(size 0.25 0.34)
			(layers "F.Paste")
			(roundrect_rratio 0.1)
			(zone_connect 0)
		)
		(pad "1" smd roundrect
			(at -1.4 -1)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -1.4 -0.5)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U1-L2)")
			(pinfunction "L2")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.4 0)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -1.4 0.5)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U1-L1)")
			(pinfunction "L1")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -1.4 1)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "Net-(SW1-C)")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.4 1)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 1.4 0.5)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-EN)")
			(pinfunction "PS/SYNC")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 1.4 0)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-EN)")
			(pinfunction "VINA")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 1.4 -0.5)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 1.4 -1)
			(size 0.6 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U1-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at -0.575 0)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 -0.95)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "11" smd custom
			(at 0 0)
			(size 1.65 2.4)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "passive")
			(zone_connect 0)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.125 -1.1) (xy 0.125 -1.1) (xy 0.125 -1.7) (xy 0.375 -1.7) (xy 0.375 1.7) (xy 0.125 1.7)
						(xy 0.125 1.1) (xy -0.125 1.1) (xy -0.125 1.7) (xy -0.375 1.7) (xy -0.375 -1.7) (xy -0.125 -1.7)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "11" thru_hole circle
			(at 0 0.95)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0.575 0)
			(size 0.5 0.5)
			(drill 0.2)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/Texas_DRC0010J.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/PocketPico.3dshapes/TPS63000DRCRG4.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 113.685148 145.6625 180)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D1"
			(at 0 2.275 0)
			(layer "F.SilkS")
		)
		(property "Value" "SD14"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2480"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 11 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 5 "+5V")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127.635148 147.0275)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 1.65 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U1-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "Net-(R4-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 133.985148 102.3375 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 2.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/SWD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "Net-(U4-SWDIO)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.105148 114.3375 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 100.072648 121.5875 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 2.6 0.0375 90)
			(layer "F.SilkS")
		)
		(property "Value" "27.4R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C31439"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "Net-(U4-D-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/USB-")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPDT_PCM12"
		(layer "F.Cu")
		(at 64.535148 91.9875 -90)
		(descr "Ultraminiature Surface Mount Slide Switch, right-angle, https://www.ckswitches.com/media/1424/pcm.pdf")
		(property "Reference" "SW3"
			(at -5.0875 -1.064852 180)
			(layer "F.SilkS")
		)
		(property "Value" "MUTE"
			(at 0 4.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPDT_PCM12"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C221841"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.2 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -3.65 -0.78 270)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" smd rect
			(at -3.65 1.43 270)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" np_thru_hole circle
			(at -1.5 0.33 270)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 1.5 0.33 270)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" smd rect
			(at 3.65 -0.78 270)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" smd rect
			(at 3.65 1.43 270)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "1" smd rect
			(at -2.25 -1.43 270)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/AMP_SD")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 -1.43 270)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.25 -1.43 270)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "unconnected-(SW3-C-Pad3)")
			(pinfunction "C")
			(pintype "passive+no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPDT_PCM12.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 124.335148 150.5275 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -1.65 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "120R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25079"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "Net-(SW1-C)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 78.335148 122.6375 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB2"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "180Ω@100MHz"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C710363"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "/AMP_ON")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(J1-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_CK_RS282G05A3"
		(layer "F.Cu")
		(at 108.285148 96.7375 -90)
		(descr "https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf")
		(tags "SPST button tactile switch")
		(property "Reference" "SW4"
			(at 0 -2.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "BOOT"
			(at 0 3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPST_CK_RS282G05A3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C483808"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.6 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.9 0 270)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.9 0 270)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(R26-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 117.085148 154.6625 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at -1.65 -0.075 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(U2-STAT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.922648 122.7375 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 1.75 -0.1125 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 102.185148 50.1375)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 137.630148 93.8025 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at -2.085 0.105 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 78.335148 124.1375 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB1"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "180Ω@100MHz"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C710363"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "/AMP_OP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 131.185148 93.7975 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -1.51 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/SD_CS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 116.895148 127.0875 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at -2 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/QSPI_CS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.335148 154.6125 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.7 -0.075 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U2-PROG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 82.535148 125.8875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 2.05 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15525"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PocketPico:ButtonPad-Circle-6mm"
		(layer "B.Cu")
		(at 121.302186 114.654703)
		(property "Reference" "SW6"
			(at -0.002186 -4.954703 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "RIGHT"
			(at 0 -6.8 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:ButtonPad-Circle-6mm"
			(at 0 -5.75 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -5.75 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 -5.75 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -8.25 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 3.35 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.6 3)
					(mid 0.257671 0)
					(end 2.6 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 -3)
					(end 4.35 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 3)
					(end 4.35 3)
					(width 0.45)
				)
				(gr_line
					(start 0.85 -1.5)
					(end 4.85 -1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.85 1.5)
					(end 4.85 1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.257671 0)
					(end 5.35 0)
					(width 0.45)
				)
			)
		)
		(pad "2" smd custom
			(at -3.3 0 270)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 45 "/BTN_RIGHT")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.249998 -1.303843)
					(mid -0.000001 -0.25)
					(end -2.249999 -1.303843)
					(width 0.45)
				)
				(gr_line
					(start 2.249998 -1.303843)
					(end 2.25 -4.175)
					(width 0.45)
				)
				(gr_line
					(start 0.75 -0.55)
					(end 0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -0.75 -0.55)
					(end -0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -2.249999 -1.303843)
					(end -2.25 -4.175)
					(width 0.45)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 124.802186 114.654703) (xy 124.783013 115.020553) (xy 124.725703 115.382394) (xy 124.630884 115.736262)
					(xy 124.499595 116.078281) (xy 124.333275 116.404703) (xy 124.133745 116.711951) (xy 123.903193 116.99666)
					(xy 123.644143 117.25571) (xy 123.359434 117.486262) (xy 123.052186 117.685792) (xy 122.725764 117.852112)
					(xy 122.383745 117.983401) (xy 122.029877 118.07822) (xy 121.668036 118.13553) (xy 121.302186 118.154703)
					(xy 120.936336 118.13553) (xy 120.574495 118.07822) (xy 120.220627 117.983401) (xy 119.878608 117.852112)
					(xy 119.552186 117.685792) (xy 119.244938 117.486262) (xy 118.960229 117.25571) (xy 118.701179 116.99666)
					(xy 118.470627 116.711951) (xy 118.271097 116.404703) (xy 118.104777 116.078281) (xy 117.973488 115.736262)
					(xy 117.878669 115.382394) (xy 117.821359 115.020553) (xy 117.802186 114.654703) (xy 117.821359 114.288853)
					(xy 117.878669 113.927012) (xy 117.973488 113.573144) (xy 118.104777 113.231125) (xy 118.271097 112.904703)
					(xy 118.470627 112.597455) (xy 118.701179 112.312746) (xy 118.960229 112.053696) (xy 119.244938 111.823144)
					(xy 119.552186 111.623614) (xy 119.878608 111.457294) (xy 120.220627 111.326005) (xy 120.574495 111.231186)
					(xy 120.936336 111.173876) (xy 121.302186 111.154703) (xy 121.668036 111.173876) (xy 122.029877 111.231186)
					(xy 122.383745 111.326005) (xy 122.725764 111.457294) (xy 123.052186 111.623614) (xy 123.359434 111.823144)
					(xy 123.644143 112.053696) (xy 123.903193 112.312746) (xy 124.133745 112.597455) (xy 124.333275 112.904703)
					(xy 124.499595 113.231125) (xy 124.630884 113.573144) (xy 124.725703 113.927012) (xy 124.783013 114.288853)
				)
			)
		)
	)
	(footprint "PocketPico:ButtonPad-Oval-9x4mm"
		(layer "B.Cu")
		(at 96.435148 137.931335)
		(property "Reference" "SW11"
			(at -0.035148 -3.531335 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "START"
			(at -0.4 3.3 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:ButtonPad-Oval-9x4mm"
			(at -0.4 4.3 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -0.4 4.3 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at -0.4 4.3 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd exclude_from_bom)
		(pad "1" smd custom
			(at -4.5 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2 2)
					(mid 0 0)
					(end 2 -2)
					(width 0.3)
				)
				(gr_line
					(start 2 2)
					(end 7 2)
					(width 0.3)
				)
				(gr_arc
					(start 7 -2)
					(mid 9 0)
					(end 7 2)
					(width 0.3)
				)
				(gr_line
					(start 5.1 1)
					(end 8.7 1)
					(width 0.3)
				)
				(gr_line
					(start 5.1 0)
					(end 8.8 0)
					(width 0.3)
				)
				(gr_line
					(start 5.1 -1)
					(end 8.7 -1)
					(width 0.3)
				)
				(gr_line
					(start 5.5 -2)
					(end 7 -2)
					(width 0.3)
				)
				(gr_line
					(start 0.4 1)
					(end 3.9 1)
					(width 0.3)
				)
				(gr_line
					(start 0.3 -1)
					(end 3.9 -1)
					(width 0.3)
				)
				(gr_line
					(start 2 -2)
					(end 3.5 -2)
					(width 0.3)
				)
				(gr_line
					(start 0.2 0)
					(end 3.9 0)
					(width 0.3)
				)
			)
		)
		(pad "2" smd custom
			(at 0 -2)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 50 "/BTN_START")
			(pinfunction "2")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_line
					(start -2.4 0.5)
					(end 2.4 0.5)
					(width 0.3)
				)
				(gr_line
					(start 0 0)
					(end 0 3.5)
					(width 0.3)
				)
				(gr_line
					(start -3.7 1.5)
					(end 3.8 1.5)
					(width 0.3)
				)
				(gr_line
					(start -3.7 2.5)
					(end 3.8 2.5)
					(width 0.3)
				)
				(gr_line
					(start -2.4 3.5)
					(end 2.4 3.5)
					(width 0.3)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.1)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(arc
						(start 93.935148 140.031335)
						(mid 91.835148 137.931335)
						(end 93.935148 135.831335)
					)
					(arc
						(start 98.935148 135.831335)
						(mid 101.035148 137.931335)
						(end 98.935148 140.031335)
					)
				)
			)
		)
	)
	(footprint "PocketPico:ButtonPad-Circle-6mm"
		(layer "B.Cu")
		(at 136.869772 114.654703)
		(property "Reference" "SW10"
			(at -2.269772 -6.354703 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "LEFT"
			(at 0 -6.8 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:ButtonPad-Circle-6mm"
			(at 0 -5.75 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -5.75 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 -5.75 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -2.269772 -6.354703 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 3.35 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.6 3)
					(mid 0.257671 0)
					(end 2.6 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 -3)
					(end 4.35 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 3)
					(end 4.35 3)
					(width 0.45)
				)
				(gr_line
					(start 0.85 -1.5)
					(end 4.85 -1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.85 1.5)
					(end 4.85 1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.257671 0)
					(end 5.35 0)
					(width 0.45)
				)
			)
		)
		(pad "2" smd custom
			(at -3.3 0 270)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 49 "/BTN_LEFT")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.249998 -1.303843)
					(mid -0.000001 -0.25)
					(end -2.249999 -1.303843)
					(width 0.45)
				)
				(gr_line
					(start 2.249998 -1.303843)
					(end 2.25 -4.175)
					(width 0.45)
				)
				(gr_line
					(start 0.75 -0.55)
					(end 0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -0.75 -0.55)
					(end -0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -2.249999 -1.303843)
					(end -2.25 -4.175)
					(width 0.45)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 140.369772 114.654703) (xy 140.350599 115.020553) (xy 140.293289 115.382394) (xy 140.19847 115.736262)
					(xy 140.067181 116.078281) (xy 139.900861 116.404703) (xy 139.701331 116.711951) (xy 139.470779 116.99666)
					(xy 139.211729 117.25571) (xy 138.92702 117.486262) (xy 138.619772 117.685792) (xy 138.29335 117.852112)
					(xy 137.951331 117.983401) (xy 137.597463 118.07822) (xy 137.235622 118.13553) (xy 136.869772 118.154703)
					(xy 136.503922 118.13553) (xy 136.142081 118.07822) (xy 135.788213 117.983401) (xy 135.446194 117.852112)
					(xy 135.119772 117.685792) (xy 134.812524 117.486262) (xy 134.527815 117.25571) (xy 134.268765 116.99666)
					(xy 134.038213 116.711951) (xy 133.838683 116.404703) (xy 133.672363 116.078281) (xy 133.541074 115.736262)
					(xy 133.446255 115.382394) (xy 133.388945 115.020553) (xy 133.369772 114.654703) (xy 133.388945 114.288853)
					(xy 133.446255 113.927012) (xy 133.541074 113.573144) (xy 133.672363 113.231125) (xy 133.838683 112.904703)
					(xy 134.038213 112.597455) (xy 134.268765 112.312746) (xy 134.527815 112.053696) (xy 134.812524 111.823144)
					(xy 135.119772 111.623614) (xy 135.446194 111.457294) (xy 135.788213 111.326005) (xy 136.142081 111.231186)
					(xy 136.503922 111.173876) (xy 136.869772 111.154703) (xy 137.235622 111.173876) (xy 137.597463 111.231186)
					(xy 137.951331 111.326005) (xy 138.29335 111.457294) (xy 138.619772 111.623614) (xy 138.92702 111.823144)
					(xy 139.211729 112.053696) (xy 139.470779 112.312746) (xy 139.701331 112.597455) (xy 139.900861 112.904703)
					(xy 140.067181 113.231125) (xy 140.19847 113.573144) (xy 140.293289 113.927012) (xy 140.350599 114.288853)
				)
			)
		)
	)
	(footprint "PocketPico:ButtonPad-Circle-6mm"
		(layer "B.Cu")
		(at 82.085148 116.9375 180)
		(property "Reference" "SW12"
			(at -0.014852 4.9375 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "B"
			(at 0 -6.8 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:ButtonPad-Circle-6mm"
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 3.35 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.6 3)
					(mid 0.257671 0)
					(end 2.6 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 -3)
					(end 4.35 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 3)
					(end 4.35 3)
					(width 0.45)
				)
				(gr_line
					(start 0.85 -1.5)
					(end 4.85 -1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.85 1.5)
					(end 4.85 1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.257671 0)
					(end 5.35 0)
					(width 0.45)
				)
			)
		)
		(pad "2" smd custom
			(at -3.3 0 90)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 51 "/BTN_B")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.249998 -1.303843)
					(mid -0.000001 -0.25)
					(end -2.249999 -1.303843)
					(width 0.45)
				)
				(gr_line
					(start 2.249998 -1.303843)
					(end 2.25 -4.175)
					(width 0.45)
				)
				(gr_line
					(start 0.75 -0.55)
					(end 0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -0.75 -0.55)
					(end -0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -2.249999 -1.303843)
					(end -2.25 -4.175)
					(width 0.45)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 78.585148 116.9375) (xy 78.604321 116.57165) (xy 78.661631 116.209809) (xy 78.75645 115.855941)
					(xy 78.887739 115.513922) (xy 79.054059 115.1875) (xy 79.253589 114.880252) (xy 79.484141 114.595543)
					(xy 79.743191 114.336493) (xy 80.0279 114.105941) (xy 80.335148 113.906411) (xy 80.66157 113.740091)
					(xy 81.003589 113.608802) (xy 81.357457 113.513983) (xy 81.719298 113.456673) (xy 82.085148 113.4375)
					(xy 82.450998 113.456673) (xy 82.812839 113.513983) (xy 83.166707 113.608802) (xy 83.508726 113.740091)
					(xy 83.835148 113.906411) (xy 84.142396 114.105941) (xy 84.427105 114.336493) (xy 84.686155 114.595543)
					(xy 84.916707 114.880252) (xy 85.116237 115.1875) (xy 85.282557 115.513922) (xy 85.413846 115.855941)
					(xy 85.508665 116.209809) (xy 85.565975 116.57165) (xy 85.585148 116.9375) (xy 85.565975 117.30335)
					(xy 85.508665 117.665191) (xy 85.413846 118.019059) (xy 85.282557 118.361078) (xy 85.116237 118.6875)
					(xy 84.916707 118.994748) (xy 84.686155 119.279457) (xy 84.427105 119.538507) (xy 84.142396 119.769059)
					(xy 83.835148 119.968589) (xy 83.508726 120.134909) (xy 83.166707 120.266198) (xy 82.812839 120.361017)
					(xy 82.450998 120.418327) (xy 82.085148 120.4375) (xy 81.719298 120.418327) (xy 81.357457 120.361017)
					(xy 81.003589 120.266198) (xy 80.66157 120.134909) (xy 80.335148 119.968589) (xy 80.0279 119.769059)
					(xy 79.743191 119.538507) (xy 79.484141 119.279457) (xy 79.253589 118.994748) (xy 79.054059 118.6875)
					(xy 78.887739 118.361078) (xy 78.75645 118.019059) (xy 78.661631 117.665191) (xy 78.604321 117.30335)
				)
			)
		)
	)
	(footprint "PocketPico:ButtonPad-Circle-6mm"
		(layer "B.Cu")
		(at 129.085979 106.870909 180)
		(property "Reference" "SW5"
			(at 0.085979 5.070909 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "UP"
			(at 0 -6.8 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:ButtonPad-Circle-6mm"
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -8.25 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 3.35 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.6 3)
					(mid 0.257671 0)
					(end 2.6 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 -3)
					(end 4.35 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 3)
					(end 4.35 3)
					(width 0.45)
				)
				(gr_line
					(start 0.85 -1.5)
					(end 4.85 -1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.85 1.5)
					(end 4.85 1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.257671 0)
					(end 5.35 0)
					(width 0.45)
				)
			)
		)
		(pad "2" smd custom
			(at -3.3 0 90)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 44 "/BTN_UP")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.249998 -1.303843)
					(mid -0.000001 -0.25)
					(end -2.249999 -1.303843)
					(width 0.45)
				)
				(gr_line
					(start 2.249998 -1.303843)
					(end 2.25 -4.175)
					(width 0.45)
				)
				(gr_line
					(start 0.75 -0.55)
					(end 0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -0.75 -0.55)
					(end -0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -2.249999 -1.303843)
					(end -2.25 -4.175)
					(width 0.45)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 125.585979 106.870909) (xy 125.605152 106.505059) (xy 125.662462 106.143218) (xy 125.757281 105.78935)
					(xy 125.88857 105.447331) (xy 126.05489 105.120909) (xy 126.25442 104.813661) (xy 126.484972 104.528952)
					(xy 126.744022 104.269902) (xy 127.028731 104.03935) (xy 127.335979 103.83982) (xy 127.662401 103.6735)
					(xy 128.00442 103.542211) (xy 128.358288 103.447392) (xy 128.720129 103.390082) (xy 129.085979 103.370909)
					(xy 129.451829 103.390082) (xy 129.81367 103.447392) (xy 130.167538 103.542211) (xy 130.509557 103.6735)
					(xy 130.835979 103.83982) (xy 131.143227 104.03935) (xy 131.427936 104.269902) (xy 131.686986 104.528952)
					(xy 131.917538 104.813661) (xy 132.117068 105.120909) (xy 132.283388 105.447331) (xy 132.414677 105.78935)
					(xy 132.509496 106.143218) (xy 132.566806 106.505059) (xy 132.585979 106.870909) (xy 132.566806 107.236759)
					(xy 132.509496 107.5986) (xy 132.414677 107.952468) (xy 132.283388 108.294487) (xy 132.117068 108.620909)
					(xy 131.917538 108.928157) (xy 131.686986 109.212866) (xy 131.427936 109.471916) (xy 131.143227 109.702468)
					(xy 130.835979 109.901998) (xy 130.509557 110.068318) (xy 130.167538 110.199607) (xy 129.81367 110.294426)
					(xy 129.451829 110.351736) (xy 129.085979 110.370909) (xy 128.720129 110.351736) (xy 128.358288 110.294426)
					(xy 128.00442 110.199607) (xy 127.662401 110.068318) (xy 127.335979 109.901998) (xy 127.028731 109.702468)
					(xy 126.744022 109.471916) (xy 126.484972 109.212866) (xy 126.25442 108.928157) (xy 126.05489 108.620909)
					(xy 125.88857 108.294487) (xy 125.757281 107.952468) (xy 125.662462 107.5986) (xy 125.605152 107.236759)
				)
			)
		)
	)
	(footprint "PocketPico:ButtonPad-Oval-9x4mm"
		(layer "B.Cu")
		(at 107.935148 137.931335)
		(property "Reference" "SW7"
			(at -0.035148 -3.531335 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "SELECT"
			(at -0.4 3.3 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:ButtonPad-Oval-9x4mm"
			(at -0.4 4.3 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -0.4 4.3 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at -0.4 4.3 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd exclude_from_bom)
		(pad "1" smd custom
			(at -4.5 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2 2)
					(mid 0 0)
					(end 2 -2)
					(width 0.3)
				)
				(gr_line
					(start 2 2)
					(end 7 2)
					(width 0.3)
				)
				(gr_arc
					(start 7 -2)
					(mid 9 0)
					(end 7 2)
					(width 0.3)
				)
				(gr_line
					(start 5.1 1)
					(end 8.7 1)
					(width 0.3)
				)
				(gr_line
					(start 5.1 0)
					(end 8.8 0)
					(width 0.3)
				)
				(gr_line
					(start 5.1 -1)
					(end 8.7 -1)
					(width 0.3)
				)
				(gr_line
					(start 5.5 -2)
					(end 7 -2)
					(width 0.3)
				)
				(gr_line
					(start 0.4 1)
					(end 3.9 1)
					(width 0.3)
				)
				(gr_line
					(start 0.3 -1)
					(end 3.9 -1)
					(width 0.3)
				)
				(gr_line
					(start 2 -2)
					(end 3.5 -2)
					(width 0.3)
				)
				(gr_line
					(start 0.2 0)
					(end 3.9 0)
					(width 0.3)
				)
			)
		)
		(pad "2" smd custom
			(at 0 -2)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 46 "/BTN_SLCT")
			(pinfunction "2")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_line
					(start -2.4 0.5)
					(end 2.4 0.5)
					(width 0.3)
				)
				(gr_line
					(start 0 0)
					(end 0 3.5)
					(width 0.3)
				)
				(gr_line
					(start -3.7 1.5)
					(end 3.8 1.5)
					(width 0.3)
				)
				(gr_line
					(start -3.7 2.5)
					(end 3.8 2.5)
					(width 0.3)
				)
				(gr_line
					(start -2.4 3.5)
					(end 2.4 3.5)
					(width 0.3)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.1)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(arc
						(start 105.435148 140.031335)
						(mid 103.335148 137.931335)
						(end 105.435148 135.831335)
					)
					(arc
						(start 110.435148 135.831335)
						(mid 112.535148 137.931335)
						(end 110.435148 140.031335)
					)
				)
			)
		)
	)
	(footprint "PocketPico:ButtonPad-Circle-6mm"
		(layer "B.Cu")
		(at 69.224909 109.614152 180)
		(property "Reference" "SW8"
			(at 0.024909 5.114152 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "A"
			(at 0 -6.8 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:ButtonPad-Circle-6mm"
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 -5.75 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.139761 -5.323348 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 3.35 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.6 3)
					(mid 0.257671 0)
					(end 2.6 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 -3)
					(end 4.35 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 3)
					(end 4.35 3)
					(width 0.45)
				)
				(gr_line
					(start 0.85 -1.5)
					(end 4.85 -1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.85 1.5)
					(end 4.85 1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.257671 0)
					(end 5.35 0)
					(width 0.45)
				)
			)
		)
		(pad "2" smd custom
			(at -3.3 0 90)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 47 "/BTN_A")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.249998 -1.303843)
					(mid -0.000001 -0.25)
					(end -2.249999 -1.303843)
					(width 0.45)
				)
				(gr_line
					(start 2.249998 -1.303843)
					(end 2.25 -4.175)
					(width 0.45)
				)
				(gr_line
					(start 0.75 -0.55)
					(end 0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -0.75 -0.55)
					(end -0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -2.249999 -1.303843)
					(end -2.25 -4.175)
					(width 0.45)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 65.724909 109.614152) (xy 65.744082 109.248302) (xy 65.801392 108.886461) (xy 65.896211 108.532593)
					(xy 66.0275 108.190574) (xy 66.19382 107.864152) (xy 66.39335 107.556904) (xy 66.623902 107.272195)
					(xy 66.882952 107.013145) (xy 67.167661 106.782593) (xy 67.474909 106.583063) (xy 67.801331 106.416743)
					(xy 68.14335 106.285454) (xy 68.497218 106.190635) (xy 68.859059 106.133325) (xy 69.224909 106.114152)
					(xy 69.590759 106.133325) (xy 69.9526 106.190635) (xy 70.306468 106.285454) (xy 70.648487 106.416743)
					(xy 70.974909 106.583063) (xy 71.282157 106.782593) (xy 71.566866 107.013145) (xy 71.825916 107.272195)
					(xy 72.056468 107.556904) (xy 72.255998 107.864152) (xy 72.422318 108.190574) (xy 72.553607 108.532593)
					(xy 72.648426 108.886461) (xy 72.705736 109.248302) (xy 72.724909 109.614152) (xy 72.705736 109.980002)
					(xy 72.648426 110.341843) (xy 72.553607 110.695711) (xy 72.422318 111.03773) (xy 72.255998 111.364152)
					(xy 72.056468 111.6714) (xy 71.825916 111.956109) (xy 71.566866 112.215159) (xy 71.282157 112.445711)
					(xy 70.974909 112.645241) (xy 70.648487 112.811561) (xy 70.306468 112.94285) (xy 69.9526 113.037669)
					(xy 69.590759 113.094979) (xy 69.224909 113.114152) (xy 68.859059 113.094979) (xy 68.497218 113.037669)
					(xy 68.14335 112.94285) (xy 67.801331 112.811561) (xy 67.474909 112.645241) (xy 67.167661 112.445711)
					(xy 66.882952 112.215159) (xy 66.623902 111.956109) (xy 66.39335 111.6714) (xy 66.19382 111.364152)
					(xy 66.0275 111.03773) (xy 65.896211 110.695711) (xy 65.801392 110.341843) (xy 65.744082 109.980002)
				)
			)
		)
	)
	(footprint "PocketPico:LCD-ILI9225-18pins"
		(layer "B.Cu")
		(at 143.915148 39.5875 180)
		(property "Reference" "U5"
			(at 20.73 3.65 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "ILI9225 SPI 18pin"
			(at 19.9 6.2 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:LCD-ILI9225-18pins"
			(at 11.4 -35.1 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 11.4 -35.1 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 11.4 -35.1 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd)
		(fp_text user "176x220 px, 2.2''"
			(at 23.53 0.75 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at 20.4 0 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at 20.4 -0.8 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "LED-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at 20.4 -1.6 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(Q2-D)")
			(pinfunction "LED+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 20.4 -2.4 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 20.4 -3.2 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 56 "/LCD_RST")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 20.4 -4 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/LCD_RS")
			(pinfunction "RS")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 20.4 -4.8 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 63 "/LCD_SDA")
			(pinfunction "SDA")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 20.4 -5.6 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "/LCD_SCK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 20.4 -6.4 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 20.4 -7.2 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "VDDIO")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 20.4 -8 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 60 "/LCD_CS")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 20.4 -8.8 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 20.4 -9.6 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 59 "unconnected-(U5-YD-Pad13)")
			(pinfunction "YD")
			(pintype "no_connect")
		)
		(pad "14" smd roundrect
			(at 20.4 -10.4 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 62 "unconnected-(U5-XL-Pad14)")
			(pinfunction "XL")
			(pintype "no_connect")
		)
		(pad "15" smd roundrect
			(at 20.4 -11.2 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 61 "unconnected-(U5-YU-Pad15)")
			(pinfunction "YU")
			(pintype "no_connect")
		)
		(pad "16" smd roundrect
			(at 20.4 -12 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(U5-XR-Pad16)")
			(pinfunction "XR")
			(pintype "no_connect")
		)
		(pad "17" smd roundrect
			(at 20.4 -12.8 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "18" smd roundrect
			(at 20.4 -13.6 90)
			(size 0.45 2.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
	)
	(footprint "PocketPico:ButtonPad-Circle-6mm"
		(layer "B.Cu")
		(at 128.959547 122.438496 -90)
		(property "Reference" "SW9"
			(at 4.961504 -0.040453 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DOWN"
			(at 0 -6.8 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "PocketPico:ButtonPad-Circle-6mm"
			(at 0 -5.75 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -5.75 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 -5.75 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pocketpico.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -8.25 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 3.35 0 90)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.6 3)
					(mid 0.257671 0)
					(end 2.6 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 -3)
					(end 4.35 -3)
					(width 0.45)
				)
				(gr_line
					(start 2.6 3)
					(end 4.35 3)
					(width 0.45)
				)
				(gr_line
					(start 0.85 -1.5)
					(end 4.85 -1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.85 1.5)
					(end 4.85 1.5)
					(width 0.45)
				)
				(gr_line
					(start 0.257671 0)
					(end 5.35 0)
					(width 0.45)
				)
			)
		)
		(pad "2" smd custom
			(at -3.3 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 48 "/BTN_DOWN")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 2.249998 -1.303843)
					(mid -0.000001 -0.25)
					(end -2.249999 -1.303843)
					(width 0.45)
				)
				(gr_line
					(start 2.249998 -1.303843)
					(end 2.25 -4.175)
					(width 0.45)
				)
				(gr_line
					(start 0.75 -0.55)
					(end 0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -0.75 -0.55)
					(end -0.75 -5.3)
					(width 0.45)
				)
				(gr_line
					(start -2.249999 -1.303843)
					(end -2.25 -4.175)
					(width 0.45)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 128.959547 125.938496) (xy 128.593697 125.919323) (xy 128.231856 125.862013) (xy 127.877988 125.767194)
					(xy 127.535969 125.635905) (xy 127.209547 125.469585) (xy 126.902299 125.270055) (xy 126.61759 125.039503)
					(xy 126.35854 124.780453) (xy 126.127988 124.495744) (xy 125.928458 124.188496) (xy 125.762138 123.862074)
					(xy 125.630849 123.520055) (xy 125.53603 123.166187) (xy 125.47872 122.804346) (xy 125.459547 122.438496)
					(xy 125.47872 122.072646) (xy 125.53603 121.710805) (xy 125.630849 121.356937) (xy 125.762138 121.014918)
					(xy 125.928458 120.688496) (xy 126.127988 120.381248) (xy 126.35854 120.096539) (xy 126.61759 119.837489)
					(xy 126.902299 119.606937) (xy 127.209547 119.407407) (xy 127.535969 119.241087) (xy 127.877988 119.109798)
					(xy 128.231856 119.014979) (xy 128.593697 118.957669) (xy 128.959547 118.938496) (xy 129.325397 118.957669)
					(xy 129.687238 119.014979) (xy 130.041106 119.109798) (xy 130.383125 119.241087) (xy 130.709547 119.407407)
					(xy 131.016795 119.606937) (xy 131.301504 119.837489) (xy 131.560554 120.096539) (xy 131.791106 120.381248)
					(xy 131.990636 120.688496) (xy 132.156956 121.014918) (xy 132.288245 121.356937) (xy 132.383064 121.710805)
					(xy 132.440374 122.072646) (xy 132.459547 122.438496) (xy 132.440374 122.804346) (xy 132.383064 123.166187)
					(xy 132.288245 123.520055) (xy 132.156956 123.862074) (xy 131.990636 124.188496) (xy 131.791106 124.495744)
					(xy 131.560554 124.780453) (xy 131.301504 125.039503) (xy 131.016795 125.270055) (xy 130.709547 125.469585)
					(xy 130.383125 125.635905) (xy 130.041106 125.767194) (xy 129.687238 125.862013) (xy 129.325397 125.919323)
				)
			)
		)
	)
	(gr_line
		(start 90.444111 144.33889)
		(end 90.444111 158.1375)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.185148 18.1375)
		(end 62.185148 18.1375)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.185148 18.1375)
		(end 62.185148 129.338883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.185148 129.338883)
		(end 75.444108 129.338883)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.185148 158.1375)
		(end 142.185148 18.1375)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.444111 158.1375)
		(end 142.185148 158.1375)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 75.444108 129.338883)
		(mid 86.050711 133.732284)
		(end 90.444111 144.33889)
		(layer "Edge.Cuts")
	)
	(gr_text "Li-Ion\nBATTERY"
		(at 129.1 137.1 90)
		(layer "F.SilkS")
	)
	(gr_text "POWER\nOFF/ON"
		(at 133.5 157.4 0)
		(layer "F.SilkS")
	)
	(gr_text "BOOT"
		(at 108.2 91.3 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 116.4 135 0)
		(layer "F.SilkS")
	)
	(gr_text "MUTE\nON/OFF"
		(at 71.6 91.9 90)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 68.5 127.7375 0)
		(layer "F.SilkS")
	)
	(gr_text "${TITLE}"
		(at 102.185148 59.1375 0)
		(layer "F.SilkS")
	)
	(gr_text "${COMPANY}, Revision ${REVISION}, ${ISSUE_DATE}\nAuthor: ${COMMENT1} "
		(at 102.185148 64.1375 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 116.4 140.4 0)
		(layer "F.SilkS")
	)
	(gr_text "SWC\nGND\nSWD"
		(at 141.2 111.3 90)
		(layer "F.SilkS")
	)
	(gr_text "SPEAKER\nmax 3W"
		(at 69.3 125.1 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 76.585148 127.7375 0)
		(layer "F.SilkS")
	)
	(gr_text "RESET"
		(at 101 91.3 0)
		(layer "F.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 142.185148 158.1375) (xy 62.185148 129.338883)
		)
		(height 17.1)
		(orientation 0)
		(gr_text "80,0000 mm"
			(at 102.185148 174.0875 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 123.965148 37.1075) (xy 142.185148 18.1375)
		)
		(height -23.2075)
		(orientation 0)
		(gr_text "18,2200 mm"
			(at 133.075148 12.1 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 142.185148 158.1375) (xy 102.185148 159.3375)
		)
		(height 13.7)
		(orientation 0)
		(gr_text "40,0000 mm"
			(at 122.185148 170.6875 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 62.185148 18.1375) (xy 80.405148 37.1075)
		)
		(height -4.4375)
		(orientation 0)
		(gr_text "18,2200 mm"
			(at 71.295148 11.9 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 62.085148 18.4375) (xy 142.085148 18.4375) (xy 142.085148 158.4375) (xy 62.085148 158.4375)
			)
		)
	)
)
