(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "M-Coin Token")
		(date "2025-03-12")
		(rev "A")
		(company "Vlastimil Slinták")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 120.8 96)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(footprint "LOGO"
		(layer "F.Cu")
		(at 120.559566 95.735665)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Package_LGA:LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y"
		(layer "F.Cu")
		(at 130.3 97.7 30)
		(descr "LGA, 16 Pin (http://www.st.com/resource/en/datasheet/lis331hh.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "LGA NoLead")
		(property "Reference" "REF**"
			(at 0 -2.45 30)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y"
			(at 0 2.45 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd roundrect
			(at -1.225 -1 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "2" smd roundrect
			(at -1.225 -0.5 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -1.225 0 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -1.225 0.5 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "5" smd roundrect
			(at -1.225 1 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "6" smd roundrect
			(at -0.5 1.225 30)
			(size 0.35 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "7" smd roundrect
			(at 0 1.225 30)
			(size 0.35 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "8" smd roundrect
			(at 0.5 1.225 30)
			(size 0.35 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "9" smd roundrect
			(at 1.225 1 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "10" smd roundrect
			(at 1.225 0.5 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "11" smd roundrect
			(at 1.225 0 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "12" smd roundrect
			(at 1.225 -0.5 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "13" smd roundrect
			(at 1.225 -1 30)
			(size 0.55 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "14" smd roundrect
			(at 0.5 -1.225 30)
			(size 0.35 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "15" smd roundrect
			(at 0 -1.225 30)
			(size 0.35 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "16" smd roundrect
			(at -0.5 -1.225 30)
			(size 0.35 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 120.559566 95.735665)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 120.6 95.8)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 120.8 96.2 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 120.6 97.3 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(gr_circle
		(center 120.8 96)
		(end 133 96)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "M-COIN"
		(at 124.1 102.2 30)
		(layer "F.SilkS")
	)
	(gr_text "☺"
		(at 130 99.1 30)
		(layer "F.SilkS")
	)
	(gr_text "E"
		(at 122 100.1 -0)
		(layer "B.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.1)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.998887 95.657732) (xy 132.960505 94.974274) (xy 132.883862 94.294042) (xy 132.769198 93.619179)
				(xy 132.616874 92.951806) (xy 132.42737 92.294024) (xy 132.201283 91.647902) (xy 131.939322 91.015474)
				(xy 131.642313 90.398729) (xy 131.311191 89.799607) (xy 130.946996 89.219994) (xy 130.550875 88.661714)
				(xy 130.124074 88.126522) (xy 129.667936 87.616104) (xy 129.183896 87.132064) (xy 128.673478 86.675926)
				(xy 128.138286 86.249125) (xy 127.580006 85.853004) (xy 127.000393 85.488809) (xy 126.401271 85.157687)
				(xy 125.784526 84.860678) (xy 125.152098 84.598717) (xy 124.505976 84.37263) (xy 123.848194 84.183126)
				(xy 123.180821 84.030802) (xy 122.505958 83.916138) (xy 121.825726 83.839495) (xy 121.142268 83.801113)
				(xy 120.457732 83.801113) (xy 119.774274 83.839495) (xy 119.094042 83.916138) (xy 118.419179 84.030802)
				(xy 117.751806 84.183126) (xy 117.094024 84.37263) (xy 116.447902 84.598717) (xy 115.815474 84.860678)
				(xy 115.198729 85.157687) (xy 114.599607 85.488809) (xy 114.019994 85.853004) (xy 113.461714 86.249125)
				(xy 112.926522 86.675926) (xy 112.416104 87.132064) (xy 111.932064 87.616104) (xy 111.475926 88.126522)
				(xy 111.049125 88.661714) (xy 110.653004 89.219994) (xy 110.288809 89.799607) (xy 109.957687 90.398729)
				(xy 109.660678 91.015474) (xy 109.398717 91.647902) (xy 109.17263 92.294024) (xy 108.983126 92.951806)
				(xy 108.830802 93.619179) (xy 108.716138 94.294042) (xy 108.639495 94.974274) (xy 108.601113 95.657732)
				(xy 108.601113 96.342268) (xy 108.639495 97.025726) (xy 108.716138 97.705958) (xy 108.830802 98.380821)
				(xy 108.983126 99.048194) (xy 109.17263 99.705976) (xy 109.398717 100.352098) (xy 109.660678 100.984526)
				(xy 109.957687 101.601271) (xy 110.288809 102.200393) (xy 110.653004 102.780006) (xy 111.049125 103.338286)
				(xy 111.475926 103.873478) (xy 111.932064 104.383896) (xy 112.416104 104.867936) (xy 112.926522 105.324074)
				(xy 113.461714 105.750875) (xy 114.019994 106.146996) (xy 114.599607 106.511191) (xy 115.198729 106.842313)
				(xy 115.815474 107.139322) (xy 116.447902 107.401283) (xy 117.094024 107.62737) (xy 117.751806 107.816874)
				(xy 118.419179 107.969198) (xy 119.094042 108.083862) (xy 119.774274 108.160505) (xy 120.457732 108.198887)
				(xy 121.142268 108.198887) (xy 121.825726 108.160505) (xy 122.505958 108.083862) (xy 123.180821 107.969198)
				(xy 123.848194 107.816874) (xy 124.505976 107.62737) (xy 125.152098 107.401283) (xy 125.784526 107.139322)
				(xy 126.401271 106.842313) (xy 127.000393 106.511191) (xy 127.580006 106.146996) (xy 128.138286 105.750875)
				(xy 128.673478 105.324074) (xy 129.183896 104.867936) (xy 129.667936 104.383896) (xy 130.124074 103.873478)
				(xy 130.550875 103.338286) (xy 130.946996 102.780006) (xy 131.311191 102.200393) (xy 131.642313 101.601271)
				(xy 131.939322 100.984526) (xy 132.201283 100.352098) (xy 132.42737 99.705976) (xy 132.616874 99.048194)
				(xy 132.769198 98.380821) (xy 132.883862 97.705958) (xy 132.960505 97.025726) (xy 132.998887 96.342268)
			)
		)
	)
	(embedded_fonts no)
)
